# Compaq TCP/IP Services for OpenVMS
Management Command Reference

Previous | Contents | Index

R
Record Management Services
See RMS
Remote booting
See BOOTP
Remote procedure call
See RPC
remote shell
ADD PROXY command
CREATE PROXY command
Remote shell
registering clients
remote shell
registering clients
REMOVE DIRECTORY command
REMOVE EXPORT command
REMOVE FILE command
REMOVE MAIL command
REMOVE PROXY command
Resolver
See BIND
Reverse lookups
See Lookups
Reverse mapping
See Lookups
REXEC
enabling at system startup
monitoring
RIP
See Routing
RLOGIN
disabling
enabling at system startup
monitoring
Route
SET COMMUNICATION command
SET CONFIGURATION COMMUNICATION command
SHOW COMMUNICATION command
Routes Database
CREATE ROUTE command
SET MX_RECORD command
SHOW MX_RECORDS command
Routing
configuring
CREATE ROUTE command
displaying routes
SHOW ROUTE command
dynamic
SET ROUTE command
Gateway protocol routing
SET MX_RECORD command
SHOW MX_RECORDS command
starting
upon TCP/IP Services startup
static
SET ROUTE command
stopping
Routing Information Protocol (RIP)
See Routing
Routing tables
See Routing
RPC
displaying information used by Portmapper
SHOW PORTMAPPER command
RSH
disabling
enabling at system startup
monitoring
See remote shell
S
Security
ADD PROXY command #1
ADD PROXY command #2
CREATE PROXY command
REMOVE PROXY command
SEND MAIL command
Service
disabling
enabling
interactively
enabling at system startup
SET COMMUNICATION command
SET CONFIGURATION COMMUNICATION command
SHOW COMMUNICATION command
SHOW CONFIGURATION COMMUNICATION command
SHOW CONFIGURATION PROTOCOL command
Services
Database
ANALYZE SERVICE command
SET SERVICE command
SHOW SERVICE command
SET ARP command
SET BOOTP command
SET COMMUNICATION command
SET CONFIGURATION BIND command
SET CONFIGURATION COMMUNICATION command
SET CONFIGURATION ENABLE SERVICE command
SET CONFIGURATION INTERFACE command
SET CONFIGURATION MAP command
SET CONFIGURATION NAME_SERVICE command
SET CONFIGURATION PROTOCOL command
SET CONFIGURATION SMTP command
SET CONFIGURATION SNMP command
SET CONFIGURATION START ROUTING command
SET GATED command
SET HOST command
SET INTERFACE command
SET MX_RECORD command
SET NAME_SERVICE command
SET NETWORK command
SET NFS_SERVER command
SET PROTOCOL command
SET ROUTE command
SET SERVICE command
SHOW ARP command
SHOW BOOTP command
SHOW CFS command
SHOW COMMUNICATION command
SHOW CONFIGURATION command
SHOW CONFIGURATION PROTOCOL command
SHOW DEVICE
DCL command
SHOW DEVICE_SOCKET command
SHOW EXPORT command
SHOW HOST command
SHOW INTERFACE command
SHOW MAIL command
SHOW MAP command
SHOW MOUNT command
SHOW MX_RECORDS command
SHOW NAME_SERVICE command
SHOW NETWORK command
SHOW NFS_SERVER command
SHOW PORTMAPPER command
SHOW PROTOCOL command
SHOW PROXY command
SHOW ROUTE command
SHOW SERVICE command
SHOW VERSION command
Simple Mail Transfer Protocol
See SMTP
Simple Network Management Protocol
See SNMP
SLIP
controller
identifying
identifying with SET INTERFACE command
SMTP
8-bit characters
ANALYZE MAIL command
configuration
displaying
disabling
displaying queue information
enabling at system startup
headers
monitoring
options
8-bit characters
headers
queue management
queues
OpenVMS Cluster nodes
reconfiguring
REMOVE MAIL command
requeuing mail
See also MX Database
SEND MAIL command
SET MX_RECORD command
SHOW MX_RECORDS command
START MAIL command
SNMP
configuration
creating
displaying
disabling
enabling at system startup
monitoring
Specifying
address formats
file and directory names
multiple values in commands
names and addresses
numeric values
Stanford Research Institute
See APIs
START MAIL command
START ROUTING command
Static routing
See Routing
STOP ROUTING command
Subnetwork routing
See Routing
Subnetworking
See Routing
Sun ONC RPC
See RPC
Sun RPC
See RPC
T
TCP
parameters
setting
setting parameters
starting
TELNET
disabling
enabling at system startup
monitoring
Print Symbiont
See Printing
TELNETSYM
See also Printing
Terminal emulation
of IBM 3270 model terminals
See TELNET
Testing
for active connectivity
LOOP command
PING command
internet interface
SET INTERFACE /LOOPBACK command #1
SET INTERFACE /LOOPBACK command #2
TFTP
disabling
enabling at system startup
monitoring
TIME
configuration
displaying
TN3270
See TELNET
Transmission Control Protocol/Internet Protocol
See TCP/IP
Trivial File Transfer Protocol
See TFTP
Troubleshooting
internet controller
DELETE COMMUNICATION_CONTROLLER command
NFS Server
ANALYZE CONTAINER command
Services Database
ANALYZE SERVICE command
SMTP
ANALYZE MAIL command

Previous | Next | Contents | Index