Document revision date: 30 March 2001

## OpenVMS Delta/XDelta Debugger Manual

Previous | Contents | Index

P
;P command
Page faults
preventing
PCB address location
PCB vector start symbolic address
PFN (physical page number)
Physical page number
See PFN
PID
See IPID
Pn symbol #1
Pn symbol #2
Printed output command
Privileges
DELTA
XDELTA #1
XDELTA #2
Proceed from Breakpoint command
Processes
how to set writable
Processor register symbol
Processor status longword symbol
See PSL
Processor status symbol
See PS #1
See PS #2
Program execution
continuing
proceeding from breakpoint
step execution
step over subroutine execution
PS (processor status symbol) #1
PS (processor status symbol) #2
PSL (processor status longword) #1
PSL (processor status longword) #2
Q
;Q command
Q symbol
Queue
validate
" command
R
Radix
Redirecting output
DELTA
XDELTA
Registers
display contents
examining general purpose registers of another process
loading base
symbol for base
symbol for general #1
symbol for general #2
symbol for processor
RETURN command
Rn symbol
S
S command
SCH$GL_PCBVEC symbolic address
Set All Processes Writable command
Set Display Mode command
$SETPRT
used with XDELTA
Shareable images
debugging installed, protected
list information about current main and
Simple breakpoint
Single-step
fails
Sliced images #1
Sliced images #2
Sliced images #3
Stack pointer symbol #1
Stack pointer symbol #2
Stack pointer symbol #3
Step Instruction command
Step Instruction over Subroutine command
String
depositing ASCII
\string\ command
. symbol
Symbol list
System space prefix symbol
T
TAB command
Terminating DELTA
Terminating DELTA/XDELTA commands
V
Validate queue command
Value (last) displayed symbol
VAX 10000 series
requesting interrupt
VAX-11/730
requesting interrupt
VAX-11/750
requesting interrupt
VAX-11/780
requesting interrupt
VAX-11/785
requesting interrupt
VAX 4000 series
requesting interrupt
VAX 6000 series
requesting interrupt
VAX 7000 series
requesting interrupt
VAX 8200
requesting interrupt
VAX 8250
requesting interrupt
VAX 8300
requesting interrupt
VAX 8350
requesting interrupt
VAX 8530
requesting interrupt
VAX 8550
requesting interrupt
VAX 8600
requesting interrupt
VAX 8650
requesting interrupt
VAX 8810
requesting interrupt
VAX 8820
requesting interrupt
VAX 8820-N
requesting interrupt
VAX 8830
requesting interrupt
VAX 8840
requesting interrupt
VAX 9000
requesting interrupt
VAXft 3000
requesting interrupt
VAXft-410
requesting interrupt
VAXft-610
requesting interrupt
VAXft-612
requesting interrupt
VAXstation 2000
requesting interrupt
VAXstation 3500/3600 series
requesting interrupt
VAXstation 3520
requesting interrupt
VAXstation 3540
requesting interrupt
Video Terminal Display command
W
;W command
X
;X command
X4 symbol
X5 symbol
XE base register #1
XE base register #2
XF base register #1
XF base register #2
Xn symbol

| privacy and legal statement |
4540PRO_INDEX_001.HTML