# Compaq TP Desktop Connector
for ACMS
Gateway Management Guide

## Index

Previous | Contents

Master Alphabetic Index
A | B | C | D | E | F | G | I | L | M | N | O | P | R | S | T | U | V | W | X

A
ACMS system
displaying information
parameter setting
starting
ACMSDI$CLIENT
authorization check
use
ACMSDI$SHUTDOWN.COM
procedure use
ACMSDI$STARTUP.COM
procedure use #1
procedure use #2
procedure use #3
ACMSDI_LOG
environment parameter
ACMSDI_MAXBUF
setting
ACMSPARAM.COM
variables required for
ADSP Tool
AGENT_CNT
desktop effect on variable
AGENT_SUB_CNT
desktop effect on variable
Appletalk-DECnet Tool
Application
running simultaneously
AST limit
initial value
TP Desktop Connector gateway for ACMS
default value
Authorization
ACMS user
desktop system terminal
OpenVMS submitter node
task access
B
Buffer size
setting desktop client program
Buffered I/O
limit
default value
initial value
operations
default value
initial value
Building
TCP/IP-based client
Building client applications
NetWare C for DOS
NetWare C for Windows
C
CCL scripting language
CCL scripts
Communication
description
Component
network
PATHWORKS
Configuration
desktop system
Cyclic redundancy checking
D
DECnet Tool
DECnet transport
Default network transports
Desktop client program
running simultaneously
Direct I/O
TP Desktop Connector gateway for ACMS
default value
DOS
message buffer
setting
Dynamic-link libraries
E
Enqueue limit
TP Desktop Connector gateway for ACMS
default value
Environment variables
Error
desktop client program logging
Extent
TP Desktop Connector gateway for ACMS
default value
F
File limit
TP Desktop Connector gateway for ACMS
adjusting
default value
File server
application access
G
Gateway
account as agent
authorizing
TP Desktop Connector
OpenVMS authorization
overriding defaults
process quota defaults
starting
stopping
tuning process quotas
I
Integrity checking
L
Libraries
dynamic-link
static-link
Limit
AST
buffered I/O
initial
operations
open file
Links
use
Locks outstanding limit
TP Desktop Connector gateway for ACMS
default value
Logging
desktop client program
M
MacTCP Tool
Management
description
procedures
Multi-part applications
N
NetWare C client applications
See Building client applications
Network
component description
Macintosh
starting communications tool
Network DLLs
Novell NetWare
preparing the client
preparing the gateway
static-link
Novell NetWare transport
O
OpenVMS
ACMSDI_LOG
authorization
Ethernet address on
IPS/SPX stack
message buffer
setting
SAP process name
transports
Alpha
VAX
P
Page file
TP Desktop Connector gateway for ACMS
adjusting
default value
Password
system
in TP Desktop Connector authorization
Priority
TP Desktop Connector gateway for ACMS
default value
Process
quotas
TP Desktop Connector gateway for ACMS
R
REMOTE_NODE_CNT
Desktop effect on variable
REMOTE_SUB_CNT
Desktop effect on variable
Requirements for applications using DLLs
Rights identifier
ACMSDI$CLIENT
S
Serial communications
installation requirements
Macintosh
maintaining connections
switching current devices
transport
Server
access for file
Setting
alternate port on Macintosh
TCP/IP on Macintosh
Shutdown
TP Desktop Connector gateway for ACMS
Sign in
log file access
Software
synchronizing versions
Specifying port number
Starting the Serial-DECnet Gateway
Startup
TP Desktop Connector gateway
user-name assumptions
TP Desktop Connector gateway for ACMS
Static-link libraries
System
user-name assumptions
T
Task
canceling
Task-link extension
TCP/IP environment
TCP/IP transport
using Multinet
Time
synchronizing gateway and desktop system
Timer queue entries
TP Desktop Connector gateway for ACMS
default value
TP Desktop Connector gateway for ACMS
starting
stopping
tuning process quotas
Transport
DECnet
Novell NetWare
TCP/IP
Transport methodology
Troubleshooting
procedures for
Tuning
TP Desktop Connector gateway for ACMS

Previous | Next | Contents | Index