| ### Sample Environment File A sample environment file, config.env, is provided by OSF with the DCE source. You can copy the file and use it as supplied or you can use it as guide to creating your own environment file. The sample file is not copied to the install tree during DCE installation. The following figure shows this file. The file entries are in the form: variable=value To change a value, simply replace it with the new value. The possible values are listed as comments (prefaced with #) just following the variable. Sample Environment File # This file contain most of the variable used by dce_config. # You can pass this on the command line via the -e switch # or dce_config will look at /etc/dce_config.conf by default. # # This is a shell script sourced in to dce_config at startup # and can contain shell commands if you wish. # # # General config values # EXIT_ON_ERROR=n # y/n Exit if fatal error encountered, default n DO_CHECKS=n # y/n Prompt for continue after warnings, default y CELL_ADMIN=cell_admin # Principal name of Cell Administrator CELL_ADMIN_PW=-dce- # Password for CELL_ADMIN account #TOLERANCE_SEC=120 # Number of seconds clients can differ from sec server check_time=y # y/n if you want to check times, default y SYNC_CLOCKS=y # y/n Sync our clock to $TIME_SERVER TIME_SERVER="<host>" # Any host which has dts server on it, # usually the security server ($SEC_SERVER) # # Install # REMOVE_PREV_INSTALL=y # y/n Remove previous install before # installing anything. mach=`uname` case $mach in OSF1) machine=at386;; AIX) machine=rios;; HP-UX) machine=hp800;; esac # path to install area #FILESYSTEM="install/${machine}/opt/dce1.1" #MEDIA="<device>" # device to read tape from CP_OR_SYMLINK=copy # Use copy or sym-links(link) to install USE_DEF_MSG_PATH=y # y/n use default message catalog path USE_ETHER_FILE=y # y/n Trust /etc/ieee_802_addr file (OSF/1) DO_LIB_ADMIN=y # y/n Install libdce.so on OSF/1 system # # DFS install # INSTALL_OPT_SERS=y # y/n install optional servers (bak, butc, etc) INSTALL_OPT_CLIENT=y # y/n install optional client binaries (cm, etc) # # General config variables # REMOVE_PREV_CONFIG=y # y/n Remove previous config before config-ing anything CELL_NAME="<cellname>" # Name of cell to configure #HOST_NAME_IP="<ip_address>" # IP address of current host (if getip fails) # # DCE Client config # DTS_CONFIG=clerk # When doing DCE client config, what should # we be? clerk, local, global, none # # Security Config # SEC_SERVER="<host>" # Hostname of security server #SEC_SERVER_IP="<ip-address>" # fallback if getip program doesn't work KEYSEED="garBageMan" # Keyseed for initial database master # # Default values are provided, for PWD_MGMT_SVR and PWD_MGMT_SVR_OPTIONS. # # PWD_MGMT_SVR="$DCELOCAL/bin/pwd_strengthd" # Path to Password Management Server # PWD_MGMT_SVR_OPTIONS="-v" # Options for Password Management Server #SEC_REPLICA="<hostname>" # Name of the security replica database # # CDS Config # CACHE_CDS_SERVER="<hostname>" # Name of a cds server to cache #CACHE_CDS_SERVER_IP="<ip_address>" # fallback if getip program doesn't work MULTIPLE_LAN=n # y/n do you have multiple LANs #LAN_NAME="<name>" # Name of lan if MULTIPLE_LAN=y #REP_CLEARINGHOUSE="<name_ch>" # Name for new replica clearing house #DIR_REPLICATE="n" # y/n manually type in more directories # to replicate. # # GDA # # # DTS Config # NTP_HOST="<hostname>" # Name of ntp server #SEC_REPLICA="<hostname>" # Name of the security replica database # # CDS Config # CACHE_CDS_SERVER="<hostname>" # Name of a cds server to cache #CACHE_CDS_SERVER_IP="<ip_address>" # fallback if getip program doesn't work MULTIPLE_LAN=n # y/n do you have multiple LANs #LAN_NAME="<name>" # Name of lan if MULTIPLE_LAN=y #REP_CLEARINGHOUSE="<name_ch>" # Name for new replica clearing house #DIR_REPLICATE="n" # y/n manually type in more directories # to replicate. # # GDA # # # DTS Config # NTP_HOST="<hostname>" # Name of ntp server # # DFS Config # AGG_FS_TYPE=native # native/episode aggregate fs type to export AGG_DEV_NAME="<device>" # device name for the aggregate to be exported AGG_MOUNT_PATH="<path>" # mount path for aggregate AGG_NAME="<name>" # Name of aggregate AGG_ID="<number>" # numerical id of aggregate CACHE_SIZE_RAM=10000 # number of bytes for memory cache CACHE_SIZE_DISK=10000 # number of bytes for disk cache CACHE_DIR_DISK="/opt/dcelocal/var/adm/dfs/cache" # pathname of disk cache CLIENT_CACHE_LOC=disk # mem/disk where is the cache CONFIG_NFS_GATEWAY=n # configure dfs client as nfs gateway EPI_FORMAT_PART=n # y/n format partition as episode EPI_FORCE_INIT=n # y/n force initialization, even if data loss INIT_LFS=n # y/n initialize the LFS (using epiinit)? LOAD_LFS_KEXT=n # y/n load LFS kernel extensions ROOT_FILESET_NM="<name>" # Root fileset name SCM_NAME="<hostname>" # System Control Machine name ###