# DIGITAL TCP/IP Services for OpenVMS
Management

Previous | Contents

### N

- Name service
  - See DNS
- Name-to-address lookups
  - See Lookups
- NAMED.CA
  - BIND Server databases
- Network device
  - new
    - defining
    - displaying
- Network management
  - remote
    - See SNMP
  - See individual topics
- Network print services
  - See Printing
- NFS
  - failover
  - PC-NFS
    - See PC-NFS
  - Server
    - access to client superuser
    - ACLs
    - authenticating clients
    - bytes
    - container files
      - creating
  - counters
  - file system integrity
  - FILLM
  - hard mount
  - inode
  - on OpenVMS Cluster
  - opened files affect performance of
  - operations
    - displaying how many
- performance
- performance indicator for
- Portmapper
- security
- SHOW NFS_SERVER command
- starting
- stopping
- SYSGEN parameters
- tasks
  - listed

- threads
- troubleshooting
  - requirements
- tuning #1
- tuning #2
- UAF file limits
- nolisten socket type
- Nonpaged pool
  - affected by device sockets
  - requirements
- NSLOOKUP
  - case sensitivity
  - commands
  - initialization file
  - starting
  - stopping
    - current activity
    - NSLOOKUP

  ### O

  - ONC
    - See RPC
  - Online help
    - See Help
  - Open Network Computing (ONC)
    - See RPC
  - OpenVMS Cluster
    - NFS Databases
    - proxy database
  - Overview
    - of managing UCX

  ### P

  - Packets
    - checking I/O requests
  - PATHWORKS IP Driver
    - See PWIP
  - PC-NFS
    - Portmapper
    - Print Server
      - See also Printing
    - troubleshooting
      - requirements
  - PC-NFSd
    - See PC-NFS
  - Performance
    - See Troubleshooting
  - Planning
    - BOOTP
    - TFTP
  - POP server
    - error messages
    - OPCOM messages
  - Port numbers
    - used by server software
  - Portmapper
    - starting
    - stopping
  - POSTMASTER account
    - creating
  - PPP
    - messages
  - Printcap Database
    - defining entries in
    - explained
  - Printing
    - LPD
      - troubleshooting
    - queues
      - starting
    - See also LPD
    - See also LPR
    - See also PC-NFS
    - TELNETSYM
      - troubleshooting
  - Problem solving
    - See Troubleshooting
  - Protocol
    - See also individual protocols
  - Proxy
    - ADD PROXY command
    - database, adding an entry
  - Proxy Database
    - adding entries
    - on OpenVMS Cluster
  - Pseudo-interface
    - See Internet interface
  - PWIP Driver
    - starting
    - stopping

  ### Q

  - Queue
    - SMTP
      - reconfigure
      - stopped

  ### R

  - R commands
    - security
    - trusted hosts
      - setting up
  - RCP
  - Re-assembly
    - of datagrams
      - performance
  - Re-assembly time
    - of datagrams
      - setting
  - Record Management Services
    - See RMS
  - Remote booting
    - See BOOTP
  - Remote procedure call
    - See RPC
  - Requirements
    - nonpaged pool
  - Resolver
    - See BIND
  - Reverse lookups
    - See Lookups
  - Reverse mapping
    - See Lookups
  - REVTRA macro
  - REXEC
  - RIP
    - See Routing
  - RLOGIN
    - security
  - Root name servers
  - Round-robin
    - load balancing
      - DNS #1
      - DNS #2
      - DNS #3
  - Routes Database
    - SET MX_RECORDS command
    - SHOW MX_RECORDS command
  - Routing
    - broadcast address
      - defining interface routes
    - configuration
      - testing
        - LOOP command
        - PING command
    - configuring
    - direct
      - defined
    - dynamic
      - configuring
      - setting
    - gateway
      - with static routes
    - indirect
      - defined
    - interface routes
      - defining
    - metric 0 route
      - defining
    - re-assembly of datagrams
    - SET MX_RECORDS command
    - SHOW MX_RECORDS command
    - static
      - setting
    - static routes
      - defining
      - displaying
    - stopping
    - subnetwork
      - extending
    - subnetworking
      - creating
  - Routing Information Protocol (RIP)
    - See Routing
  - Routing tables
    - See Routing
  - RSH
    - See Remote Shell

  ### S

  - Security
    - ADD PROXY command
    - Anonymous FTP
    - BOOTP
    - customized driver for
    - NFS Server
    - RLOGIN
    - TFTP #1
    - TFTP #2
  - Services
    - database
      - event logging
    - end-user
      - RCP
      - REXEC
      - RLOGIN
      - RSH
    - initializing
    - Portmapper
    - starting
    - troubleshooting (general)
  - SET COMMUNICATION /ALLOW_LOG_OPTIONS command
  - SET COMMUNICATION command
    - TCP/IP cluster time interval
  - SET COMMUNICATION /FORCE_LOG_OPTIONS command
  - SET CONFIGURATION COMMUNICATION command
    - pseudo-interfaces
  - SET CONFIGURATION INTERFACE command
    - internet pseudo-interfaces
  - SET CONFIGURATION SMTP command
  - SET INTERFACE command
    - internet pseudo-interfaces
  - SET ROUTE command
    - static routes
      - defining
  - SET SERVICE command
  - SET SERVICE /LOG_OPTIONS command
  - SHOW COMMUNICATION command
    - pseudo-interfaces
  - SHOW CONFIGURATION BIND command
    - DNS
  - SHOW CONFIGURATION COMMUNICATION command
    - network interfaces
  - SHOW ROUTE command
  - Simple Mail Transfer Protocol
    - See SMTP
  - Simple Network Management Protocol
    - See SNMP
  - SLIP
    - troubleshooting
  - SMTP
    - configuring
    - DISABLE SERVICE SMTP command
    - ENABLE SERVICE SMTP command
    - Exchanger
    - log files
    - lookups
    - mail
      - utility files
    - MX records
      - creating
      - displaying #1
      - displaying #2
    - POSTMASTER account
    - queue stopped
    - queues
      - monitoring
      - reconfigure
    - queuing
    - Receiver
    - restart
    - Routes Database
    - See also MX Database
    - Sender
    - sending mechanism
    - SET CONFIGURATION SMTP command
    - START MAIL command
    - starting
    - STOP MAIL command
    - troubleshooting
    - UCX_SMTP_LOGFILE.LOG
    - UCX_SMTP_RECV_STARTUP.LOG
    - utility files
    - zones
  - SNATRAPRE.MAR
  - SNATRATBL.MAR
  - SNMP
    - configuring
      - community address
      - community name
      - community type
  - SOA record
    - BIND Server
  - Socket types
    - activation flags
    - datagram
    - for initialization
    - listen flag
    - nolisten activation flag
    - stream
  - Stanford Research Institute
    - See APIs
  - START MAIL command
  - Static routing
    - See Routing
  - STOP MAIL command
  - STOP ROUTING command
  - Subnetwork routing
    - See Routing
  - Subnetworking
    - See Routing
  - Sun ONC RPC
    - See RPC
  - Sun RPC
    - See RPC
  - SYSGEN
    - NFS server
      - tuning parameters for

  ### T

  - TCP connection
    - closing
    - DISCONNECT DEVICE_SOCKET command
  - TCP/IP cluster
    - alias
    - automatic failover
    - cluster time interval
    - configuring
    - DNS load balancing
    - SET COMMUNICATION command
  - TELNET
    - inactivity timer
    - Print Symbiont
      - See Printing
    - troubleshooting
      - inactivity timer
      - INETACP byte limit quota
      - performance
  - TELNETSYM
    - See also Printing
    - troubleshooting
  - Terminal emulation
    - of IBM 3270 model terminals
      - See TELNET
  - Testing
    - routing
      - LOOP command
      - PING command
  - TFTP
    - planning
      - security
    - security for
    - troubleshooting #1
    - troubleshooting #2
  - Threads
    - NFS Server
      - displaying
    - NFS Server performance
  - Time intervals
    - ARP cache
    - for unresolved queries in ARP database
  - TN3270
    - See TELNET
  - Translation tables
    - building
    - examples of
    - modifying
  - Transmission Control Protocol/Internet Protocol
    - See TCP/IP
  - Trivial File Transfer Protocol
    - See TFTP
  - Troubleshooting
    - BIND Server
    - BOOTP
    - buffer space
    - connectivity
      - LOOP command
      - PING command
    - device sockets
      - modifying
    - FTP
    - nonpaged pool
      - affected by device sockets
    - performance
      - checksums
      - datagram re-assembly
      - NFS Server
      - tuning
    - printing
      - LPD
      - TELNETSYM
    - problem isolation
    - services
      - analyzing
      - verifying availability
    - SLIP
    - SMTP
    - TELNET
      - inactivity timer
      - INETACP byte limit quota
      - performance
    - TFTP #1
    - TFTP #2

  Previous | Next | Contents