Document revision date: 30 March 2001

## OpenVMS VAX System Dump Analyzer Utility Manual

Previous | Contents | Index

## SHOW LAN

> Displays information contained in various local area network (LAN) data structures. The default qualifiers are /CSMACD/FDDI.

### Format

> SHOW LAN [/qualifier[,...]]

### Parameters

> None.

### Qualifiers

> #### /CLIENT=xx

> Specifies that information be displayed for the specified client. Valid client designators are SCA, DECNET, LAT, MOPRC, TCPIP, DIAG, ELN, BIOS, LAST, USER, ARP, MOPDL, LOOP, BRIDGE, DNAME, ENCRY, DTIME, and LTM. /CLIENT, /DEVICE, and /UNIT are synonymous and mutually exclusive; each must be the last qualifier stated on an SDA command line.

> #### /CLUEXIT

> Specifies that cluster protocol information be displayed.

> #### /COUNTERS

> Specifies that the LAN station block (LSB) and unit control block (UCB) counters be displayed.

> #### /CSMACD

> Specifies that Carrier Sense, Multiple Access with Collision Detect (CSMACD) information for the LAN be displayed.

> #### /CSMACD/FDDI (default)

> Displays both Ethernet and FDDI information.

> #### /DEVICE=xx[dn]

> Specifies that information be displayed for the specified device. Device designators are specified in the format xxdn, where xx is the type of device, d is the device letter, and n is the unit number. The device letter and unit number are optional. /CLIENT, /DEVICE, and /UNIT are synonymous and mutually exclusive; each must be the last qualifier stated on an SDA command line.

> #### /ERRORS

> Specifies that the LSB and UCB error counters be displayed.

> #### /FDDI

> Specifies that Fiber Distributed Data Interface (FDDI) controller information for the LAN be displayed.

> #### /FULL

> Specifies that all information from the LAN, LSB, and UCB data structures be displayed.

> #### /SUMMARY

> Specifies that only a summary of LAN information (a list of flags, LSBs, UCBs, and base addresses) be printed. This is the default.

> #### /TIMESTAMPS

> Specifies to print time information (start and stop times and error times) from the device and unit data structures. SDA displays the data in chronological order.

> #### /UNIT=xx/[dn]

> Specifies that information be displayed for the specified unit. Unit designators are specified in the format xx/[dn], where xx is the type of unit, d is the device letter, and n is the unit number. The device letter and unit number are optional. /CLIENT, /DEVICE, and /UNIT are synonymous and mutually exclusive; each must be the last qualifier stated on an SDA command line.

### Description

> The SHOW LAN command displays information contained in various local area network (LAN) data structures. By default, or when you specify the /SUMMARY qualifier, SHOW LAN displays a list of flags, LSBs, UCBs, and base addresses. When you specify the /FULL qualifier, SHOW LAN displays all information found in the LAN, LSB, and UCB data structures.

###

#### Examples

#1
    SDA> SHOW LAN

                    -- LAN Device Summary 26-JAN-1993 20:57:41 --

    LAN block address  = 9834C680  (6 stations)
    LAN flags:  0002 LAN_init

    LSB address  = 98358B40
    Device state = 001B Inited,Run,Ctl_Rdy,Timer

                     -- EXA Unit Summary 26-JAN-1993 20:57:41 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    EXA0    98358540
    EXA1    98376340  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    EXA3    98ACD240  Eth   60-03           DECNET  0004 Uniq
    EXA5    983A9580  Eth   80-41           LAST    0015 Strtn,Uniq,Strtd

    LSB address  = 98369B40
    Device state = 4013 Inited,Run,Timer

                     -- FXA Unit Summary 26-JAN-1993 20:57:41 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    FXA0    98369840
    FXA1    98391980  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    FXA2    98AC9680  Eth   60-03           DECNET  0017 Strtn,Len,Uniq,Strtd
    FXA3    98AC7100  Eth   60-01           MOPDL   001F Strtn,Uniq,Share,Strtd
    FXA4    98AC9B80  Eth   90-00           LOOP    001D Strtn,Uniq,Share,Strtd
    FXA5    98395380  Eth   60-04           LAT     0015 Strtn,Uniq,Strtd

    LSB address  = 9836CE00
    Device state = 001B Inited,Run,Ctl_Rdy,Timer

                     -- EXB Unit Summary 26-JAN-1993 20:57:41 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    EXB0    98358880
    EXB1    983B8B00  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    EXB2    98ACD500  Eth   60-03           DECNET  0004 Uniq

    LSB address  = 9836FE00
    Device state = 001B Inited,Run,Ctl_Rdy,Timer

                     -- EXC Unit Summary 26-JAN-1993 20:57:41 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    EXC0    9836CA80
    EXC1    983C08C0  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    EXC2    98ACD7C0  Eth   60-03           DECNET  0004 Uniq

    LSB address  = 98376600
    Device state = 001B Inited,Run,Ctl_Rdy,Timer

                     -- EXD Unit Summary 26-JAN-1993 20:57:41 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    EXD0    9836FA80
    EXD1    983C8680  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    EXD2    98ACDA80  Eth   60-03           DECNET  0004 Uniq

    LSB address  = 98378340
    Device state = 4013 Inited,Run,Timer

                     -- FXB Unit Summary 26-JAN-1993 20:57:41 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    FXB0    98377F80
    FXB1    983D0440  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    FXB2    98AC9900  Eth   60-03           DECNET  0004 Uniq

> The SHOW LAN command in this example displays information about LAN data structures, including CSMACD and FDDI information.

#2
    SDA>  SHOW LAN/COUNTERS/DEV=DECNET
         -- EZA1 60-03 (DECNET) Counters Information 19-JUL-1993 14:27:02 --
    Last receive                    None    Last transmit        19-JUL 14:26:51
    Octets received               580539    Octets sent               2399353240
    PDUs received                   8194    PDUs sent                       5618
    Mcast octets received              0    Mcast octets sent                  0
    Mcast PDUs received                0    Mcast PDUs sent                    0
    Unavail user buffer                0    Last start attempt              None
    Last start done      19-JUL 06:40:22    Last start failed               None

> The SHOW LAN command in this example displays the counters for device DECNET.

#3
    SDA> SHOW LAN/CSMACD

                    -- LAN Device Summary 26-JAN-1993 20:57:22 --

    LAN block address  = 9834C680  (6 stations)
    LAN flags:  0002 LAN_init

    LSB address  = 98358B40
    Device state = 001B Inited,Run,Ctl_Rdy,Timer

                     -- EXA Unit Summary 26-JAN-1993 20:57:22 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    EXA0    98358540
    EXA1    98376340  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    EXA3    98ACD240  Eth   60-03           DECNET  0004 Uniq
    EXA5    983A9580  Eth   80-41           LAST    0015 Strtn,Uniq,Strtd

    LSB address  = 9836CE00
    Device state = 001B Inited,Run,Ctl_Rdy,Timer

                     -- EXB Unit Summary 26-JAN-1993 20:57:22 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    EXB0    98358880
    EXB1    983B8B00  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    EXB2    98ACD500  Eth   60-03           DECNET  0004 Uniq

    LSB address  = 9836FE00
    Device state = 001B Inited,Run,Ctl_Rdy,Timer

                     -- EXC Unit Summary 26-JAN-1993 20:57:22 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    EXC0    9836CA80
    EXC1    983C08C0  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    EXC2    98ACD7C0  Eth   60-03           DECNET  0004 Uniq

    LSB address  = 98376600
    Device state = 001B Inited,Run,Ctl_Rdy,Timer

                     -- EXD Unit Summary 26-JAN-1993 20:57:22 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    EXD0    9836FA80
    EXD1    983C8680  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    EXD2    98ACDA80  Eth   60-03           DECNET  0004 Uniq

> The SHOW LAN command in this example displays CSMACD information for the LAN.

#4
    SDA SHOW LAN/FDDI
                    -- LAN Device Summary 26-JAN-1993 20:57:07 --

    LAN block address  = 9834C680  (6 stations)
    LAN flags:  0002 LAN_init

    LSB address  = 98369B40
    Device state = 4013 Inited,Run,Timer

                     -- FXA Unit Summary 26-JAN-1993 20:57:07 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    FXA0    98369840
    FXA1    98391980  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    FXA2    98AC9680  Eth   60-03           DECNET  0017 Strtn,Len,Uniq,Strtd
    FXA3    98AC7100  Eth   60-01           MOPDL   001F Strtn,Uniq,Share,Strtd
    FXA4    98AC9B80  Eth   90-00           LOOP    001D Strtn,Uniq,Share,Strtd
    FXA5    98395380  Eth   60-04           LAT     0015 Strtn,Uniq,Strtd

    LSB address  = 98378340
    Device state = 4013 Inited,Run,Timer

                     -- FXB Unit Summary 26-JAN-1993 20:57:07 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    FXB0    98377F80
    FXB1    983D0440  Eth   60-07           SCA     0017 Strtn,Len,Uniq,Strtd
    FXB2    98AC9900  Eth   60-03           DECNET  0004 Uniq

> The SHOW LAN command in this example displays FDDI information.

#5
    SDA> SHOW LAN/FULL
    LAN Data Structures

                 -- LAN Information Summary 27-JAN-1993 09:54:50 --

    LAN flags:  0002 LAN_init

    LAN module version                 1    First SVAPTE                81FAFC14
    LAN address                 80EA8C00    Number of PTEs                     4
    Number of stations                 1    SVA of pages                80A00A00
    First LSB address           80ECE700

              -- LAN CSMACD Network Management 27-JAN-1993 09:54:50 --

    Creation time                   None    Times created                      0
    Deletion time                   None    Times deleted                      0
    Module EAB                  00000000    Latest EIB                  00000000
    Port EAB                    00000000
    Station EAB                 00000000

               -- LAN FDDI Network Management 27-JAN-1993 09:54:50 --

    Creation time                   None    Times created                      0
    Deletion time                   None    Times deleted                      0
    Module EAB                  00000000    Latest EIB                  00000000
    Port EAB                    00000000
    Station EAB                 00000000
    Link EAB                    00000000
    PHY port EAB                00000000

                  -- ESA Device Information 27-JAN-1993 09:54:50 --

    LSB address                 80ECE700    Active unit count                  2
    LAN version        00000001 06000036    Driver version     00000001 06000009
    LAN code address            80EC8BF9    Driver code address         80EC68B0
    Device name                 ES_LANCE    Device type                       24
    Device version     00000000 00000000    DLL type                      CSMACD

    Data chaining                     ON    All multicast state              OFF
    Controller mode               NORMAL    Promiscuous mode                 OFF
    CRC generation mode               ON    Hardware mode                   0000
    Physical address   AA-00-04-00-50-FD    Hardware address   08-00-2B-2A-D7-F7

    Flags:  0000                            Characteristics: 0000
    Status: 0013 Inited,Run,Timer

    DAT stage                   00000000    DAT xmt status     0000001A 001A0001
    DAT number started                 1    DAT xmt complete     26-JAN 13:20:31
    DAT number failed                  0    DAT rcv found                   None
    Creation time                   None    Create count                       0
    Deletion time                   None    Enable count                       0
    Enabled time                    None    Fatal error count                  0
    Disabled time                   None    Excessive collisons                0

    Last receive         27-JAN 09:54:50    Last fatal error                None
    Last transmit        27-JAN 09:54:47    Prev fatal error                None
    Last fork sched      27-JAN 09:54:50    Last exc collision   26-JAN 16:36:26
    Last fork time       27-JAN 09:54:50

    Rcv buffers owned by device        9    System buffer quota                0
    Xmt entries owned by device        0    Device dependent longword   00000000
    Xmt entries owned by host          0    # restarts pending                 0

    NMgmt advised buffer count         0    Events logged                      0
    EIB address                 00000000    NMgmt assigned adr 00-00-00-00-00-00
    LPB address                 00000000

                  -- ESA Queue Information 27-JAN-1993 09:54:50 --

    Control hold queue      80ECE820  Status:  Valid, empty
    Control request queue   80ECE828  Status:  Valid, empty
    Control pending queue   80ECE830  Status:  Valid, empty
    Transmit request queue  80ECE818  Status:  Valid, empty
    Transmit pending queue  80ECE838  Status:  Valid, empty
    Receive buffer queue    80ECE840  Status:  Valid, empty
    Receive pending queue   80ECE848  Status:  Valid, 9 elements
    Post process queue      80ECE850  Status:  Valid, empty
    Delay queue             80ECE858  Status:  Valid, empty
    Auto restart queue      80ECE860  Status:  Valid, empty
    Netwrk mgmt hold queue  80ECE868  Status:  Valid, empty

            -- ESA Multicast Address Information 27-JAN-1993 09:54:50 --

    AB-00-00-04-00-00
    09-00-2B-04-00-00

                     -- ESA Unit Summary 27-JAN-1993 09:54:50 --

    UCB     UCB Addr  Fmt   Value           Client     State
    ---     --------  ---   -----           ------  -----------
    ESA0    80EC61C0
    ESA2    80EFD600  Eth   60-03           DECNET  0017 Strtn,Len,Uniq,Strtd
    ESA4    80F505C0  Eth   80-41           LAST    0015 Strtn,Uniq,Strtd

      .
      .
      .

            -- ESA Internal Counters Information 27-JAN-1993 09:54:50 --

    Internal counters address   80ECF6E8    Internal counters size            30
    Number of ports                    0    Global page transmits              0
    No work transmits                  0    SVAPTE/BOFF transmits              0
    Bad PTE transmits                  0    Buffer_Adr transmits               0

    Fatal error count                  0    RDL errors                         0
    Transmit timeouts                  0    Last fatal error                None
    Restart failures                   0    Prev fatal error                None
    Power failures                     0    Last error CSR              00000000
    Hardware errors                    0    Fatal error code                None
    Control timeouts                   0    Prev fatal error                None

    Loopback sent                      0    Loopback failures                  0
    System ID sent                   121    System ID failures                 0
    ReqCounters sent                   0    ReqCounters failures               0

              -- ESA0 Template Unit Information 27-JAN-1993 09:54:50 --

    LSB address                 80ECE700    VCIB address                00000000
    Packet format               Ethernet    Error count                        0
    Device buffer size              1500    LAN medium                    CSMACD
    Maximum buffer size             1500    Eth protocol type              00-00
    Hardware buffer quota              9    802E protocol ID      00-00-00-00-00
    Receive buffer quota               0    802.2 SAP                         00
    Allow prom client                 ON    802.2 Group SAPs         00,00,00,00
    Promiscuous mode                 OFF    Maximum header size                0
    802.2 service                    OFF    Hardware address   08-00-2B-2A-D7-F7
    Data chaining                    OFF    Physical address   FF-FF-FF-FF-FF-FF
    Padding mode                      ON    Can change address               OFF
    Automatic restart                OFF    Access mode                EXCLUSIVE
    CRC generation mode               ON    Controller mode               NORMAL
    Maintenance state                 ON    Rcv buffs to queue                 1
    P2 parameters               00000000    Starter's PID               00000000
    All multicast mode               OFF    Creator's PID               00000000
    Rcv buffer quota                   0    LSB size                        5986

           -- ESA2 60-03 (DECNET) Unit Information 27-JAN-1993 09:54:50 --

    LSB address                 80ECE700    VCIB address                00000000
    Packet format               Ethernet    Error count                        0
    Device buffer size              1500    LAN medium                    CSMACD
    Maximum buffer size             1498    Eth protocol type              60-03
    Hardware buffer quota              9    802E protocol ID      00-00-00-00-00
    Receive buffer quota           15040    802.2 SAP                         00
    Allow prom client                 ON    802.2 Group SAPs         00,00,00,00
    Promiscuous mode                 OFF    Maximum header size               16
    802.2 service                    OFF    Hardware address   08-00-2B-2A-D7-F7
    Data chaining                    OFF    Physical address   AA-00-04-00-50-FD
    Padding mode                      ON    Can change address               OFF
    Automatic restart                OFF    Access mode                EXCLUSIVE
    CRC generation mode               ON    Controller mode               NORMAL
    Maintenance state                 ON    Rcv buffs to queue                10
    P2 parameters               00374395    Starter's PID               0001000C
    All multicast mode               OFF    Creator's PID               0001000C
    Rcv buffer quota               15040    LSB size                        5986

         -- ESA2 60-03 (DECNET) Counters & Misc Info 27-JAN-1993 09:54:50 --

    Last receive         27-JAN 09:54:50    Last transmit        27-JAN 09:54:47
    Octets received              5087025    Octets sent                  2310540
    PDUs received                  34018    PDUs sent                      29121
    Mcast octets received        2189558    Mcast octets sent             246850
    Mcast PDUs received             9877    Mcast PDUs sent                 4937
    Unavail user buffer               11    Last start attempt              None
    Last start done      26-JAN 13:20:32    Last start failed               None
                                            Share UCB total quota              0

    Receive IRP queue       80EFD7C4  Status:  Valid, 1 element
    Shared users queue      80EFD7B4  Status:  Valid, empty
    Receive pending queue   80EFD7BC  Status:  Valid, empty

        -- ESA2 60-03 (DECNET) Multicast Address Info 27-JAN-1993 09:54:50 --

    Multicast address table, embedded:
      AB-00-00-04-00-00

            -- ESA4 80-41 (LAST) Unit Information 27-JAN-1993 09:54:50 --

    LSB address                 80ECE700    VCIB address                80F504F3
    Packet format               Ethernet    Error count                        0
       .
       .
       .

          -- ESA4 80-41 (LAST) Counters & Misc Info 27-JAN-1993 09:54:50 --

    Last receive         27-JAN 09:54:39    Last transmit        27-JAN 09:54:38
    Octets received              1941967    Octets sent                   371740
       .
       .
       .
         -- ESA4 80-41 (LAST) Multicast Address Info 27-JAN-1993 09:54:50 --

    Multicast address table, embedded:
      09-00-2B-04-00-00

> The SHOW LAN/FULL command in this example displays information for all LAN, LSB, and UCB data structures.

#6
    SDA> SHOW LAN/TIMESTAMPS
    LAN Data Structures
    -------------------
                 -- LAN History Information 19-JUL-1993 14:27:38 --
    19-JUL 14:27:38.93  EZA               Last receive
    19-JUL 14:27:38.93  EZA               Last fork scheduled
    19-JUL 14:27:38.93  EZA               Last fork time
    19-JUL 14:27:36.05  EZA               Last transmit
    19-JUL 14:27:36.05  EZA1     DECNET   Last transmit
    19-JUL 14:23:54.41  EZA164   DIAG     Last start completed
    19-JUL 08:05:16.09  EZA               Last excessive collision
    19-JUL 06:40:22.94  EZA1     DECNET   Last start completed
    19-JUL 06:40:21.94  EZA               Last DAT transmit

> The SHOW LAN command displays LAN timestamp information.

## SHOW LOCK

> Displays information about all lock management locks in the system, cached locks, or a specified lock.

### Format

> SHOW LOCK {lock-id|/ALL|/CACHED|/NAME=resource-name}

### Parameters

> #### lock-id

> Name of a specific lock. You cannot specify both a lock-id and a resource-name in the same command line.

### Qualifiers

> #### /ALL

> Lists all locks that exist in the system. This is the default behavior of the SHOW LOCK command.

> #### /CACHED

> Shows only cached lock blocks (LKBs).

> #### /NAME=resource-name

> Displays information about the resource associated with the lock whose resource name begins with the specified resource-name. For case-sensitive names, enclose the resource-name in quotation marks. You cannot specify both a lock-id and resource-name in the same command line.

### Description

> The SHOW LOCK command displays the information described in Table SDA-15 for each lock management lock in the system or for the lock indicated by lock-id. (Use the SHOW SPINLOCK command to display information about spin locks.) You can obtain a similar display for the locks owned by a specific process by issuing the appropriate SHOW PROCESS/LOCKS command. See the OpenVMS System Services Reference Manual for additional discussion of the significance of this information.

> You can display information about the resource to which a lock is queued by issuing the SHOW RESOURCE command and specifying the lock-id of the resource.

> Table SDA-15 Contents of the SHOW LOCK and SHOW PROCESS/LOCKS Displays
> Display Element | Description
> --- | ---
> Process Index 1 | Index into the PCB array to a pointer to the process control block (PCB) of the process that owns the lock.
> Name 1 | Name of the process that owns the lock.
> Extended PID 1 | Clusterwide identification of the process that owns the lock.
> Lock ID | Identification of the lock.
> PID | Systemwide identification of the lock.
> Flags | Information specified in the request for the lock.
> Par. ID | Identification of the lock's parent lock.
> Granted at | Lock mode at which the lock was granted.
> Sublocks | Identification numbers of the locks that the lock owns.
> LKB | Address of the lock block (LKB). If a blocking AST has been enabled for this lock, the notation "BLKAST" appears next to the LKB address.
> Resource | Dump of the resource name. The two leftmost columns of the dump show its contents as hexadecimal values, the least significant byte being represented by the rightmost two digits. The rightmost column represents its contents as ASCII text, the least significant byte being represented by the leftmost character.
> Status | Status of the lock, information used internally by the lock manager.
> Length | Length of the resource name.
> --- | Processor access mode of the name space in which the resource block (RSB) associated with the lock resides.
> --- | Owner of the resource. Certain resources owned by the operating system list "System" as the owner. Resources owned by a group have the number (in octal) of the owning group in this field.
> --- | Indication of whether the lock is mastered on the local system or is a process copy.

1You produce this display element only by using the SHOW PROCESS/LOCKS command.

###

#### Examples

#1
    SDA> SHOW LOCK
    Lock database
    -------------

    Lock id:  00010001   PID:    00000000   Flags:   NOQUEUE SYNCSTS SYSTEM
    Par. id:  00000000   Granted at    EX            CVTSYS
    Sublocks:        1
    LKB:      80D0B8A0
    Resource:      5F535953 24535953    SYS$SYS_  Status:  NOQUOTA
     Length   16   00000000 4C774449    IDwL....
     Exec. mode    00000000 00000000    ........
     System        00000000 00000000    ........
    Local copy

    Lock id:  00010004   PID:    00000000   Flags:   CONVERT SYNCSTS CVTSYS
    Par. id:  00000000   Granted at    CR
    Sublocks:       16
    LKB:      80D091A0   BLKAST
    Resource:      4D567624 42313146    F11B$vVM  Status:  NOQUOTA
     Length   18   20204E41 4A353153    S15JAN
     Kernel mode   00000000 00002020      ......
     System        00000000 00000000    ........
    Local copy

    Lock id:  00280009   PID:    00000000   Flags:   VALBLK  CONVERT SYNCSTS
    Par. id:  00000000   Granted at    CR            NOQUOTA CVTSYS
    Sublocks:        0
    LKB:      80CDA880
    Resource:      52414B5F 24535953    SYS$_KAR  Status:  MSTCPY
     Length   17   30415544 24455441    ATE$DUA0
     Kernel mode   00000000 0000003A    :.......
     System        00000000 00000000    ........
    Master copy of lock 001C00F5 on system 000100A1
       .
       .
       .
    SDA>  SHOW RESOURCE/LOCK=280009
    Resource database
    -----------------
    Address of RSB:  80BD2150  Group grant mode:       CR
    Parent RSB:      00000000  Conversion grant mode:  CR
    Sub-RSB count:          0  BLKAST count:            0
    Value block:   00000000 00000000 00000000 00000019   Seq. #:  0000002D
    Resource:      52414B5F 24535953    SYS$_KAR
     Length   17   30415544 24455441    ATE$DUA0         CSID:  00000000
     Kernel mode   00000000 0000003A    :.......
     System        00000000 00000000    ........

    Granted queue (Lock ID / Gr mode):
         00DA1269  CR       00280009  CR       0094054D  CR
         00270B9F  CR       00D70BFE  CR       000D0F4F  CR
         000D1017  CR       00601418  CR       01131450  CR
         000F1964  CR       000200DF  CR

    Conversion queue (Lock ID / Gr/Rq mode):
         *** EMPTY QUEUE ***

    Waiting queue (Lock ID / Rq mode):
         *** EMPTY QUEUE ***

> Previous | Next | Contents | Index

> | privacy and legal statement |
> 4556PRO_011.HTML