# DIGITAL TCP/IP Services for OpenVMS
Management Command Reference

Previous | Contents

## Index

### A

- Account
  - OpenVMS user
    - creating #1
    - creating #2
    - deleting
    - displaying
- ADD EXPORT command
- ADD PROXY command
- Address
  - 0.0.0.0
    - displaying device sockets
  - host-name-to-address lookups
    - See Lookups
  - IP
    - defining #1
    - defining #2
    - displaying
    - how to specify
  - mapping IP to Ethernet/FDDI #1
  - mapping IP to Ethernet/FDDI #2
- Address Resolution Protocol
  - See ARP
- Alias
  - for defining a cluster
- ANALYZE CONTAINER command
- ANALYZE MAIL command
- ANALYZE SERVICE command
- Anonymous FTP
  - See FTP
- "ANY host"
  - displaying device sockets
- Applications
  - customer-developed
    - ADD PROXY command
    - registering clients
- ARP
  - parameters
    - setting #1
    - setting #2
  - SET ARP command
  - SHOW ARP command
- Authentication
  - ADD PROXY command #1
  - ADD PROXY command #2
  - CREATE PROXY command
  - REMOVE PROXY command
- AUTHORIZE command (DCL)
- Auxiliary Server
  - connect requests to client
  - messages from
  - multithreading
- Auxiliary server
  - restarting the NFS server
- Auxiliary Server
  - service rejected
  - uses the BIND Resolver
- Auxiliary server
  - uses the BIND resolver
- Auxiliary Server
  - when activates a service

### B

- Berkeley Internet Name Domain
  - See BIND
- BG device driver
  - See Internet interface
- BIND
  - Resolver
    - configuration
      - displaying
- configuring #1
- configuring #2
- defining the domain #1
- defining the domain #2
- deleting the domain #1
- deleting the domain #2
- disabling
- displaying the configuration
- enabling
- SHOW HOST command
- stopping

- Server
  - configuration
    - displaying
- configuring
- CONVERT/ULTRIX BIND command
- Database
  - CONVERT/ULTRIX BIND command
- disabling
- monitoring
- reloading
- SET CONFIGURATION BIND command
- BIND command
  - See MAP command
- BIND Database
  - SHOW HOST command
- Binding
  - See MAP command
- Booting, remote
  - See BOOTP
- BOOTP
  - Database
    - adding entries to
    - CONVERT/VMS BOOTP command
    - creating
    - displaying
  - disabling
  - enabling
    - upon system startup
  - monitoring
  - SET BOOTP command
  - SHOW BOOTP command
- Bootstrap Protocol
  - See BOOTP
- Buffers
  - displaying
    - SHOW COMMUNICATION command
  - Ethernet
    - allocating
  - FDDI
    - allocating
  - setting
    - SET COMMUNICATION command
  - size
    - setting for Remote Login
    - setting for TELNET

  ### C

  - Case sensitivity
    - when typing commands
      - file names
  - Cluster load balancing
    - See BIND Server
  - Commands
    - braces in documentation
    - brackets in documentation
    - command descriptions
      - how to use
    - DCL
      - AUTHORIZE
      - SHOW DEVICE
    - program design
      - configuration commands
      - CONVERT commands
      - creating database files
      - database files
        - default protections of
    - displaying information
    - local lookups
    - /LOCAL qualifier
    - managing NFS
    - starting software
    - stopping software
    - validating databases
  - See individual commands
  - typing
  - UNIX
    - /etc/mount
  - using
    - how to type
    - program design
  - valid values
    - specifying
  - wildcards
    - using when deleting
- Configuration
  - BIND Server
    - creating
  - copying
  - creating
  - Database
    - BIND Server entries
      - creating
  - copying
  - creating
  - displaying
  - lower-layer software entries
    - creating
- lower-level protocol entries
  - creating
- Name Server entries
  - creating
- SMTP entries
  - creating
- SNMP entries
  - creating
- TIME
  - resetting
- displaying
- Name Server
  - creating
- permanent
  - See also individual SET CONFIGURATION commands
- SMTP
  - creating
- SNMP
  - creating
- TIME
  - resetting
- Controller
  - Ethernet
    - identifying with SET INTERFACE command
    - zeroing counters
  - FDDI
    - identifying with SET INTERFACE command
    - zeroing counters
  - SLIP
    - identifying with SET INTERFACE command
- Conventions
  - for typing commands
    - file names
    - lowercase
    - multiple values
    - uppercase
    - wildcards
- CONVERT/ULTRIX BIND command
- CONVERT/ULTRIX HOST command
- CONVERT/ULTRIX NETWORK command
- CONVERT/VMS BOOTP command
- CONVERT/VMS HOST command
- CONVERT/VMS NETWORK command
- CONVERT/VMS PROXY command
- COPY CONFIGURATION command
- Counters
  - resetting
    - protocol
- CREATE BOOTP command
- CREATE CONFIGURATION command
- CREATE CONTAINER command
- CREATE DIRECTORY command
- CREATE EXPORT command
- CREATE HOST
- CREATE NETWORK
- CREATE PROXY command
- CREATE ROUTE command
- Customer-developed applications
  - ADD PROXY command
  - registering clients

  ### D

  - Data link
    - See Internet interface
  - Data link interface
    - See Internet interface
  - Database
    - BIND
      - SHOW HOST command
    - BIND Server
      - CONVERT/ULTRIX BIND command
    - BOOTP
      - adding entries to
      - CONVERT/VMS BOOTP command
      - creating
      - displaying
    - Configuration
      - BIND Server entries
        - creating
    - copying
    - creating
    - displaying
    - lower-layer software entries
      - creating
  - lower-level protocol entries
    - creating
- Name Server entries
  - creating
- SMTP entries
  - creating
- SNMP entries
  - creating
- TIME
  - resetting
- Export
  - adding directory names in the Export Database
  - CREATE EXPORT command
  - deleting directory names from the Export Database
  - SHOW EXPORT command
- files
  - default protections of
- Hosts
  - cluster alias
    - specifying
- CONVERT/ULTRIX HOST command
- CONVERT/VMS HOST command
- SHOW HOST command
- MX
  - SET MX_RECORD command
  - SHOW MX_RECORDS command
- Network
  - CONVERT/ULTRIX NETWORK
  - CONVERT/VMS NETWORK
- Networks
  - adding entries
  - displaying entries
- Proxy
  - adding entries to #1
  - adding entries to #2
  - creating
  - deleting entries from
  - SHOW PROXY command
- Routes
  - CREATE ROUTE command
  - SET MX_RECORD command
  - SHOW MX_RECORDS command
- Services
  - ANALYZE SERVICE command
  - SET SERVICE command
  - SHOW SERVICE command
- SHOW MX_RECORDS command
- DCL
  - AUTHORIZE command
  - SHOW DEVICE command
- Defense Data Network
  - See DDN
- DEFINE COMMUNICATION_CONTROLLER command
- Defining
  - cluster alias
    - interface identifier
- DELETE COMMUNICATION_CONTROLLER command
- DELETE CONTAINER command
- Design
  - of UCX management program
- Device driver
  - internet #1
  - internet #2
  - internet #3
  - internet #4
- Device socket
  - SET COMMUNICATION command
  - SET CONFIGURATION COMMUNICATION command
  - SHOW COMMUNICATION command
  - SHOW DEVICE_SOCKET command
- Directory
  - multiple names
    - on command lines
- DIRECTORY command
- DISABLE SERVICE command
- DISCONNECT DEVICE_SOCKET command
- DISMOUNT command
- DNFSn:
  - See NFS
- DNS
  - See also BIND
- Domain
  - SET CONFIGURATION BIND command
- Domain Name Service
  - See BIND
  - See DNS
- Downline loading
  - See Downloading
- Dynamic routing
  - See Routing

  Previous | Next | Contents