Document revision date: 30 March 2001

## OpenVMS Delta/XDelta Debugger Manual

## Index

Previous | Contents

Master Alphabetic Index
A | B | C | D | E | F | G | H | I | K | L | M | N | O | P | Q | R | S | T | V | W | X

A
Address location
changing the value
closing current #1
closing current #2
command strings (XDELTA) #1
command strings (XDELTA) #2
displaying contents of current
displaying, from other processes
displaying in ASCII
displaying location pointed to by current location
displaying next
displaying previous
displaying range
listing for executive images
PCB
referencing
using base address and offsets #1
using base address and offsets #2
Address symbol
current
Arithmetic operators
Arithmetic shift
ASCII
depositing string
displaying contents
B
;B command
Base register
loading
symbol
Boot command
qualifiers for XDELTA
Boot procedures for XDELTA
See also entries for individual computers
Breakpoint
accessing initial on Alpha
accessing initial on VAX
clearing #1
clearing #2
complex
initial in multiprocessor environment
initial in XDELTA
multiprocessor environment #1
multiprocessor environment #2
multiprocessor environment #3
proceeding from
proceeding from initial
range for DELTA
range for XDELTA
setting #1
setting #2
setting #3
showing #1
showing #2
simple
XDELTA restriction on breakpoint 1
Breakpoint command
Bugcheck information
C
;C command
Close Current Location, Open Next command
Code pages
making writable
' command
/ command
= command
[ command
Command list
Complex breakpoint
Control region space prefix symbol
Copy-on-reference
See CRF
CPU ID #1
CPU ID #2
Crash command
CRF (copy-on-reference)
D
Debugging
at elevated IPL
at IPL 0
code that does not match compiler listing
kernel mode code in process space
privileged code
user-mode programs
Delta/XDelta Debugger
exiting from DELTA
exiting from XDELTA
invoking DELTA
invoking XDELTA
Delta/XDelta utility
debugging an installed, protected, shareable image
Deposit ASCII String command
Display information commands
See List commands
Display mode
how to set
Display Value of Expression command
E
;E command
Eh? error message
ESC command
ESC key equivalent
Evaluation precedence
Exclamation Point (!) command
Execute Command String command
Executive images
listing names and addresses #1
listing names and addresses #2
Exit command
Exiting
from DELTA #1
from DELTA #2
from XDELTA
Expressions
precedence in
See also Numeric expressions
F
Floating-point control register (FPCR)
Floating-point registers
FPCR symbol
G
;G command
G symbol
General register symbol #1
General register symbol #2
General register symbol #3
Go command
H
;H command
H symbol
Hardcopy output command
I
;I command
Image code
does not match compiler listing
Images, sliced #1
Images, sliced #2
Images, sliced #3
Immediate mode text display command
INI$BRK routine #1
INI$BRK routine #2
INI$BRK routine #3
Alpha
VAX
Initial breakpoint
See Breakpoint
Instructions
how to display
Internal processor register
Interrupt request for XDELTA
See also entries for individual computers
Invoking
DELTA
See also Boot procedures for XDELTA; Interrupt request for XDELTA
XDELTA
IPID #1
IPID #2
IPID #3
IPID #4
IPID #5
IPR symbolic names
Alpha
K
Kernel mode code in process space
debugging
L
;L command
privileges required
LINEFEED command
Linefeed key equivalent
Linker options file
used with XDELTA
LIS file #1
LIS file #2
LIS file #3
LIS file #4
List commands
Information About the Current Main Image and Its Shareable Images
Name and Location of a Single Image
Names and Addresses of Loaded Executive Images
Load Base Register command
M
;M command
privileges required
MAP file #1
MAP file #2
MAP file #3
MAP file #4
MicroVAX 2000
requesting interrupt
MicroVAX 3300/3400 series
requesting interrupt
MicroVAX 3500/3600 series
requesting interrupt
MicroVAX 3800/3900 series
requesting interrupt
MicroVAX II
requesting interrupt
Multiprocessor environment
initial breakpoint
XDELTA breakpoints #1
XDELTA breakpoints #2
XDELTA breakpoints #3
XDELTA breakpoints #4
XDELTA operation
N
Numeric expressions #1
Numeric expressions #2
O
O command
Open Location and Display Contents command
Open Location and Display Contents in Instruction Mode command
Open Location and Display Indirect Location command
Open Location and Display Previous Location command
Operators
arithmetic
Output
from DELTA
from XDELTA

Previous | Next | Contents | Index

| privacy and legal statement |
4540PRO_INDEX.HTML