| #### Configuring a System Control Machine To configure a System Control machine, perform the following steps: 1. Type 3 on the DCE Configuration Menu and press <Return>. The dce_config script displays the following message: S:****** Configuring DFS System Control Machine... and then prompts: Enter Cell Administrator's principal name: (cell_admin) 2. Type the name of the principal who was defined to be the initial privileged user of the registry database during the configuration of the master Security server and press <Return> . The dce_config script prompts: Enter password: 3. Type the password for the initial privileged user's account and press <Return>. Note that this password is not displayed as you type it. The dce_config script loads the DFS kernel extensions and displays the following messages: S:****** Loading kernel extensions... rpc_config: installed krpc device at major number 71 Then the dce_config script prompts for whether LFS (Episode) should be loaded Should the LFS Kernel Extension be loaded (n)? 4. Type y to configure the machine to use LFS or n to not and press <Return>. The dce_config script displays: Should LFS be initialized (n)? 5. Type y to initialize LFS or n to not and press <Return>. The dce_config script displays: S:****** Modifying the registry database for DFS server operation... S:****** Starting bosserver... S:****** Creating BOS admin lists. S:****** Starting upserver... When the configuration is complete, dce_config displays the Additional Server Configuration menu. ####