# Compaq ACMS for OpenVMS
Remote Systems Management Guide

Previous | Contents | Index

# 11.34 ACMSMGR SHOW MANAGER

Displays run-time information about a Remote Manager on one or more nodes.

## Format

> ### ACMSMGR SHOW MANAGER [/qualifiers]

> Command Qualifier | Default
> --- | ---
> /INTERVAL=interval | Command is executed once.
> /NODE=node-name | Translation of logical ACMS$MGMT_SERVER_NODE
> /OUT=file-name | None
> /USER=user-name | Translation of logical ACMS$MGMT_USER

## Privileges Required

> ACMS$MGMT_READ

## Parameters

> None.

## Qualifiers

> ### /INTERVAL=interval

> This qualifier causes the command to be reissued automatically at a specified interval (in seconds). Use either Ctrl/C or Ctrl/Y to interrupt the command. If this qualifier is not specified, the command is executed only once.

> ### /NODE=node-name

> This qualifier specifies a fully- or partially-qualified TCP/IP host name. This name must match the current DECnet host name. IP addresses and host names (or aliases) that exceed six characters or include mixed case are not allowed. For more information on TCP/IP host names and defining aliases, see Section 2.2.1.

> If the /NODE qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_SERVER_NODE. If the logical is defined, the value of the logical is used by default.

> In order for the command to execute, either the /NODE qualifier must be provided on the command line, or the ACMS$MGMT_SERVER_NODE logical must be defined.

> ### /OUT=file-name

> This qualifier causes output to be written to the specified file. If this qualifier is not specified, output is displayed to the terminal (SYS$OUTPUT).

> ### /USER=user-name

> This qualifier specifies the name of the OpenVMS account on the server node to be used for authorization. If this qualifier is specified, an explicit login must already have been completed successfully (see Section 11.9).

> If the /USER qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_USER. If the logical is defined, the value of the logical is used by default.

> If the /USER qualifier is not specified and the ACMS$MGMT_USER logical is not defined, the ACMSMGR utility attempts proxy access. See Section 4.4.1.2 for a discussion of proxy access.

## Notes

> See Section 9.8 for a discussion of each field displayed.

## Example

    $  ACMSMGR SHOW MANAGER

    ACMS Remote Management -- Command line utility

    ACMS V4.4-0 Remote Manager Status Table Display  Time: 18-APR-2001 13:59:22.76

     Node         Fields
    ------------- ----------------------------------------------------------
     VLCROW       Collection Count                   0
     VLCROW       Interfaces Count                   2
     VLCROW       Trap Count                         0
     VLCROW       RPC UDP State                      1
     VLCROW       RPC TCP State                      1
     VLCROW       Timer Count                        0

> This command displays summary information about the Remote Manager on the node specified by the logical name ACMS$MGMT_SERVER_NODE. Authorization is performed for the user specified by the logical name ACMS$MGMT_USER, or by proxy if the logical is not defined.

# 11.35 ACMSMGR SHOW PARAMETER

Displays Remote Manager configuration parameters for a server on one or more nodes.

## Format

> ### ACMSMGR SHOW PARAMETER [/qualifiers]

> Command Qualifier | Default
> --- | ---
> /INTERVAL=interval | Command is executed once.
> /NODE=node-name | Translation of logical ACMS$MGMT_SERVER_NODE
> /OUT=file-name | None
> /USER=user-name | Translation of logical ACMS$MGMT_USER

## Privileges Required

> ACMS$MGMT_READ

## Parameters

> None.

## Qualifiers

> ### /INTERVAL=interval

> This qualifier causes the command to be reissued automatically at a specified interval (in seconds). Use either Ctrl/C or Ctrl/Y to interrupt the command. If this qualifier is not specified, the command is executed only once.

> ### /NODE=node-name

> This qualifier specifies a fully- or partially-qualified TCP/IP host name. This name must match the current DECnet host name. IP addresses and host names (or aliases) that exceed six characters or include mixed case are not allowed. For more information on TCP/IP host names and defining aliases, see Section 2.2.1.

> If the /NODE qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_SERVER_NODE. If the logical is defined, the value of the logical is used by default.

> In order for the command to execute, either the /NODE qualifier must be provided on the command line, or the ACMS$MGMT_SERVER_NODE logical must be defined.

> ### /OUT=file-name

> This qualifier causes output to be written to the specified file. If this qualifier is not specified, output is displayed to the terminal (SYS$OUTPUT).

> ### /USER=user-name

> This qualifier specifies the name of the OpenVMS account on the server node to be used for authorization. If this qualifier is specified, an explicit login must already have been completed successfully (see Section 11.9).

> If the /USER qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_USER. If the logical is defined, the value of the logical is used by default.

> If the /USER qualifier is not specified and the ACMS$MGMT_USER logical is not defined, the ACMSMGR utility attempts proxy access. See Section 4.4.1.2 for a discussion of proxy access.

## Notes

> See Section 9.9 for a description of each parameter.

## Example

    $   ACMSMGR SHOW PARAMETER /NODE=VLCROW
    ACMS Remote Management -- Command line utility

    ACMS V4.4-0  Parameters Table Display           Time: 18-APR-2001 13:59:24.79

     Node     Parameter               Value    Default   Min     Max           Units

    ---------------------------------------------------------------------------------------------
     VLCROW   dcl_audit_level         E        E         0                 F    (D)
     VLCROW   dcl_mgr_priority        5        5         1                10
     VLCROW   dcl_stacksize           300      300       1        2147483647    k (Vax), 8k (Alpha)
     VLCROW   event_log_priority      5        5         1                10
     VLCROW   error_interval         10       10         1         863999999    seconds (D)
     VLCROW   log_stacksize           300      300       1        2147483647    K (Vax), 8k (Alpha)
     VLCROW   login_creds_lifetime    60       60        1          14399999    minutes (D)
     VLCROW   max_logins              20       20        1        2147483647    (D)
     VLCROW   max_rpc_return_recs     20       20        1        2147483647
     VLCROW   mgr_audit_level         E        E         0                 F    (D)
     VLCROW   msg_proc_audit_level    E        E         0                 F    (D)
     VLCROW   msg_proc_priority       5        5         1                10
     VLCROW   msg_proc_stacksize      300      300       1        2147483647    k (Vax), 8k (Alpha)
     VLCROW   mss_coll_interval       10       10        1         863999999    seconds (D)
     VLCROW   proc_mon_audit_level    E        E         0                 F    (D)
     VLCROW   proc_mon_interval       3        30        1          14399999    seconds (D)
     VLCROW   proc_mon_priority       5        5         1                10
     VLCROW   proc_mon_stacksize      300      300       1        2147483647    K (Vax), 8k (Alpha)
     VLCROW   proxy_creds_lifetime    60       60        1          14399999    minutes (D)
     VLCROW   rpc_audit_level         E        E         0                 F    (D)
     VLCROW   rpc_priority            5        5         1                10
     VLCROW   rpc_stacksize           30       300       1        2147483647    k (Vax), 8k (Alpha)
     VLCROW   security_audit_level    E        E         0                 F    (D)
     VLCROW   snap_audit_level        E        E         0                 F    (D)
     VLCROW   snap_priority           5        5         1                10
     VLCROW   snap_stacksize          300      300       1        2147483647    k (Vax), 8k (Alpha)
     VLCROW   snmp_agent_time_out     10       10        1         863999999    seconds
     VLCROW   snmp_are_you_there      300      300       2         863999999    seconds
     VLCROW   snmp_audit_level        E        E         0                 F    (D)
     VLCROW   snmp_priority           5        5         1                10
     VLCROW   snmp_sel_time_out       5        5         1         863999999    seconds
     VLCROW   snmp_stacksize          300      300       1        2147483647    k (Vax), 8k (Alpha)
     VLCROW   tcp_enabled             1        1         0                 1    [0,1] 1=enabled
     VLCROW   timer_audit_level       E        E         0                 F    (D)
     VLCROW   timer_interval          30       30        1         863999999    seconds (D)
     VLCROW   timer_priority          5        5         1                10
     VLCROW   timer_stacksize         300      300       1        2147483647    k (Vax), 8k (Alpha)
     VLCROW   total_entity_slots      20       20        1        2147483647
     VLCROW   trace_msg_wait_time     5        5         1          14399999    seconds (D)
     VLCROW   trace_start_wait_time   5        5         1          14399999    seconds (D)
     VLCROW   trap_audit_level        E        E         0                 F    (D)
     VLCROW   trap_priority           5        5         1                10
     VLCROW   trap_stacksize          300      300       1        2147483647    k (Vax), 8k (Alpha)
     VLCROW   udp_enabled             1        1         0                 1    [0,1] 1=enabled
     VLCROW   vms_coll_interval       10       10        0         863999999    seconds (D)
     VLCROW   wksp_coll_interval      10       10        1         863999999    seconds (D)

> This command displays data from the Remote Manager Parameter table on node VLCROW. Authorization is performed on the user specified by the logical name ACMS$MGMT_USER, or by proxy if the logical is not defined.

# 11.36 ACMSMGR SHOW PROCESS

Displays summary data collection information for processes on one or more nodes.

## Format

> ### ACMSMGR SHOW PROCESS [/qualifiers]

> Command Qualifier | Default
> --- | ---
> /ALL | Current processes only.
> /[BRIEF,FULL] | /BRIEF
> /INTERVAL=interval | Command is executed once.
> /NODE=node-name | Translation of logical ACMS$MGMT_SERVER_NODE
> /OUT=file-name | None
> /USER=user-name | Translation of logical ACMS$MGMT_USER

## Privileges Required

> ACMS$MGMT_READ

## Parameters

> None.

## Qualifiers

> ### /ALL

> This qualifier displays all available application data, even data for applications that may no longer be running. When applications are stopped, the table row they were occupying is marked for reuse. If the row has not been reused, the data remains available for display. This qualifier allows that data to be displayed. Inactive rows are flagged with an asterisk (*) in the output.

> To inhibit the display of old data, do not specify this qualifier. By default, only data for currently running processes is displayed.

> ### /[BRIEF,FULL]

> Specifies the format of the data displayed. /BRIEF is the default and displays data in tabular format.

> ### /INTERVAL=interval

> This qualifier causes the command to be reissued automatically at a specified interval (in seconds). Use either Ctrl/C or Ctrl/Y to interrupt the command. If this qualifier is not specified, the command is executed only once.

> ### /NODE=node-name

> This qualifier specifies a fully- or partially-qualified TCP/IP host name. This name must match the current DECnet host name. IP addresses and host names (or aliases) that exceed six characters or include mixed case are not allowed. For more information on TCP/IP host names and defining aliases, see Section 2.2.1.

> If the /NODE qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_SERVER_NODE. If the logical is defined, the value of the logical is used by default.

> In order for the command to execute, either the /NODE qualifier must be provided on the command line, or the ACMS$MGMT_SERVER_NODE logical must be defined.

> ### /OUT=file-name

> This qualifier causes output to be written to the specified file. If this qualifier is not specified, output is displayed to the terminal (SYS$OUTPUT).

> ### /USER=user-name

> This qualifier specifies the name of the OpenVMS account on the server node to be used for authorization. If this qualifier is specified, an explicit login must already have been completed successfully (see Section 11.9).

> If the /USER qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_USER. If the logical is defined, the value of the logical is used by default.

> If the /USER qualifier is not specified and the ACMS$MGMT_USER logical is not defined, the ACMSMGR utility attempts proxy access. See Section 4.4.1.2 for a discussion of proxy access.

## Notes

> This command displays the current data-collection states for all process entry slots. Both active and inactive process data is displayed. Inactive data is flagged with an asterisk (*) in the first column. The following fields are displayed:
> - Server Node: The node from which the information was fetched.
> - Entity Type: The ACMS entity type to which the data belongs.
> - PID: The OpenVMS PID of the process.
> - Process Name: The process name for the process.
> - Collection States: The current collection state of the process for each class (ID, CONFIG, RUNTIME, POOL, and ERROR). Collection states are displayed as binary values.
>   - 0 = Collection is currently disabled.
>   - 1 = Collection is currently enabled.

## Example

    $  ACMSMGR SHOW PROCESS

    ACMS Remote Management -- Command line utility

    ACMS V4.4-0  Process Table Display               Time: 18-APR-2001 13:59:26.77

    Server Entity          Process Name -or- Application.          Collection States
    Node   Type    PID     [server_name, task_group_name]          ID   Cfg  RT   Pool Err
    ------ ------ -------- --------------------------------------  ---- ---- ---- ---- ----
    VLCROW acc    37C0024F ACMS01ACC001000                         1    1    1    1    1
    VLCROW tsc    37C00251 ACMS01TSC001000                         1    1    1    1    1
    VLCROW cp     37C00252 ACMS01CP001000                          1    1    1    1    1
    VLCROW cp     37C00253 ACMS01CP002000                          1    1    1    1    1
    VLCROW cp     37C00254 ACMS01CP003000                          1    1    1    1    1
    VLCROW cp     37C00255 ACMS01CP004000                          1    1    1    1    1
    VLCROW exc    37C0025A ACMS01EXC001000                         1    1    1    1    1
    VLCROW          server LDT_APPL_A.TESTSRV01                    1    1    1    1    1
    VLCROW           group LDT_APPL_A.TEST_GRP01                   1    1    0    1    1

> This command displays Collection state information on a per-process basis from the node specified by the logical name ACMS$MGMT_SERVER_NODE. Authorization is performed for the user specified by the logical name ACMS$MGMT_USER, or by proxy if the logical is not defined.

# 11.37 ACMSMGR SHOW QTI

Displays information about QTIs on one or more remote nodes.

## Format

> ### ACMSMGR SHOW QTI [/qualifiers]

> Command Qualifier | Default
> --- | ---
> /ACTIVE | See Notes.
> /ALL | Current process data only.
> /[BRIEF,FULL] | /FULL if no class qualifier (/CONFIG, /ERROR, /ID, /POOL,
> | or /RUNTIME) is specified. Otherwise, /BRIEF.
> /[class-name] | * (all)
> /INTERVAL=interval | Command is executed once.
> /NODE=node-name | Translation of logical ACMS$MGMT_SERVER_NODE
> /OUT=file-name | None
> /STORED | See Notes.
> /USER=user-name | Translation of logical ACMS$MGMT_USER

## Privileges Required

> ACMS$MGMT_READ

## Parameters

> None.

## Qualifiers

> ### /ACTIVE

> When specified with the /BRIEF qualifier, this qualifier causes active ACMSGEN field values to be displayed. /ACTIVE is effective only when used with the /CONFIG qualifier. If /BRIEF is not specified, or if /FULL is specified, this qualifier has no effect (both active and stored values are displayed).

> ### /ALL

> This qualifier displays all available QTI data, including data for processes that are no longer running. When QTI processes are stopped, the QTI table row they were occupying is marked for reuse. If the row has not been reused, the data remains available for display. This qualifier allows that data to be displayed. Inactive rows are flagged with an asterisk (*) in the output.

> To inhibit the display of old data, do not specify this qualifier. By default, only data for currently running processes is displayed.

> ### /[BRIEF,FULL]

> This qualifier causes either summary (/BRIEF) or detailed (/FULL) information to be displayed. If no class qualifier (/CONFIG, /ERROR, /ID, /POOL, or /RUNTIME) is specified, this qualifier is ignored and all details are displayed (equivalent to /FULL). Available OpenVMS process quota and SYSGEN parameter information is only displayed when /FULL is specified.

> ### /[CONFIG,ERROR,ID,POOL,RUNTIME]

> This qualifier causes data for only the specified class to be displayed. If this qualifier is omitted, the default is to display information for all classes.

> ### /INTERVAL=interval

> This qualifier causes the command to be reissued automatically at a specified interval (in seconds). Use either Ctrl/C or Ctrl/Y to interrupt the command. If this qualifier is not specified, the command is executed only once.

> ### /NODE=node-name

> This qualifier specifies a fully- or partially-qualified TCP/IP host name. This name must match the current DECnet host name. IP addresses and host names (or aliases) that exceed six characters or include mixed case are not allowed. For more information on TCP/IP host names and defining aliases, see Section 2.2.1.

> If the /NODE qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_SERVER_NODE. If the logical is defined, the value of the logical is used by default.

> In order for the command to execute, either the /NODE qualifier must be provided on the command line, or the ACMS$MGMT_SERVER_NODE logical must be defined.

> ### /OUT=file-name

> This qualifier causes output to be written to the specified file. If this qualifier is not specified, output is displayed to the terminal (SYS$OUTPUT).

> ### /STORED

> When specified with the /BRIEF qualifier, this qualifier causes field values from the ACMSGEN file (not those active in memory) to be displayed. The /STORED qualifier is effective only when used with the /CONFIG qualifier. If /BRIEF is not specified, or if /FULL is specified, this qualifier has no effect (both active and stored values are displayed).

> ### /USER=user-name

> This qualifier specifies the name of the OpenVMS account on the server node to be used for authorization. If this qualifier is specified, an explicit login must already have been completed successfully (see Section 11.9).

> If the /USER qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_USER. If the logical is defined, the value of the logical is used by default.

> If the /USER qualifier is not specified and the ACMS$MGMT_USER logical is not defined, the ACMSMGR utility attempts proxy access. See Section 4.4.1.2 for a discussion of proxy access.

## Notes

> This command displays information about the QTIs on the target nodes. The /BRIEF and /FULL qualifiers control the format of information to be displayed. To display OpenVMS process quota and SYSGEN parameter information, use the /FULL qualifier.

> See Section 9.10 for a discussion of each field displayed.

> Note that some information may not be current, depending on whether the class to which the data belongs has been enabled for the QTI. The Runtime Class field indicates whether or not information is being collected for that class.

## Example

    $  ACMSMGR SHOW QTI /NODE=KAZONS /RUNTIME

    ACMS Remote Management -- Command line utility

    ACMS V4.4-0  QTI  Table Display                 Time: 18-APR-2001 13:41:11.09

           Runtime  Started Current   Task    Tasks    Tasks   Current  Errors
    Node    Class   Queues  Tasks   Retries  Success   Failed  Submitrs Queued
    ------ -------- ------- ------- -------- -------- -------- -------- --------
    kazons enabled  3       17      4361     14859    5783     5        1329

> This command displays summary run-time information for the QTI on node KAZONS. Authorization is performed for the user specified by the logical name ACMS$MGMT_USER, or by proxy if the logical is not defined.

# 11.38 ACMSMGR SHOW SERVER

Displays information about one or more ACMS application server types on one or more nodes.

## Format

> ### ACMSMGR SHOW SERVER [/qualifiers]

> Command Qualifier | Default
> --- | ---
> /APPL=application-name | * (all)
> /[BRIEF,FULL] | /FULL if no class qualifier (/CONFIG, /ERROR, /ID,
> | or /RUNTIME) is specified. Otherwise, /BRIEF.
> /[class-name] | * (all)
> /INTERVAL=interval | Command is executed once.
> /NODE=node-name | Translation of logical ACMS$MGMT_SERVER_NODE
> /OUT=file-name | None
> /SERVER=server-name | * (all)
> /USER=user-name | Translation of logical ACMS$MGMT_USER

## Privileges Required

> ACMS$MGMT_READ

## Parameters

> None.

## Qualifiers

> ### /APPL=application-name

> Use this qualifer to specify a particular ACMS application to display. Wildcard matching is performed on the name provided; use of asterisks (*) is allowed.

> ### /[BRIEF,FULL]

> This qualifier causes either summary (/BRIEF) or detailed (/FULL) information to be displayed. If no class qualifier (/CONFIG, /ERROR, /ID, or /RUNTIME) is specified, this qualifier is ignored and all details are displayed (equivalent to /FULL).

> ### /[CONFIG,ERROR,ID,RUNTIME]

> This qualifier causes data for only the specified class to be displayed. If this qualifier is omitted, the default is to display information for all classes.

> ### /INTERVAL=interval

> This qualifier causes the command to be reissued automatically at a specified interval (in seconds). Use either Ctrl/C or Ctrl/Y to interrupt the command. If this qualifier is not specified, the command is executed only once.

> ### /NODE=node-name

> This qualifier specifies a fully- or partially-qualified TCP/IP host name. This name must match the current DECnet host name. IP addresses and host names (or aliases) that exceed six characters or include mixed case are not allowed. For more information on TCP/IP host names and defining aliases, see Section 2.2.1.

> If the /NODE qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_SERVER_NODE. If the logical is defined, the value of the logical is used by default.

> In order for the command to execute, either the /NODE qualifier must be provided on the command line, or the ACMS$MGMT_SERVER_NODE logical must be defined.

> ### /OUT=file-name

> This qualifier causes output to be written to the specified file. If this qualifier is not specified, output is displayed to the terminal (SYS$OUTPUT).

> ### /SERVER=server-name

> This qualifier specifies a particular ACMS application server to display. Wildcard matching is performed on the name provided; use of asterisks (*) is allowed.

> ### /USER=user-name

> This qualifier specifies the name of the OpenVMS account on the server node to be used for authorization. If this qualifier is specified, an explicit login must already have been completed successfully (see Section 11.9).

> If the /USER qualifier is not specified, the ACMSMGR utility checks for the presence of the logical name ACMS$MGMT_USER. If the logical is defined, the value of the logical is used by default.

> If the /USER qualifier is not specified and the ACMS$MGMT_USER logical is not defined, the ACMSMGR utility attempts proxy access. See Section 4.4.1.2 for a discussion of proxy access.

## Notes

> This command displays information about ACMS application servers on the target node. The /BRIEF and /FULL qualifiers control the format of information to be displayed.

> See Section 9.11 for a discussion of each field displayed.

> Note that some information may not be current, depending on whether the class to which the data belongs has been enabled for the server. The Runtime Class field indicates whether or not information is being collected for that class.

## Example

    $  ACMSMGR SHOW SERVER /NODE=VLCROW /RUNTIME

    ACMS Remote Management -- Command line utility

    ACMS V4.4-0  SER Table Display                   Time: 18-APR-2001 13:59:33.60

           Runtime Application                      Current Waiting Server Server
     Node  Class   Name        Server Name          Servers Tasks   Starts Failures
    ------ ------- ----------- -------------------- ------- -----   ------ --------
    VLCROW enabled LDT_APPL_A  TESTSRV01            2       0       2      0
    VLCROW enabled LDT_APPL_A  TESTSRV1D            0       0       3419   0
    VLCROW enabled LDT_APPL_A  TESTSRV2D            1       0       19     0
    VLCROW enabled LDT_APPL_A  TESTSRV3D            1       0       1      0
    VLCROW enabled LDT_APPL_A  TESTSRV05            0       0       0      0
    VLCROW enabled LDT_APPL_A  TLOAD001S            4       0       6      0
    VLCROW enabled LDT_APPL_A  TLOAD002S            1       0       1      0
    VLCROW enabled LDT_APPL_A  DBMSLSRV1            1       0       1      0
    VLCROW enabled LDT_APPL_A  DBMSLSRV2            1       0       1      0
    VLCROW enabled LDT_APPL_A  RDBLSRV1             1       0       44     0
    VLCROW enabled LDT_APPL_A  RMSRSERVR            1       0       33     0
    VLCROW enabled LDT_APPL_A  TCT_LDT_PROC_SERVER  1       0       1      0
    VLCROW enabled LDT_APPL_A  TCT_LDT_CHAIN_SERVER 1       0       1      0
    VLCROW enabled LDT_APPL_A  TCT_LDT_DCL_SERVER   0       0       0      0
    VLCROW enabled LDT_APPL_A  RI_DCL_SERVER        2       0       9      0
    VLCROW enabled LDT_APPL_A  RI_V3016_FMS_SERVER  1       0       1      0
    VLCROW enabled LDT_APPL_A  RI_V3016_RI_SERVER   1       0       1      0
    VLCROW enabled LDT_APPL_A  VF_V3111_SERVER      0       0       0      0
    VLCROW enabled LDT_APPL_A  LDT_CS_V3111_SERVER  3       0       3      0
    VLCROW enabled LDT_APPL_A  TESTV32_RMS_SERVER   8       0       28     0
    VLCROW enabled LDT_APPL_A  TESTV32_RDB_SERVER   8       0       375    0
    VLCROW enabled LDT_APPL_A  TESTV32_DBMS_SERVER  8       0       47     0
    VLCROW enabled LDT_APPL_A  TESTV32_SQL_SERVER   8       0       405    0
    VLCROW enabled LDT_APPL_A  TESTV32_RM_SERVER    4       0       4      0
    VLCROW enabled LDT_APPL_A  GEN_INPUT_SERVER     4       0       24     0
    VLCROW enabled LDT_APPL_A  NOOP_SERVER          4       0       4      0
    VLCROW enabled LDT_APPL_A  UNUSED_VF_V32        0       0       0      0
    VLCROW enabled LDT_APPL_A  V_SERVER_W_DCL       1       0       1      0
    VLCROW enabled LDT_APPL_A  I_SERVER_W_DCL       1       0       1      0
    VLCROW enabled LDT_APPL_A  DETASK_SERVER        2       0       3      0

> Previous | Next | Contents | Index