Document revision date: 30 March 2001

## Guidelines for OpenVMS Cluster Configurations

Previous | Contents | Index

T
T3 communications service
Tapes
backup
capacity
performance
TCP/IP Services
network transport
Terminal servers
for availability
Terminators
for SCSI
Third-party products
storage requirements
Throughput
CI
Ethernet
FDDI
MEMORY CHANNEL
SCSI
Timers
polling
TIMVCFAIL system parameter
TMSCP servers
role in OpenVMS Cluster
Traffic isolation
in extended LANs
Troubleshooting
SCSI configurations
U
User data
storage requirements
User-written programs
storage requirements
V
VAX CDD/Repository
VAX systems
coexisting with Alpha systems #1
coexisting with Alpha systems #2
coexisting with Alpha systems #3
Virtual I/O cache
VLGBICs (very long Gigabit interface converters)
VMSMAIL_PROFILE.DATA file
Volume shadowing
Fibre Channel devices
multipath devices #1
multipath devices #2
Volume Shadowing for OpenVMS
across controllers
across nodes
description
effect on I/O throughput
for OpenVMS Cluster availability
guidelines in CI OpenVMS Clusters
inside a controller
minicopy
MSCP overhead
OpenVMS Cluster availability
RAID level 1
read performance
read/write ratio
scalability
support in SCSI OpenVMS Cluster configurations
with striping
VOTES system parameter
W
WAN intersite link specifications
WAN requirements
multisite cluster
Bellcore Communications Research
OpenVMS Cluster
WAN T3/SONET option card #1
WAN T3/SONET option card #2
management information
protocol options
WANs (wide area networks)
using in a multiple-site OpenVMS Cluster system
Warranted support
Wide area networks
See WANs
Workstations
Alpha #1
Alpha #2
uses
WWID
See Device IDs
Fibre Channel
wwidmgr -quickset command
wwidmgr -show wwid command
X
XFC
See Extended File Cache

| privacy and legal statement |
6318PRO_INDEX_004.HTML