Document revision date: 30 March 2001

## OpenVMS System Messages: Companion Guide for Help Message Users

Previous | Contents | Index

> JBCMIXUP, fatal job controller interaction problem

Facility: LOGIN, Login Procedure
Explanation: An internal error occurred in the job controller during the login; the login cannot be performed.
User Action: Repeat the login procedure. If the failure persists, notify the system operator or manager.

> JNLACP, Fatal error detected by journal ACP

Facility: BUGCHECK, System Bugcheck
Explanation: The OpenVMS software detected an irrecoverable, inconsistent condition. After all physical memory is written to a system dump file, the system automatically reboots if the BUGREBOOT system parameter is set to 1.
User Action: Use the BACKUP command with the /IGNORE=NOBACKUP qualifier to make a backup save set of the system dump file and the error log file active at the time of the error. Contact a Compaq support representative and describe the conditions leading to the error.

> JNLDRV, Fatal error detected by journal driver

Facility: BUGCHECK, System Bugcheck
Explanation: The OpenVMS software detected an irrecoverable, inconsistent condition. After all physical memory is written to a system dump file, the system automatically reboots if the BUGREBOOT system parameter is set to 1.
User Action: Use the BACKUP command with the /IGNORE=NOBACKUP qualifier to make a backup save set of the system dump file and the error log file active at the time of the error. Contact a Compaq support representative and describe the conditions leading to the error.

> JOURNAL, journaling to 'file-spec'

Facility: BACKUP, Backup Utility
Explanation: The Backup utility is writing journal records to the specified file in response to the /JOURNAL qualifier. This message is displayed only if the /LOG qualifier is specified.
User Action: None.

> KRNLSTAKNV, kernel stack not valid

Facility: BUGCHECK, System Bugcheck
Explanation: The OpenVMS software detected an irrecoverable, inconsistent condition. After all physical memory is written to a system dump file, the system automatically reboots if the BUGREBOOT system parameter is set to 1.
User Action: Use the BACKUP command with the /IGNORE=NOBACKUP qualifier to make a backup save set of the system dump file and the error log file active at the time of the error. Contact a Compaq support representative and describe the conditions leading to the error.

> LABELERR, error in tape label processing on 'save-set-spec'

Facility: BACKUP, Backup Utility
Explanation: The Backup utility encountered an error during an attempt to process the file labels on the specified volume.
User Action: Take action based on the accompanying message.

> LARGECNT, 'device-name' is too large to be processed

Facility: BACKUP, Backup Utility
Explanation: The specified volume is too large to be processed by the Backup utility. Possibly the specified cluster factor is too small.
User Action: Retry the operation using a larger volume cluster factor.

> LBLOVRWRITE, volume label 'label' overwritten, new label is 'label'

Facility: BACKUP, Backup Utility
Explanation: The loaded volume was overwritten and a new label was written to the volume. The labels specified in this message provide additional information.
User Action: None.

> LINE_TRUNCATED, more than 'number' characters in line, at line 'line-number'.

Facility: READ_CONFIG, File-Based Autoconfiguration
Explanation: The command line exceeds the maximum allowable number of characters. The device description will not be added.
User Action: Correct the command so that it contains 256 or fewer characters, and retry the operation.

> LISINPSAV, /LIST requires save set as input

Facility: BACKUP, Backup Utility
Explanation: The input specification for a listing operation must reference a save set.
User Action: Correct the specification and reenter the command.

> LKBGRANTED, LKB is granted, but shouldn't be

Facility: BUGCHECK, System Bugcheck
Explanation: The OpenVMS software detected an irrecoverable, inconsistent condition. After all physical memory is written to a system dump file, the system automatically reboots if the BUGREBOOT system parameter is set to 1.
User Action: Use the BACKUP command with the /IGNORE=NOBACKUP qualifier to make a backup save set of the system dump file and the error log file active at the time of the error. Contact a Compaq support representative and describe the conditions leading to the error.

> LKBREFNEG, LKB reference count negative

Facility: BUGCHECK, System Bugcheck
Explanation: The OpenVMS software detected an irrecoverable, inconsistent condition. After all physical memory is written to a system dump file, the system automatically reboots if the BUGREBOOT system parameter is set to 1.
User Action: Use the BACKUP command with the /IGNORE=NOBACKUP qualifier to make a backup save set of the system dump file and the error log file active at the time of the error. Contact a Compaq support representative and describe the conditions leading to the error.

> LOADERR, error configuring device 'device-name', driver 'driver-name'

Facility: IOGEN
Explanation: An error occurred during autoconfiguration.
User Action: Take action based on the accompanying message.

> LOCKERR, failed to lock volume

Facility: RBLD, REBUILD Command (Mount Utility)
Explanation: An error occurred while trying to lock the volume set against modification.
User Action: Take action based on the accompanying message.

> LOCKMGRERR, error detected by Lock Manager

Facility: BUGCHECK, System Bugcheck
Explanation: The OpenVMS software detected an irrecoverable, inconsistent condition. After all physical memory is written to a system dump file, the system automatically reboots if the BUGREBOOT system parameter is set to 1.
User Action: Use the BACKUP command with the /IGNORE=NOBACKUP qualifier to make a backup save set of the system dump file and the error log file active at the time of the error. Contact a Compaq support representative and describe the conditions leading to the error.

> LOGDISABL, logins are currently disabled - try again later

Facility: LOGIN, Login Procedure
Explanation: Logins are currently disabled.
User Action: Do not attempt to log in at this time. Try again later.

> LOGNAME, logical name is too long

Facility: MOUNT, Mount Utility
Explanation: A logical name contains more than 255 characters.
User Action: Correct and reenter the command.

Low Priority Command Queue Insert Failure
Facility: Cluster Port Driver
Explanation: The port driver attempts to reinitialize the port; after 50 failed attempts, it marks the device off line. This error is caused by a failure to obtain access to an interlocked queue. Possible sources of the problem are CI hardware failures or memory, SBI (VAX-11/780), CMI (VAX-11/750), BI, PCI, or XMI contention.
User Action: Contact a Compaq support representative.

Previous | Next | Contents | Index

| privacy and legal statement |
6023PRO_010.HTML