# Compaq OpenVMS
OpenVMS Cluster 構成ガイド

前へ | 次へ | 目次 | 索引

# 7.7 OpenVMS で使用するための HSG のセットアップ

この節では，OpenVMS に HSG を使用するための基本セットアップ要件を説明します。 HSG60 と HSG80 のセットアップ手順は同じですが，ここに示す例は， HSG80 の出力です。詳細については，『HSG80 Array Controller ACS Version 8.4 Configuration and CLI Reference Guide 』を参照してください。

以下に，OpenVMS 用に HSG を構成するための手順を示します。

1. HSG にデュアル・コントローラがある場合は，マルチバス・フェールオーバ・モードに設定します ( 第 7.7.1 項 )。

2. コントローラの SCSI バージョンは SCSI-3 に設定します ( 第 7.7.2 項 )。

   注意 コントローラの割り当てクラスの値は設定する必要はありません。このパラメータは， HSG 付きの OpenVMS では使用しないからです。

3. OpenVMS から HSG コマンド・コンソール LUN (CCL) にアクセスする場合，デバイス識別子に割り当ててください ( 第 7.7.3 項 )。
   これにより，OpenVMS は CCL を汎用 SCSI デバイスとして構成します。

   注意 OpenVMS の現在のバージョンでは，デバイス識別子を CCL に割り当てる必要があります。この要件は，将来のアップデートでは解消される予定です。

4. HSG FC ポートのパラメータを設定します ( 第 7.7.4 項 )。
   各ポートの FC プロファイルは，PLDA に設定し，そのトポロジは FABRIC に設定します。

5. 論理ユニットを HSG 構成に追加します ( 第 7.7.5 項 )。
   このとき，論理ユニット番号とデバイス識別子を各論理ユニットに割り当てる必要があります。

   注意 論理ユニットの優先パス・パラメータは設定不要です。OpenVMS では，パス選択時に優先パス・パラメータを使用しません。

6. HSG ホスト接続テーブルを構成します ( 第 7.7.6 項 )。

## 7.7.1 デュアル HSG をマルチバス・フェールオーバ・モードに設定

デュアル HSG をマルチバス・フェールオーバ・モードに設定するとき， HSG コンソールで以下のコマンドを使用できます。

- デュアル・コントローラがフェールオーバに構成されているかどうかを確認するための最初の SHOW コマンド。

- コントローラをマルチバス・モードにするための SET コマンド。他のコントローラが再起動します。

- デュアル・コントローラがマルチバス・フェールオーバに構成されたかどうかを確認するための 2 番目の SHOW コマンド。

以上のコマンドの出力を 例 7-5 に示します。

例 7-5 デュアル HSG をマルチバス・フェールオーバ・モードに設定
    HSG> SHOW THIS_CONTROLLER
    Controller:
            HSG80 ZG80900677 Software R024F-0，Hardware  E01
            NODE_ID          = 5000-1FE1-0000-0D10
            ALLOCATION_CLASS = 0
            SCSI_VERSION     = SCSI-2
            Not configured for dual-redundancy
                Controller misconfigured -- other controller present
            Device Port SCSI address 6
            Time: NOT SET
            Command Console LUN is disabled
    Host PORT_1:
            Reported PORT_ID = 5000-1FE1-0000-0D11
            PORT_1_PROFILE   = SCC
            PORT_1_TOPOLOGY  = OFFLINE (offline)
    Host PORT_2:
            Reported PORT_ID = 5000-1FE1-0000-0D12
            PORT_2_PROFILE   = SCC
            PORT_2_TOPOLOGY  = OFFLINE (offline)
            NOREMOTE_COPY
    Cache:
            128 megabyte write cache，version 0012
            Cache is GOOD
            No unflushed data in cache
            CACHE_FLUSH_TIMER = DEFAULT (10 seconds)
    Mirrored Cache:
            Not enabled
    Battery:
            FULLY CHARGED
            Expires:             27-APR-2000
            NOCACHE_UPS
    %CER--HSG> --13-JAN-1946 04:32:49 (time not set)-- Controllers misconfigured. -
    Type SHOW THIS_CONTROLLER

    HSG> SET MULTIBUS_FAILOVER COPY = THIS_CONTROLLER

    %EVL--HSG> --13-JAN-1946 04:38:37 (time not set)-- Instance Code: 07050064 (not
    yet reported to host)
    Template: 5.(05)
    Power On Time: 0. Years，284. Days，5. Hours，18. Minutes，27. Seconds
    Controller Model: HSG80
    Serial Number: ZG80900677 Hardware Version:  E01(29)
    Software Version: R024F(FF)
    Informational Report
    Instance Code: 07050064
    Last Failure Code: 08080000 (No Last Failure Parameters)

    %EVL--HSG> --13-JAN-1946 04:38:37 (time not set)-- Instance Code: 43010064 (not
    yet reported to host)
    Template: 4.(04)
    Power On Time: 0. Years，284. Days，5. Hours，18. Minutes，28. Seconds
    Controller Model: HSG80
    Serial Number: ZG80900677 Hardware Version:  E01(29)
    Software Version: R024F(FF)
    Informational Report
    Other Controller Serial Number: ZG80900641
    Failed Controller Target Number: 0.(00)
    LUNs Taken By This Controller:
      00000000
      00000000
      00000000
      00000000
      00000000
      00000000
      00000000
      00000000
    Instance Code: 43010064

    ...
    %CER--HSG> --13-JAN-1946 04:38:37 (time not set)-- Received LAST GASP message-
    from other controller，Last Failure Code: 08080000
    HSG>

    ...
    %CER--HSG> --13-JAN-1946 04:39:23 (time not set)-- Other controller restarted
    HSG> SHOW THIS_CONTROLLER
    Controller:
            HSG80 ZG80900677 Software R024F-0，Hardware  E01
            NODE_ID          = 5000-1FE1-0000-0D10
            ALLOCATION_CLASS = 0
            SCSI_VERSION     = SCSI-2
            Configured for MULTIBUS_FAILOVER with ZG80900641
                In dual-redundant configuration
            Device Port SCSI address 6
            Time: NOT SET
            Command Console LUN is disabled
    Host PORT_1:
            Reported PORT_ID = 5000-1FE1-0000-0D11
            PORT_1_PROFILE   = SCC
            PORT_1_TOPOLOGY  = OFFLINE (offline)
    Host PORT_2:
            Reported PORT_ID = 5000-1FE1-0000-0D12
            PORT_2_PROFILE   = SCC
            PORT_2_TOPOLOGY  = OFFLINE (offline)
            NOREMOTE_COPY
    Cache:
            128 megabyte write cache，version 0012
            Cache is GOOD
            No unflushed data in cache
            CACHE_FLUSH_TIMER = DEFAULT (10 seconds)
    Mirrored Cache:
            Not enabled
    Battery:
            FULLY CHARGED
            Expires:             27-APR-2000
            NOCACHE_UPS
    Other controller restarted

## 7.7.2 HSG を SCSI-3 モードに設定

例 7-6 は，HSG を SCSI-3 モードに設定する方法を示したものです。デュアル構成の他のコントローラは，自動的に同じモードに設定されます。この設定を有効にするには，コントローラを再起動する必要があります。

例 7-6 HSG を SCSI-3 モードに設定
    HSG> SET THIS_CONTROLLER SCSI_VERSION = SCSI-3
    Warning 4030: Any units that would appear as unit 0 to a host will not be
                  available when in SCSI-3 mode
    Warning 4020: A restart of both this and the other controller is required
                  before all the parameters modified will take effect
    %CER--HSG> --13-JAN-1946 04:42:28 (time not set)-- Restart of this controller-
    required
    %CER--HSG> --13-JAN-1946 04:42:28 (time not set)-- Restart of the other-
    controller required
    Restart of this controller required
    Restart of the other controller required

## 7.7.3 デバイス識別子を CCL 用に設定

OpenVMS で CCL を構成する場合は，コントローラのペアに同じ識別子を割り当てる必要があります。この識別子は，クラスタ内のすべての HSG コントローラのペアに対して一意にする必要があります。

以下のコマンドは，コントローラのペアの CCL 用のデバイス識別子を 42 に設定します。これにより，OpenVMS は CCL を汎用 SCSI デバイスに構成します。デバイス名は $1$GGA42 になります。 SHOW THIS_CONTROLLER コマンドで設定を確認してください。

    HSG> SET THIS_CONTROLLER IDENTIFIER = 42

注意 OpenVMS の現在のバージョンでは，CCL にデバイス識別子を割り当てる必要があります。この要件は，将来のアップデートで解消される予定です。

## 7.7.4 HSG ポート・パラメータの設定

各 HSG ポートのプロファイルを PLDA に設定し，トポロジを FABRIC に設定するには， 例 7-7 に示すコマンドを使用します。設定は， SHOW THIS コマンドと SHOW OTHER コマンドで確認できます。

各ポートには，5000-1FE1-0000-0D11 という形式の一意の 64 ビット識別子が割り当てられます。これらの識別子は，ラベル `Reported PORT_ID`の次の SHOW THIS 表示と SHOW OTHER 表示で確認できます。ホストと論理ユニットの間に設定できる複数のパスを，OpenVMS はこれらの識別子で表します。

注意 例 7-7 に示す，コマンド `HSG> SET THIS_CONTROLLER PORT_1_PROFILE=PLDA`は， ACS 8.4 を使用している場合に必要です。ACS 8.5 以上を使用している場合は，この手順を実行する必要はありません。)

例 7-7 HSG ポート・パラメータの設定
    HSG> SET THIS_CONTROLLER PORT_1_PROFILE = PLDA
    Warning 4000: A restart of this controller is required before all the
                  parameters modified will take effect
    %CER--HSG> --17-MAR-1999 12:24:09-- Restart of this controller required
    Restart of this controller required
    HSG> SET THIS_CONTROLLER PORT_1_TOPOLOGY = FABRIC
    Warning 4000: A restart of this controller is required before all the
                  parameters modified will take effect
    %CER--HSG> --17-MAR-1999 12:25:02-- Restart of this controller required
    Restart of this controller required
    HSG> SET THIS_CONTROLLER PORT_2_PROFILE = PLDA
    Warning 4000: A restart of this controller is required before all the
                  parameters modified will take effect
    %CER--HSG> --17-MAR-1999 12:25:26-- Restart of this controller required
    Restart of this controller required
    HSG> SET THIS_CONTROLLER PORT_2_TOPOLOGY = FABRIC
    Warning 4000: A restart of this controller is required before all the
                  parameters modified will take effect
    %CER--HSG> --17-MAR-1999 12:25:39-- Restart of this controller required
    Restart of this controller required

    HSG> SHOW THIS_CONTROLLER
    Controller:
            HSG80 ZG80900677 Software R024F-0，Hardware  E01
            NODE_ID          = 5000-1FE1-0000-0D10
            ALLOCATION_CLASS = 0
            SCSI_VERSION     = SCSI-3
            Configured for MULTIBUS_FAILOVER with ZG80900641
                In dual-redundant configuration
            Device Port SCSI address 6
            Time: 17-MAR-1999 12:25:55
            Command Console LUN is lun 0 (IDENTIFIER = 42)
    Host PORT_1:
            Reported PORT_ID = 5000-1FE1-0000-0D11
            PORT_1_PROFILE   = PLDA
            PORT_1_TOPOLOGY  = FABRIC (offline)
    Host PORT_2:
            Reported PORT_ID = 5000-1FE1-0000-0D12
            PORT_2_PROFILE   = PLDA
            PORT_2_TOPOLOGY  = FABRIC (offline)
            NOREMOTE_COPY
    Cache:
            128 megabyte write cache，version 0012
            Cache is GOOD
            No unflushed data in cache
            CACHE_FLUSH_TIMER = DEFAULT (10 seconds)
    Mirrored Cache:
            Not enabled
    Battery:
            FULLY CHARGED
            Expires:             27-APR-2000
            NOCACHE_UPS

    HSG> SET OTHER_CONTROLLER PORT_1_PROFILE = PLDA
    Warning 4010: A restart of the other controller is required before all the
                  parameters modified will take effect
    %CER--HSG> --17-MAR-1999 12:26:46-- Restart of the other controller required
    Restart of the other controller required
    HSG> SET OTHER_CONTROLLER PORT_1_TOPOLOGY = FABRIC
    Warning 4010: A restart of the other controller is required before all the
                  parameters modified will take effect
    %CER--HSG> --17-MAR-1999 12:26:59-- Restart of the other controller required
    Restart of the other controller required
    HSG> SET OTHER_CONTROLLER PORT_2_PROFILE = PLDA
    Warning 4010: A restart of the other controller is required before all the
                  parameters modified will take effect
    %CER--HSG> --17-MAR-1999 12:27:08-- Restart of the other controller required
    Restart of the other controller required
    HSG> SET OTHER_CONTROLLER PORT_2_TOPOLOGY = FABRIC
    Warning 4010: A restart of the other controller is required before all the
                  parameters modified will take effect
    %CER--HSG> --17-MAR-1999 12:27:15-- Restart of the other controller required
    Restart of the other controller required

    HSG> SHOW OTHER_CONTROLLER
    Controller:
            HSG80 ZG80900641 Software R024F-0，Hardware  E01
            NODE_ID          = 5000-1FE1-0000-0D10
            ALLOCATION_CLASS = 0
            SCSI_VERSION     = SCSI-3
            Configured for MULTIBUS_FAILOVER with ZG80900677
                In dual-redundant configuration
            Device Port SCSI address 7
            Time: 17-MAR-1999 12:27:31
            Command Console LUN is lun 0 (IDENTIFIER = 42)
    Host PORT_1:
            Reported PORT_ID = 5000-1FE1-0000-0D13
            PORT_1_PROFILE   = PLDA
            PORT_1_TOPOLOGY  = FABRIC (offline)
    Host PORT_2:
            Reported PORT_ID = 5000-1FE1-0000-0D14
            PORT_2_PROFILE   = PLDA
            PORT_2_TOPOLOGY  = FABRIC (offline)
            NOREMOTE_COPY
    Cache:
            128 megabyte write cache，version 0012
            Cache is GOOD
            No unflushed data in cache
            CACHE_FLUSH_TIMER = DEFAULT (10 seconds)
    Mirrored Cache:
            Not enabled
    Battery:
            FULLY CHARGED
            Expires:             27-APR-2000
            NOCACHE_UPS

## 7.7.5 HSG における論理ユニットのセットアップ

HSG における論理ユニットのセットアップの手順を 例 7-8 を基に以下に示します。

1. HSG 上のすべての物理ディスク装置を CONFIG コマンドで構成します。

2. 各ディスク装置を論理ユニットとして以下のように構成します。

   1. INITIALIZE コマンドでディスクを初期化します。

   2. ホストが認識できる論理ユニットとして初期化したディスクを ADD コマンドで追加します。
      HSG ストレージ・サブシステムで一意の論理ユニット番号を選択します。 例 7-8 では 20 を選択しています。そのため，論理ユニット名は D20 になります。

   3. OpenVMS デバイス名の基本になるデバイス識別子を SET コマンドで設定します。
      このデバイス識別子は，OpenVMS Cluster のすべての FC ディスクに対して一意であるものとします。 例 7-8 では 32020 を選択しています。そのため，論理ユニットの OpenVMS デバイス名は $1$DGA32020 になります。
      注意: FC デバイスが MSCP サービス対象の場合，このデバイス識別子に使用できる最大文字数は 9999 です。この制限事項は将来のリリースで解消される予定です。

例 7-8 HSG における論理ユニットのセットアップ
    HSG> RUN CONFIG

    Config Local Program Invoked

    Config is building its tables and determining what devices exist
    on the subsystem. Please be patient.

    add disk DISK10000   1 0 0
    add disk DISK10100   1 1 0
    add disk DISK10200   1 2 0
    add disk DISK20000   2 0 0

    Config - Normal Termination
    HSG> SHOW DISK FULL
    Name          Type                      Port Targ  Lun        Used by
    ------------------------------------------------------------------------------
    ...
    DISK20000     disk                         2    0    0
              DEC      RZ1CD-CS (C) DEC 0306
            Switches:
              NOTRANSPORTABLE
              TRANSFER_RATE_REQUESTED = 20MHZ (synchronous 20.00 MHZ negotiated)
            Size: 8378028 blocks

    HSG> SHOW UNITS
    No LUNs
    HSG> INITIALIZE DISK20000
    HSG> ADD UNIT D20 DISK20000
    HSG> SET D20 IDENTIFIER = 32020
    HSG> SHOW UNITS FULL
        LUN                                      Uses             Used by
    ------------------------------------------------------------------------------

      D20                                        DISK20000
            LUN ID:      6000-1FE1-0000-0D10-0009-8090-0677-0024
            IDENTIFIER = 32020
            Switches:
              RUN                    NOWRITE_PROTECT        READ_CACHE
              READAHEAD_CACHE        WRITEBACK_CACHE
              MAXIMUM_CACHED_TRANSFER_SIZE = 32
            Access:
                    ALL
            State:
              ONLINE to this controller
              Not reserved
              NOPREFERRED_PATH
            Size: 8378028 blocks
            Geometry (C/H/S): ( 3708 / 20 / 113 )

## 7.7.6 HSG ホスト接続の構成

HSG で，デフォルトのホスト接続情報を自動的に作成できます。また，ホスト接続情報はマニュアルでも設定できます。詳細については，『HSG80 Array Controller ACS Version 8.4 Configuration and CLI Reference Guide 』を参照してください。自動設定をする場合，デフォルト設定を変更する必要があります。

初めて使用するときには，HSG にホスト接続は設定されていません。ホストを FC インターコネクトに接続し電源を入れると，HSG はホストを認識し， 例 7_9 のようにデフォルトの接続情報を作成します。このデフォルト情報の作成後，接続値を環境に応じた意味の値に変更できます。 例 7-9 を参照してください。

さらに，次の作業をします。

- オペレーティング・システム名を各接続の VMS に設定します。 例 7-9 を参照してください。

- 各接続の装置オフセット値がゼロ (0) に設定されているか，確認します。ゼロになっていない場合は，ゼロに設定します。

例 7-9 HSG ホスト接続の構成
    HSG> SHOW CONNECTIONS
    No Connections
    HSG> SHOW CONNECTIONS
    Connection                                                                Unit
       Name      Operating System    Controller  Port    Address    Status   Offset

    !NEWCON44         WINNT             THIS       2      210713   OL this       0
               HOST_ID=1000-0000-C920-A7DB         ADAPTER_ID=1000-0000-C920-A7DB

    !NEWCON45         WINNT             OTHER      2      210713   OL other      0
               HOST_ID=1000-0000-C920-A7DB         ADAPTER_ID=1000-0000-C920-A7DB

    !NEWCON46         WINNT             THIS       1      210713   OL this       0
               HOST_ID=1000-0000-C920-A694         ADAPTER_ID=1000-0000-C920-A694

    !NEWCON47         WINNT             OTHER      1      210713   OL other      0
               HOST_ID=1000-0000-C920-A694         ADAPTER_ID=1000-0000-C920-A694
    HSG> RENAME !NEWCON44 FCNOD1A_T
    HSG> RENAME !NEWCON45 FCNOD1A_O
    HSG> RENAME !NEWCON46 FCNOD1B_T
    HSG> RENAME !NEWCON47 FCNOD1B_O
    HSG> SHOW CONNECTIONS
    Connection                                                                Unit
       Name      Operating System    Controller  Port    Address    Status   Offset

    FCNOD1A_O          WINNT             OTHER      2      210713   OL other      0
               HOST_ID=1000-0000-C920-A7DB         ADAPTER_ID=1000-0000-C920-A7DB

    FCNOD1A_T          WINNT             THIS       2      210713   OL this       0
               HOST_ID=1000-0000-C920-A7DB         ADAPTER_ID=1000-0000-C920-A7DB

    FCNOD1B_O          WINNT             OTHER      1      210713   OL other      0
               HOST_ID=1000-0000-C920-A694         ADAPTER_ID=1000-0000-C920-A694

    FCNOD1B_T          WINNT             THIS       1      210713   OL this       0
               HOST_ID=1000-0000-C920-A694         ADAPTER_ID=1000-0000-C920-A694
    HSG> SET FCNOD1A_O OPERATING_SYSTEM = VMS
    HSG> SET FCNOD1A_T OPERATING_SYSTEM = VMS
    HSG> SET FCNOD1B_O OPERATING_SYSTEM = VMS
    HSG> SET FCNOD1B_T OPERATING_SYSTEM = VMS
    HSG> SHOW CONNECTIONS
    Connection                                                                Unit
       Name      Operating System    Controller  Port    Address    Status   Offset

    FCNOD1A_O           VMS              OTHER      2      210713   OL other      0
               HOST_ID=1000-0000-C920-A7DB         ADAPTER_ID=1000-0000-C920-A7DB

    FCNOD1A_T           VMS              THIS       2      210713   OL this       0
               HOST_ID=1000-0000-C920-A7DB         ADAPTER_ID=1000-0000-C920-A7DB

    FCNOD1B_O           VMS              OTHER      1      210713   OL other      0
               HOST_ID=1000-0000-C920-A694         ADAPTER_ID=1000-0000-C920-A694

    FCNOD1B_T           VMS              THIS       1      210713   OL this       0
               HOST_ID=1000-0000-C920-A694         ADAPTER_ID=1000-0000-C920-A694

前へ | 次へ | 目次 | 索引