# Compq OpenVMS
システム管理ユーティリティ・リファレンス・マニュアル

前へ | 次へ | 目次 | 索引

# 10.4 ANALYZE/ERROR_LOG ユーティリティの出力例

エラー・ログ・レポート例

エラー・ログ・レポート・エントリは，識別部分と装置依存データ部分 2 つの部分から構成されます。識別部分は， 1 から 4 行目までで，すべてのレポートに対して作成されます。識別部分に続く装置依存データ部分には，選択したエラー・ログ・エントリの情報が格納されます。

識別部分の 1 行目は，エラー・エントリ番号です。この番号により，エラー・ログ・ファイルの特定のエラー・ログ・エントリを指定できます。 2 行目は，エラー・シーケンス番号とシステム識別値です。エラー・シーケンス番号は，エラー・ログ・エントリが消失したかどうかを判定することを目的としてオペレーティング・システムが設定する値です。このシーケンス番号は，システムを再ブートしたときに 0 に再設定されます。3，4 行目は，レポート対象のエラー・ログ・エントリのタイプ，エントリを入力した日時，プロセッサ・タイプと改訂レベル，システム・シリアル番号です。

装置依存データ部分の 1 行目は，エラーが発生した装置またはサブシステムを示します。その他の部分は，装置レジスタの内容を示すハードウェア情報と，エラー発生時の入出力データベースの内容を示すソフトウェア情報です。

エラー・ログ・エントリを始めとするエラー・ログ・レポートの詳細については，『Compaq OpenVMS システム管理者マニュアル』を参照してください。それぞれのエントリに適した処理が説明されています。

次のレポートは，システム上のディスクの装置エラー，装置アテンション，装置タイムアウト別の出力例です。

     Error Log Report Generator                                         Version 7.3

     ******************************* ENTRY     904. *******************************
     ERROR SEQUENCE 709.                             LOGGED ON:  CPU_TYPE 00000002
     DATE/TIME 20-AUG-2000 15:21:10.79                           SYS_TYPE 00000003
     SYSTEM UPTIME: 1 DAYS 01:35:47
     SCS NODE: LSR3                                                 OpenVMS V7.3

     DEVICE ERROR SYS_TYPE = 03

     RZ57 SUB-SYSTEM, UNIT _LSR3$DKA0:

           HW REVISION     30303035
                                           HW REVISION = 5000
           ERROR TYPE            03
                                           COMMAND TRANSMISSION FAILURE
           SCSI ID               00
                                           SCSI ID = 0.
           SCSI LUN              00
                                           SCSI LUN = 0.
           SCSI SUBLUN           00
                                           SCSI SUBLUN = 0.
           PORT STATUS     00000054
                                           %SYSTEM-F-CTRLERR, FATAL CONTROLLER
                                            ERROR
           SCSI CMD        00000000
                               0000
                                           TEST UNIT RDY
           SCSI STATUS           FF
                                           NO STATUS RECEIVED
           UCB$B_ERTCNT          0F
                                           15. RETRIES REMAINING
           UCB$B_ERTMAX          00
                                           0. RETRIES ALLOWABLE
           ORB$L_OWNER     00000000
                                           OWNER UIC [000,000]
           UCB$L_CHAR      1CC54008
                                           DIRECTORY STRUCTURED
                                           FILE ORIENTED
                                           SHARABLE
                                           AVAILABLE
                                           ERROR LOGGING
                                           ALLOCATED
                                           CAPABLE OF INPUT
                                           CAPABLE OF OUTPUT
                                           RANDOM ACCESS
           UCB$L_STS           56544552
                                           INTERRUPT EXPECTED
                                           ONLINE
                                           TIMED OUT
                                           BUSY
                                           DEALLOCATE AT DISMOUNT
                                           "MOUNT VERIFICATION" IN-PROGRESS
           UCB$L_OPCNT     00000000
                                           0. QIO'S THIS UNIT
           UCB$W_ERRCNT        0001
                                           1. ERRORS THIS UNIT
           Error Log Report Generator                                   Version 7.3

           IRP$L_BCNT          00000000
                                           TRANSFER SIZE 0. BYTE(S)
           IRP$L_BOFF          00000000
                                           TRANSFER PAGE ALIGNED
           IRP$L_PID       00010042
                                           REQUESTOR "PID"
           IRP$Q_IOSB      0000014E
                           430A0002        IOSB, 0. BYTE(S) TRANSFERRED

タイムスタンプ，ボリューム・マウント，ボリューム・ディスマウント・エントリ例

システム・タイムスタンプ，ボリューム・マウント，ボリューム・ディスマウントのエントリ例を次に示します。タイムスタンプ・エントリは，10 分間隔でオペレーティング・システムが記録する識別部分だけで構成されます。 10 分以内に新たなエラー・ログ・エントリが記録されない場合，以前のタイムスタンプは，現在のタイムスタンプで上書きされます。

マウント・ボリューム・エントリは，識別部分と装置依存データ部分で構成されます。装置依存データ部分は，ボリュームがマウントされている装置の名前，ボリュームにラベルがある場合そのラベル，装置の入出力処理とエラー回数を示します。

ディスマウント・ボリューム・エントリは，ボリューム・マウント・エントリのデータに加えて，ボリュームがマウントされていた装置の入出力処理とエラー回数を示します。

    **************************** ENTRY      93. ****************************
    ERROR SEQUENCE 421.                               LOGGED ON SID 01380101

    TIME STAMP, 4-MAR-00 11:10:08.79
                KA780 REV# 7. SERIAL# 7.
    **************************** ENTRY      94. ****************************
    ERROR SEQUENCE 422.                               LOGGED ON SID 01380101

    MOUNT VOLUME, 4-MAR-00 11:14:12.51
                  KA780 REV# 7. SERIAL# 7.

          UNIT _DMA0:, VOLUME LABEL "TEST"

          656. QIO OPERATIONS THIS UNIT, 1. ERRORS THIS UNIT
    **************************** ENTRY      95. ****************************
    ERROR SEQUENCE 423.                               LOGGED ON SID 01380101

    DISMOUNT VOLUME, 4-MAR-00 11:14:41.30
                     KA780 REV# 7. SERIAL# 7.

          UNIT _DMA0:, VOLUME LABEL "TEST"

          697. QIO OPERATIONS THIS UNIT, 1. ERRORS THIS UNIT
          41. QIO OPERATIONS THIS VOLUME, 0. ERRORS THIS VOLUME

マシン・チェック・エントリ例

マシン・チェック・エラーのレポート例を次に示します。このレポートは，識別部分，プログラム・カウンタと要約コード部分，エラー依存部分で構成されます。

プログラム・カウンタと要約コード部分は，プログラム・カウンタ，プロセッサ状態ロングワード，要約コードの内容を示します。プロセッサ状態ロングワードと要約コードの内容は，レポートの右側にテキストで記述されます。

エラー依存部分は，マシン・チェックの結果記録された CPU 依存情報を示します。

     ******************************* ENTRY       2. *******************************
     ERROR SEQUENCE 2.                                LOGGED ON:  CPU_TYPE 00000002
     DATE/TIME  4-SEP-2000 09:39:51.19                            SYS_TYPE 00000002
     SYSTEM UPTIME: 90 DAYS 00:01:25
     SCS NODE: COBRA6                                               OpenVMS V7.3
     MACHINE CHECK SYS_TYPE = 02
     KERNEL EVENT HEADER
           FRAME REVISION      0000
           SCB VECTOR          0670
           1ST MOST PRB FRU      00
                                           FIELD NOT VALID
           2ND MOST PRB FRU      00
                                           FIELD NOT VALID
           SEVERITY            0000
                                           FIELD NOT VALID
           CPU ID              0000
           ERROR COUNT         0001
           THRESHOLD           0000
           FAIL CODE           0000
           ERR FIELD LOW   00000005
                           00000008
                                           CPU_0 BUS COMMAND NO-ACK
                                           CPU_O BUS READ PARITY ERROR
                                           CPU CYCLE ABORTED WITH HARD ERROR
           ERR FIELD HIGH  00000000
                           00000000
           RETRY/BYTE CNT  00000250
                           00000000
                                           BYTE COUNT = 00000250(X)
                                           CAN'T RETRY
           PALTEMP0        00000001
                           00000000
           PALTEMP1        000000BE
                           00000000
           PALTEMP2        00000004
                           001FC0F8
           PALTEMP3        00000000
                           00000000
           PALTEMP4        805C3FC0
                           FFFFFFFF
           PALTEMP5        00000000
                           00000000
           PALTEMP6        84FDE000
                           FFFFFFFF
           PALTEMP7        00004200
                           00000000
           PALTEMP8        00000400
                           00000000
           PALTEMP9        00000003
                           00000000
           PALTEMP10       29CB0233
                           00000003
           PALTEMP11       00000000
                           00000000
           PALTEMP12       00000001

           Error Log Report Generator                                   Version 7.3

                           00000000
           PALTEMP13       8042F4C0
                           FFFFFFFF
           PALTEMP14       00000000
                           00000000
           PALTEMP15       00000000
                           00000000
           PALTEMP16       0000C000
                           00000000
           PALTEMP17       00000000
                           00000000
           PALTEMP18       BEBC2000
                           00000000
           PALTEMP19       7FFBF924
                           00000000
           PALTEMP20       00002041
                           00000000
           PALTEMP21       40000000
                           00000002
           PALTEMP22       00000000
                           00000000
           PALTEMP23       00000000
                           00000000
           PALTEMP24       805C0000
                           FFFFFFFF
           PALTEMP25       00000000
                           00000000
           PALTEMP26       7FF96000
                           00000000
           PALTEMP27       00000000
                           00000000
           PALTEMP28       00D7C000
                           00000000
           PALTEMP29       00000000
                           00000002
           PALTEMP30       002F6000
                           00000000
           PALTEMP31       00D62080
                           00000000
           EXCP ADDR REG   0000815E
                           00000000
                                           Not PALmode instruction
                                           EXCEPTION PC  = 0000000000002057(X)
           EXCP SUM REG    00000000
                           00000000
           EXCP MASK REG   00000000
                           00000000
           ICCS REG        00000004
                           001FC0F8
           PAL BASE        00008000
                           00000000
                                           PAL BASE PA = 000008000(X)
           HW INTR EN REG  FFFFDCF0
                           00000001
                                           CRD ERROR INT. ENABLE
                                           HARDWARE INT. ENABLED ON PIN 3
           Error Log Report Generator                                    Version 7.3

                                           HARDWARE INT. ENABLED ON PIN 4
                                           HARDWARE INT. ENABLED ON PIN 5
                                           PC1 INT. DISABLED
                                           PC0 INT. DISABLED
                                           HARDWARE INT. ENABLED ON PIN 0
                                           HARDWARE INT. ENABLED ON PIN 1
                                           HARDWARE INT. ENABLED ON PIN 2
                                           SLU INT. DISABLE
                                           SOFTWARE INT. LEVEL 1 ENABLED
                                           SOFTWARE INT. LEVEL 2 ENABLED
                                           SOFTWARE INT. LEVEL 3 ENABLED
                                           SOFTWARE INT. LEVEL 4 ENABLED
                                           SOFTWARE INT. LEVEL 5 ENABLED
                                           SOFTWARE INT. LEVEL 6 ENABLED
                                           SOFTWARE INT. LEVEL 7 ENABLED
                                           SOFTWARE INT. LEVEL 8 ENABLED
                                           SOFTWARE INT. LEVEL 9 ENABLED
                                           SOFTWARE INT. LEVEL 10 ENABLED
                                           SOFTWARE INT. LEVEL 11 ENABLED
                                           SOFTWARE INT. LEVEL 12 ENABLED
                                           SOFTWARE INT. LEVEL 13 ENABLED
                                           SOFTWARE INT. LEVEL 14 ENABLED
                                           SOFTWARE INT. LEVEL 15 ENABLED
                                           KERNAL MODE AST INT. ENABLED
                                           EXEC. MODE AST INT. ENABLED
                                           SUPER. MODE AST INT. ENABLED
                                           USER MODE AST INT. ENABLED
           HW INTR REQ REG 00000702
                           00000000
                                           HW INTR. REQ
                                           PC1 INTR REQ.
                                           PC0 INTR REQ.
                                           CPU INTR REQ. on pin 0
           MEM MGMT ER/DTB 00005110
                           00000000
                                           Integer Reg. used is R = 11(X)
                                           OP code = 28(X)
           D-CACHE STA REG 000002E0
                           00000000
           D-CACHE ADD REG FFFFFFFF
                           00000007
           ABOX CTL REG    0000040E
                           00000000
                                           MCHECK ENABLED for UNCOR. ERR
                                           CRD INTR. ENABLE
                                           ICACHE STREAM BUFFER ENABLED
                                           DCACHE ENABLED
           BIU STATUS REG  00002041
                           00000000
                                           Hard Error
                                           Dcache fill error
                                           READ_BLOCK
           BIU ADD REG     40000000
                           00000002
           BIU CTL REG     30006337
                           0000000C

           Error Log Report Generator                                    Version 7.3

                                           External Cache Enable
                                           ECC Checking
                                           Output Enable of Cache RAMs
                                           BCache Read Speed in cycles = 4(X)
                                           BCache Write Speed in cycles = 4(X)
           ECC SYNDROMES   00000000
                           00000000
           FILL ADDR REG   00006120
                           00000000
           MACHINE CHK VA  00006190
                           00000000
           B-CACHE TAG REG 12491412
                           14480005
                                           TAG Control P
                                           TAG Control V
                                           B-Cache TAG  = 48A0(X)
           CSR0            400001C1
                           400001C1
           BCC             400001C1
           CSR1            00000000
           BCCE            00000000
           CSR2            00000000
           BCCEA           00000000
           CSR3            00000900
           BCUE            00000900
           CSR4            00D40A2D
           BCUEA           00D40A2D
           CSR5            0011D4B4
           DTER            0011D4B4
           CSR6            00007F28
           CBCTL           00007F28
                           98004082
           CSR7            98004082
           CBE             9C001042
           CSR8            90000003
           CBEAL           90000003
           CSR9            FF200083
           CBEAH           FF200083
           CSR10           00000000
           PMBX            00000000
           CSR11           00000000
           IPIR            00000000
           CSR12           00000004
           SIC             00000001
           CSR13           000C1388
           ADLK            000C1388
           CSR14           00104B7B
           MADRL           00104B6B

           Error Log Report Generator                                    Version 7.3

    **************************** ENTRY       6. ****************************
    ERROR SEQUENCE 3.                                 LOGGED ON SID 03003700

    MACHINE CHECK,  6-MAR-2000 10:11:34.70
                    KA730 REV# 0. MIC# 55.

          EXCEPTION PC    80038DC0

          ERROR PSL       01C00000
                                          INTERRUPT PRIORITY LEVEL = 00.
                                          PREVIOUS MODE = USER
                                          CURRENT MODE  = EXECUTIVE

          SUMMARY CODE    00000007
                                          UNCORRECTABLE ECC ERROR
          1ST PARAMETER   00166200
                                          PAGE #2865. IN ERROR
    **************************** ENTRY      60. ****************************
    ERROR SEQUENCE 4872.                              LOGGED ON SID 02006148

    MACHINE CHECK, 6-MAR-2000 03:50:08.28
                   KA750 REV# 72. MIC# 97.

          EXCEPTION PC    80006173

          ERROR PSL       00C80009
                                          C-BIT
                                          N-BIT
                                          INTERRUPT PRIORITY LEVEL = 08.
                                          PREVIOUS MODE = USER
                                          CURRENT MODE  = KERNEL
          SUMMARY CODE    00000002
                                          TRANSLATION BUFFER OR BUS ERROR
          VA LAST REF     800A079E
          PC AT ERROR     80006178
          MDR             8009F38C
          SMR             00000008
                                          CPU MODE = KERNEL
                                          VIRTUAL
                                          READ
          RLTO            00000000
          TBER            00000007
                                          TB G0 DATA ERROR
                                          TB G1 DATA ERROR
                                          TB G0 TAG ERROR
          CAER            00000000
          BER             00000000
          MCESR           00000004
                                          OPERAND REFERENCE
                                          TB PARITY ERROR
    **************************** ENTRY      84. ****************************
    ERROR SEQUENCE 4949.                              LOGGED ON SID 01388525

    MACHINE CHECK,  6-MAR-2000 15:09:11.31
                    KA780 REV# 7. SERIAL# 1317.

          EXCEPTION PC    00004890

          ERROR PSL       03C00000
                                          INTERRUPT PRIORITY LEVEL = 00.
                                          PREVIOUS MODE = USER
                                          CURRENT MODE  = USER

          SUMMARY CODE    00000000
                                          CP READ TIMEOUT
                                          - OR ERROR CONFIRMATION FAULT
          CES             00010084
                                          SUPERVISOR AST PENDING
                                          ALU C31
                                          NESTED ERROR
          MICRO PC        00000200
          VA/VIBA         7FF735D4
          D REGISTER      FFFFC284
          TBER0           0000DC81
                                          ENABLE MEMORY MANAGEMENT
                                          TB HIT GROUP 1
                                          MICRO CODE "MCT" FIELD = 07
                                          MICRO CODE "ADS"
                                          MICRO CODE "FS"
          TBER1           00000040
                                          LAST TB WRITE PULSE TO GROUP 1
          SBITA           E00B83F5
                                          TIMEOUT CONSOLE ADDR = 002E0FD4
                                          PROTECTION CHECKED REFERENCE
                                          TIMEOUT REFERENCE IN USER MODE
          CACHE PE REG    00004000
                                          CP ERROR
          SBIER           00001802
                                          SBI NOT BUSY
                                          WAITING FOR READ DATA TIMEOUT
                                          CPU TIMEOUT

     **************************** ENTRY      82. ****************************
     ERROR SEQUENCE 1077.                              LOGGED ON SID 04FFFFFF
     MACHINE CHECK  30-MAR-2000 20:55:17.41
                    KA86  REV# 255.  SERIAL# 4095.  MFG PLANT 7.
           EHMSTS          40000802
                                           VMS ERROR CODE = EBOX
                                           MICRO TRAP VECTOR = 08 (X)
                                           EHM ENTERED
           EVMQSAV         00000004
                                           VIRTUAL ADDRESS FOR EBOX PORT
                                           _ REQUESTS
           EBCS            00000800
                                           ECS PARITY ERROR
           EDPSR           00000000
           CSLINT          04183D1F
                                           C BUS ADDRESS = 1F (X)
                                           C BUS DATA = 3D (X)
                                           INTERRUPT PRIORITY REQUEST = 8.
                                           INTERNAL SOURCE
                                           I/O ADAPTER = 0.
                                           INTERVAL TIMER
           IBESR           00004000
                                           UOP SEL = IBOX REGISTER SELECT
                                           UTPR <2:0> = EBOX PORT
                                           ENABLE ETRAP
           EBXWD1          00000004
                                           TOP OF "SP STACK"
                                           _ CONTENT IS ONE OF THE LAST
                                           _ LONGWORDS WRITTEN TO MBOX
           EBXWD2          7FF593D0
                                           TOP OF "SP STACK" MINUS ONE
                                           _ CONTENT IS ONE OF THE LAST
                                           _ LONGWORDS WRITTEN TO MBOX
           VASAV           7FF593F8
                                           VIRTUAL ADDRESS FOR OP FETCH
                                           _ PORT REQUEST ADDRESS
                                           _ CALCULATION FOR OPERAND
                                           _ PRE-FETCH AND RESULT DELIVERY
           VIBASAV         0000E7FF
                                           VIRTUAL ADDRESS OF NEXT IBUF
                                           _ PORT REQUEST TO FILL IBUFFER
           ESASAV          0000E7F2
                                           PC OF INSTRUCTION DURING EBOX
                                           _ EXECUTION AND RESULT STORAGE
           ISASAV          0000E7F2
                                           PC OF INSTRUCTION WHICH VA
                                           _ CALCULATION UNIT IS DOING ADDRESS
                                           _ CALCULATION OR OPERAND PRE-FETCH
                                           _ OR IS PASSING OPERAND DATA
           CPC             0000E7F4
                                           PC OF INSTRUCTION IN
                                           _ DECODE UNIT
           MSTAT1          84006004
                                           C0 TAG MISS
                                           BLOCK HIT
                                           ABUS ADAPTER = 0.
                                           WORD COUNT = 0.
                                           CYCLE TYPE = READ REGISTER
                                           DEST CP = EBOX
           MSTAT2          00004F00
                                           DIAGNOSTIC STATUS FROM SBIA
                                           _    RD COM/MSK <3:0> = F (X)
                                           _    RD DAT L/S <1:0> = 0 (X)
                                           _    ABUS BAD DATA CODE
                                           PAMM DATA = ARRAY #0.,SLOT #1.
           MDECC           00066200
                                           (* DATA NOT VALID *)
           MERG            04000100
                                           MEMORY MANAGEMENT ENABLE
           CSHCTL          00000003
                                           CACHE 0 ENABLE
                                           CACHE 1 ENABLE
           MEAR            0000007C
                                           PHYSICAL ADDRESS IN PA LATCH
                                           AT TIME OF ERROR = 0000007C
           MEDR            0000001F
                                           DATA WORD USED DURING ERROR
           FBXERR          FFFFFFFF
                                           (* DATA NOT VALID *)
           CSES            1BD73E01
                                           CS CODE = EBOX CONTROL STORE PARITY ERROR
                                           CS SYNDROME = 3E (X)
                                           CS ADDRESS = 1BD7 (X)
           ERROR PC        0000E7F2

           ERROR PSL       03C00004
                                           Z-BIT
                                           INTERRUPT PRIORITY LEVEL = 00.
                                           PREVIOUS MODE = USER
                                           CURRENT MODE  = USER
           IOA ES          00000000
                                           (* DATA NOT VALID *)

    AN/ER/INC=MACH ERR:ERRLOG.SYS_31MAR2000/ENT=S=82/OUT=DP.

メモリ・エラー・エントリ例

メモリ・エラー・ログ・エントリには，回復不可能エラーと回復可能エラーの 2 種類があります。回復可能メモリ・エラーは，メモリ記憶位置内の不正ビットが 1 つだけであり，ECC (エラー訂正コード) がこのエラーを補正しデータを修正できたエラーです。回復不可能エラーは，不正ビットが複数あり， ECC がデータを修正できなかったエラーです。

回復不可能メモリ・エントリと回復可能メモリ・エントリの形式は同じです。メモリ・エラー・ログ・レポートは，2 つの部分の論理情報に分割できます。第 1 の部分は，識別情報です。第 2 の部分は，メモリ・コントローラ固有情報です。このデータは，メモリ・エラー発生時にメモリ・コントローラ・レジスタに格納されていた情報です。レジスタの内容はビットからテキストに変換され，レポートの右側に表示されます。

    **************************** ENTRY       7. ****************************
    ERROR SEQUENCE 4.                                 LOGGED ON SID 03003700

    MEMORY ERROR,  6-MAR-2000 10:11:34.70
                   KA730 REV# 0. MIC# 55.

          CSR0            00166200
                                          ERROR SYNDROME = 7F
                                          CORRECTED ERROR, BIT #31.
                                          ARRAY #1. IN ERROR
          CSR1            18000000
                                          MEMORY MAPPING ENABLE
                                          ENABLE "CRD" REPORTING
          CSR2            8100000F
                                          MEMORY SIZE = 2048.K
                                          64K RAMS PRESENT

    **************************** ENTRY      91. ****************************
    ERROR SEQUENCE 342.                               LOGGED ON SID 0138207A

    FATAL MEMORY ERROR, 4-MAR-00 08:16:45.20
                        KA780 REV# 7. SERIAL# 122.

    CONTROLLER AT TR #5.

          PRTCFNG         00000040
                                          ADAPTER IS MULTI-PORT MEMORY
                                          PORT NUMBER = 0.
          PRTCR           00000003
                                          MASTER INTERRUPT ENABLE
                                          PORT INTERFACE INTERRUPT ENABLE
                                          RAM COUNT 0.
          PCSR            07870003
                                          ERROR INTERRUPT ENABLE
          IVDTCR          01870001
                                          INVALIDATE CACHE DEVICE ID = 0.
                                          8. ARRAY BOARD(S) PRESENT
                                          MEMORY BASE ADDRESS = 6144.K
          AER             16A70005
                                          ERROR SYNDROME = 05
                                          RDS ERROR
                                          ARRAY #6. IN ERROR
                                          ARRAY BANK #1. IN ERROR
                                          ERROR LOG REQUEST
          CSR0            0000C2C8
                                          MEMORY CONTAINS VALID DATA
                                          PORT #2. POWERED DOWN
                                          PORT #3. POWERED DOWN
                                          ERROR INTERRUPT FROM PORT #1.
                                          PORT #2. OFFLINE
                                          PORT #3. OFFLINE
          CSR1            0000380A
                                          PORT #0. CONNECTED TO AN SBI
                                          PORT #1. CONNECTED TO AN SBI
                                          PORT #2. NOT PRESENT
                                          PORT #3. NOT PRESENT
                                          INVALIDATION MAP PRESENT
                                          PORT #0. INVALIDATION ACK RECEIVED
                                          PORT #1. INVALIDATION ACK RECEIVED
          MAT             0000C000

前へ | 次へ | 目次 | 索引