| ### Counters clock settings Specifies the number of times the node clock has been set nonmonotonically (abruptly). creation time Specifies the time at which the DTS entity was created and the counters were initialized. different epochs detected Specifies the number of times the node received time response messages from servers or clerks that had epoch numbers different from its own. This counter is shown only for servers. disable directives completed Specifies the number of times the DTS has been disabled. enable directives completed Specifies the number of times the DTS has been enabled. epoch changes completed Specifies the number of times the server's epoch has changed. insufficient resources detected Specifies the number of times the node has been unable to allocate virtual memory. local servers not in group Specifies the number of times that a local server was contacted, but it was not in the dts security group. local times not intersecting Specifies the number of times the node's time interval failed to intersect the computed interval of the servers. no global servers detected Specifies the number of times the courier server could not contact any global servers. This counter is shown only for servers. protocol mismatches detected Specifies the number of times the local node failed to process a received message containing an incompatible protocol version. servers not in group Specifies the number of times that a non-local server was contacted, but it was not in the dts security group. This counter is shown only for servers. servers not responding Specifies the number of times the courier server could not contact a specific global server. This counter is shown only for servers. servers times not intersecting Specifies the number of times a server has detected faulty servers (other than itself). This counter is shown only for servers. synchronizations completed Specifies the number of times the node successfully synchronized. system errors detected Specifies the number of times a DTS operation detected a system error. time provider failures detected Specifies the number of times the external time provider signaled a failure or the node was unable to access the time provider. time provider timeouts detected Specifies the number of times a dtsd server process initiated contact with a time provider and did not receive the initial response within the interval specified by local set timeout (the default interval is 5 seconds). This counter is shown only for servers. time representation version mismatches detected Specifies the number of times the local node failed to process a received message containing an incompatible timestamp format. too few servers detected Specifies the number of times a node failed to synchronize because it could not contact the required minimum number of servers. updates initiated Specifies the number of times a server has attempted to update its clock. This counter is shown only for servers. ###