| ## rpc_server_inq_if(3rpc) Returns the manager entry point vector registered for an interface Used by server applications. Synopsis #include <dce/rpc.h> void rpc_server_inq_if( rpc_if_handle_t if_handle, uuid_t *mgr_type_uuid, rpc_mgr_epv_t *mgr_epv, unsigned32 *status); Parameters Input if_handle Specifies the interface specification whose manager Entry Point Vector (EPV) pointer is returned in the mgr_epv parameter. mgr_type_uuid Specifies a type UUID for the manager whose EPV pointer is returned in the mgr_epv parameter. Specifying the value NULL (or a nil UUID) has this routine return a pointer to the manager EPV that is registered with if_handle and the nil type UUID of the manager. Output mgr_epv Returns a pointer to the manager EPV corresponding to if_handle and mgr_type_uuid. status Returns the status code from this routine. This status code indicates whether the routine completed successfully or, if not, why not. Description A server application calls the rpc_server_inq_if( ) routine to determine the manager EPV for a registered interface and type UUID of the manager. Return Values No value is returned. Errors The following describes a partial list of errors that might be returned. Refer to the OSF DCE Problem Determination Guide for complete descriptions of all error messages. rpc_s_ok Success. rpc_s_unknown_if Unknown interface. rpc_s_unknown_mgr_type Unknown manager type. Related Information Functions: rpc_server_register_if(3rpc) ##