# 日本語 Compaq TCP/IP Services for OpenVMS
インストレーション/ コンフィギュレーション・ガイド

前へ | 目次 | 索引

## 3.8.1 TCPIP$CONFIG コマンド・プロシージャからの IVP の実行

TCP/IP Services for OpenVMS のメインのコンフィギュレーション・メニューで，オプション 7 (Run tests) を選択します。次の例のように「Test」メニューが表示されます。

    Compaq TCP/IP Services for OpenVMS TEST Menu

            Test options:

                     1  -  Internet IVP
                     2  -  SNMP IVP

                     A  -  Tests 1 - 2
                    [E] -  Exit menu

    Enter test option:

実行したいテストに適したオプションを選択します。

## 3.8.2 OpenVMS DCL プロンプトからの IVP の実行

コンフィギュレーション・プロシージャの終了後に， DCL プロンプトから IVP を実行するには，次のコマンドを入力します。このプロシージャでは，TCPIP$CONFIG 「Test」メニューのオプション1 (Internet IVP) と同じテストが実行されます。

    $ @SYS$TEST:TCPIP$IVP

## 3.8.3 TCP/IP Services インターネット・コンフィギュレーションの検証

TCPIP$CONFIG 「Test」メニューからオプション1またはオプションAを選択するか，またはコマンド行で TCPIP$IVP コマンド・プロシージャを実行する場合， IVP は，次の例に示すように，TCP/IP Services ソフトウェアの基本的なコンフィギュレーションをテストします。この例では，テストは正常に終了します。

    Enter test option: 1 [Return]

    %%% TCPIP IVP: started %%%

    UDP/IP test started at 5-MAR-2002 16:13:03.02
    UDP/IP test ended at 5-MAR-2002 16:13:03.69
    UDP/IP transferred successfully in 0 seconds 4198400 bytes

    TCP/IP test started at 5-MAR-2002 16:13:04.20
    TCP/IP test ended at 5-MAR-2002 16:13:41.21
    TCP/IP transferred successfully in 37 seconds 4198400 bytes

    RAW_IP test started at 5-MAR-2002 16:13:41.71
    RAW_IP test ended at 5-MAR-2002 16:13:41.79
    RAW_IP transferred successfully in 0 seconds 251000 bytes

    %%% TCPIP IVP: completed successfully %%%
    IVP request completed.
    Press Return to continue ...

IVPが正常に終了しなかった場合，プロシージャはエラー・メッセージを表示します。 IVPエラーはすべて，OpenVMSシステム・メッセージと同じ書式を使用します。次に IVPエラーの出力例を示します。

    %TCPIP-E-IDENT, explanation of error.

表 3-2 に，IVPエラー・メッセージの原因となる一般的な問題を示します。推奨される処置を行っても問題が解決しない場合には，Compaqの最寄りの支店/営業所にお問い合わせください。

表 3-2 IVPエラーのトラブルシューティング
問題 | 処置
--- | ---
ネットワーク・コンフィギュレーションに問題がある。 | TCP/IP Services をシャットダウンし，コンフィギュレーション・プロシージャを再度実行します。
起動に失敗した。 | MODPARAMS.DATファイル中のシステム・パラメータをチェックし，必要に応じて値を調整します( 第 1.2.7 項 を参照)。その後，TCP/IP Servicesをシャットダウンして再起動します。
インストレーション・キットに欠陥がある。 | キットの交換をお申し出ください。
PAKがないためにIVPが失敗した。 | 日本語 Compaq TCP/IP Services for OpenVMS PAKを登録してください。

## 3.8.4 SNMP コンフィギュレーションの検証

TCPIP$CONFIG「Test」メニューからオプション2またはオプションAのいずれかを選択すると， IVP は，次の例のように SNMP サービスをテストします。

    Begin SNMP IVP...

    The SNMP IVP requires that TCPIP/IP Services be running.
    It performs the following startups and shutdowns on the
    SNMP service only (other TCP/IP services are not affected):

    - If SNMP is running, shuts down SNMP before initial
      configuration
    - Starts SNMP and runs tests
    - Shuts down SNMP and restores initial configuration
    - Before exiting, starts SNMP

    Shutting down the SNMP service... done.

    Creating temporary read/write community SNMPIVP_6520.

    Enabling SET operations.

    Starting up the SNMP service... done.

          Saving sysContact: Ralph Nickleby
      Setting sysContact to: Julius Caesar
       Retrieved sysContact: Julius Caesar
    (Retrieved value matches SET value.)
    Restoring sysContact to: Ralph Nickleby

        Saving snmpEnableAuthenTraps: 1 (enabled)
    Setting snmpEnableAuthenTraps to: 2 (disabled)
     Retrieved snmpEnableAuthenTraps: 2 (disabled)
    (Retrieved value matches SET value.)
     Restoring snmpEnableAuthenTraps: 1 (enabled)

    Disabling SET operations.

    Deleting temporary read/write community SNMPIVP_6520.

    Shutting down and restarting the SNMP service...
    Shutting down the SNMP service... done.

    Starting up the SNMP service... done.

    SNMP IVP request completed.
    Press Return to continue ...

SNMP テストのうちのいずれかが失敗した場合には，次のようなメッセージが表示されます。

    SNMPIVP: unexpected text in response to SNMP request:
    "No reply."
    See file SYS$SYSDEVICE:[TCPIP$SNMP]TCPIP$SNMP_REQUEST.DAT for more
    details.
    Verify that SNMP trace is not enabled.
    sysContact could not be retrieved. Status = 0
    The SNMP IVP has NOT completed successfully.

この場合のエラーは，起動されていない SNMP 構成要素があるか，または SNMP トレースが有効になっていて無効にする必要があることを示している可能性があります。 SNMP トレースの詳細については，『 Compaq TCP/IP Services for OpenVMS Management 』を参照してください。

# 3.9 追加のコンフィギュレーション作業

TCPIP$CONFIGを実行して，ネットワークに必要な機能と構成要素を使用可能にした後は，製品アプリケーションへのアクセスを可能にするため，追加のコンフィギュレーション作業を終了させる必要があります。 TCP/IP Servicesには，環境に合わせてソフトウェアを変更したり，カスタマイズできる管理コマンド・インタフェースと論理名が用意されています。

追加のコンフィギュレーション作業には次のようなものがあります。

- データベースのポピュレート(たとえば，BINDやDHCP用に)

- ユーザ・アカウントの設定

- 通信およびNFSプロキシの設定

- プリント・キューの定義

- ファイル・システムの設定，エクスポート，および保守

- 最適なパフォーマンスを得るためのシステムのチューニング

サービスの多くは，追加のコンフィギュレーション作業や最適化を必要とします。各サービスのコンフィギュレーション方法についての詳細は，『 Compaq TCP/IP Services for OpenVMS Management 』を参照してください。

# 3.10 コマンドによるTCP/IP Servicesの起動と停止

第 3.10.1 項 で説明するように， OpenVMS スタートアップ・ファイルのコマンドを使用して， OpenVMS システムがスタートアップまたはシャットダウンした際に， TCP/IP Services を自動的に起動または停止することができます。これらのコマンドは，システムにインストールされているすべての TCP/IP Services 構成要素の起動または停止を行います。代わりの方法として，現在実行中の他の TCP/IP Services 構成要素に影響を与えることなく，個々の TCP/IP Services クライアントまたはサーバ構成要素の起動または停止を行うこともできます。個々の構成要素の起動または停止についての詳細は， 第 3.10.3 項 を参照してください。

必要な場合には， 第 3.10.2 項 で説明するように， TCP/IP Services の起動および停止を手動で行うことができます。また， 第 3.10.4 項 で説明するように，ユーザ作成のサービスの起動および停止を行うこともできます。

## 3.10.1 TCP/IP Services の自動起動と自動停止

TCP/IP Servicesソフトウェアをシステムの起動時に自動的に起動させ，システムのシャットダウン時に自動的に停止させるには，
SYS$COMMON:[SYSMGR]SYSTARTUP_VMS.COMファイルを編集して，次のコマンドを追加します。

    @SYS$STARTUP:TCPIP$STARTUP

システムに以前のバージョンの TCP/IP Services がインストールされていた場合には， UCX$STARTUP.COM ファイルと UCX$SHUTDOWN.COM ファイルが存在している可能性があります。これらのファイルはもう適用できないため，これらのファイルに関係する定義はすべて，SYS$MANAGER:SYSTARTUP_VMS.COM から削除してください。

OpenVMSアカウントへログインした後にTCP/IP Servicesが起動するようにしたい場合は， OpenVMSのシステム単位のログイン・プロシージャ (通常SYS$MANAGER:SYLOGIN.COM)のworldの読み取りと実行の保護 (W:RE) が設定されていなければなりません。

現在の保護を表示するには，次のコマンドを入力します。

    $ DIR/PROTECTION SYS$MANAGER:SYLOGIN.COM

保護についての情報は，OpenVMS のマニュアルを参照してください。

## 3.10.2 TCP/IP Services の手動による起動と停止

TCP/IP Services を手動で起動するには，次のコマンドを入力します。

    $ @SYS$STARTUP:TCPIP$STARTUP

TCP/IP Services を手動で停止するには，次のコマンドを入力します。

    $ @SYS$STARTUP:TCPIP$SHUTDOWN

## 3.10.3 個々のサービスの起動と停止

TCP/IP Services をすでに実行しているシステムでは，システムで実行中の他の TCP/IP Services 構成要素に影響を及ぼすこともなく，また TCP/IP Services を再起動する必要もなく，個々のサーバまたはクライアント構成要素のコンフィギュレーションを行うことができます。

ほとんどのサービスは，単独でシャットダウンしたり起動したりすることができます。これは，パラメータや論理名を変更する際にサービスを再起動する必要のある場合に便利です。

次のファイルが提供されています。

- SYS$STARTUP:TCPIP$service_STARTUP.COM を使用すると， service サービスを起動することができます。

- SYS$STARTUP:TCPIP$service_SHUTDOWN.COM を使用すると， service サービスをシャットダウンすることができます。

サイト固有のパラメータ設定およびコマンドを保持するには，次のファイルを作成します。これらのファイルは， TCP/IP Services を再インストールしても上書きされません。

- SYS$STARTUP:TCPIP$service_SYSTARTUP.COM は， service を起動する際に呼び出されるサイト固有の定義およびパラメータのリポジトリとして使用することができます。

- SYS$STARTUP:TCPIP$service_SYSHUTDOWN.COM は， service をシャットダウンする際に呼び出されるサイト固有の定義およびパラメータのリポジトリとして使用することができます。

これらのファイル名で，service は，起動またはシャットダウンするサービスの名前です。たとえば，NTP サービスをシャットダウンするには TCPIP$NTP_SHUTDOWN を使用します。

詳細については，『 Compaq TCP/IP Services for OpenVMS Management 』を参照してください。

## 3.10.4 ユーザ作成サービスの起動と停止

TCP/IP Services では，ユーザ作成サービスの起動および停止を行うためのコマンド・プロシージャを提供しています。ユーザ作成サービスを起動するには，次のコマンドを入力します。

    $ SYS$STARTUP:TCPIP$CUSTOMER_SERVICE_STARTUP service-name

service-nameには，TCP/IP 管理コマンドの SET SERVICE を使用して定義したサービスの名前を指定します。

ユーザ作成サービスを停止するには，次のコマンドを入力します。

    $ SYS$STARTUP:TCPIP$CUSTOMER_SERVICE_SHUTDOWN service-name

# 3.11 TCP/IP ServicesをDECwindowsアプリケーションのトランスポートに指定

TCP/IP ServicesをDECwinsowsアプリケーションのトランスポート・インタフェースとして使用可能にするには，次の行を SYS$MANAGER:DECW$PRIVATE_SERVER_SETUP.COMコマンド・プロシージャに追加します。

    $ DECW$SERVER_TRANSPORTS == "DECNET,LOCAL,TCPIP"

続いて，次のコマンドを入力してDECwindowsを再起動します。

    $ @SYS$STARTUP:DECW$STARTUP RESTART

システムで，DECnetまたはDECnet-Plusソフトウェアを使用している場合には，これも起動します。

DECwindowsクライアント(リモート・ホスト)で実行されている DECwindowsアプリケーションをDECwindowsサーバ(あなたが使用しているワークステーション)に表示するには，次の手順に従います。

1. リモート・ホストのセキュリティを設定します。

2. ローカル・ホスト・データベースにリモート・クライアントを追加します。

3. 次の行をSYS$MANAGER:DECW$PRIVATE_SERVER_SETUP.COMに追加します。

       $ DECW$SERVER_TRANSPORTS == "DECNET,LOCAL,TCPIP"

4. アプリケーションの表示をリモート・ホストに設定します。

       $ SET DISPLAY/CREATE/NODE=remote-host/TRANSPORT=TCPIP

# 付録 A
TCP/IP Services の新規のインストレーションとコンフィギュレーションの例

この付録では，TCP/IP Services 製品を一度もインストールしたことがないシステムでの，TCP/IP Services のインストレーションとコンフィギュレーションの例を示します。

# A.1 新規のインストレーション・プロシージャの例

次の例は， TCP/IP Services のインストレーションでの対話のサンプルを示しています。この例では，インストレーションは，製品がまだインストールされていないシステムで行われています。 TCP/IP Services が以前にインストールされていたシスムでは，インストレーションでの対話がわずかに異なります ( 第 2 章 を参照)。

注意 次の例中の xx は，製品の 2 桁のアップデート・バージョン番号を示します。

    Choose one or more items from the menu separated by commas: 1

    The following product has been selected:
        DEC VAXVMS TCPIPJA V5.3-xx               Layered Product

    Do you want to continue? [YES] [Return]

    Configuration phase starting ...

    You will be asked to choose options, if any, for each selected product and for
    any products that may be installed to satisfy software dependency requirements.

    DEC VAXVMS TCPIPJA V5.3-xx: Compaq TCP/IP Services/Japanese for OpenVMS.

        Copyright 2002 Compaq Information Technologies Group, L.P

        Compaq Computer Corporation

        Compaq TCP/IP Services/Japanese for OpenVMS offers several license options.

    Do you want the defaults for all options? [YES] [Return]

    Do you want to review the options? [NO] [Return]

    Execution phase starting ...

    The following product will be installed to destination:
        DEC VAXVMS TCPIPJA V5.3-xx               DISK$OVMSVAXSYS:[VMS$COMMON.]

    Portion done: 0%...10%...20%...30%...40%...50%...60%...70%...80%...90%
    %PCSI-I-PRCOUTPUT, output from subprocess follows ...
    % TCPIP-W-PCSI_INSTALL
    % - Execute SYS$MANAGER:TCPIP$CONFIG.COM to proceed with configuration of
    %   Compaq TCP/IP Services.
    %

    Portion done: 100%

    The following product has been installed:
        DEC VAXVMS TCPIPJA V5.3-xx               Layered Product

    DEC VAXVMS TCPIPJA V5.3-xx: Compaq TCP/IP Services/Japanese for OpenVMS.

        Check the release notes for current status of the product.

# A.2 新規のコンフィギュレーション・プロシージャ

次の例は， TCP/IP Services のコンフィギュレーションでの対話のサンプルを示しています。この例では，次の構成要素のコンフィギュレーションが行われます。

- コア環境

- TELNET クライアント

- FTP サーバ

この例では，コンフィギュレーションは，製品のコンフィギュレーションがまだ行われたことがないシステムで行われます。システムで以前に TCP/IP Services のコンフィギュレーションが行われたことがある場合，対話はわずかに異なります ( 第 3 章 を参照)。

      TCP/IP Network Configuration Procedure

    This procedure helps you define the parameters required
    to run Compaq TCP/IP Services for OpenVMS on this system.

    Checking TCP/IP Services for OpenVMS configuration database files.

    Creating SYS$COMMON:[SYSEXE]TCPIP$SERVICE.DAT
    Creating SYS$COMMON:[SYSEXE]TCPIP$HOST.DAT
    Creating SYS$COMMON:[SYSEXE]TCPIP$NETWORK.DAT
    Creating SYS$COMMON:[SYSEXE]TCPIP$ROUTE.DAT
    Creating SYS$COMMON:[SYSEXE]TCPIP$PROXY.DAT
    Creating SYS$COMMON:[SYSEXE]TCPIP$CONFIGURATION.DAT
    Creating TCPIP$ETC:SYSCONFIGTAB.DAT

    Compaq TCP/IP Services for OpenVMS requires a definition for at
    least one interface.  There are no interfaces defined on this
    system.

    Please select the Interface option from the Core Environment Menu.

      Compaq TCP/IP Services for OpenVMS Configuration Menu

      Configuration options:

           1  -  Core environment
           2  -  Client components
           3  -  Server components
           4  -  Optional components

           5  -  Shutdown Compaq TCP/IP Services for OpenVMS
           6  -  Startup Compaq TCP/IP Services for OpenVMS
           7  -  Run tests

           A  -  Configure options 1 - 4
          [E] -  Exit configuration procedure

    Enter configuration option: 1 [Return]

      Compaq TCP/IP Services for OpenVMS Core Environment Configuration Menu

      Configuration options:

           1  -  Domain
           2  -  Interfaces
           3  -  Routing
           4  -  BIND Resolver
           5  -  Time Zone

           A  -  Configure options 1 - 5
          [E] -  Exit menu

    Enter configuration option: A [Return]

    DOMAIN Configuration

    Enter Internet domain: budget.acme.com

    INTERFACE Configuration

      The Ethernet device(s) on your system are: EWA0:  * Not Configured *

      Start of configuration questions for Internet interface WE0.

      WE0 is the Ethernet device ESA0:

      WE0 has not been configured

      Compaq TCP/IP Services for OpenVMS Interface WE0 Configuration Menu

        Configuration options:

             1  -  Configure interface manually
             2  -  Let DHCP configure interface

            [E] -  Exit menu (Do not configure interface WE0)

    Enter configuration option: 1 [Return]
    Enter fully qualified host name: HEARTS.BUDGET.ACME.COM [Return]
    Enter Internet address for hearts: 10.0.2.4 [Return]
    Enter Internet network mask for hearts [255.0.1.0]: 255.1.12.1[Return]
    Enter broadcast mask for hearts [10.0.2.255]: [Return]

        The following parameters will be used to define the
        Internet interface WE0:

          Host name:         hearts.budget.acme.com
          Internet address:  10.0.2.4
          Network mask:      255.0.0.0
          Broadcast mask:    10.0.2.255

     * Is the above correct [YES]: [Return]

        End of configuration questions for Internet interface WE0

    DYNAMIC ROUTING Configuration

         Dynamic routing has not been configured.

         You may configure dynamic ROUTED or GATED routing.
         You cannot enable both at the same time.  If you want
         to change from one to the other, you must disable the
         current routing first, then enable the desired routing.

         If you enable dynamic ROUTED routing, this host will use the
         Routing Information Protocol (RIP) - Version 1 to listen
         for all dynamic routing information coming from other
         hosts to update its internal routing tables.
         It will also supply its own Internet addresses to
         routing requests made from remote hosts.

         If you enable dynamic GATED routing, you will be able to
         configure this host to use any combination of the following
         routing protocols to exchange dynamic routing information
         with other hosts on the network:
            Routing Information Protocol (RIP) - Version 1 & 2
            Router Discovery Protocol (RDISC)
            Open Shortest Path First (OSPF)
            Exterior Gateway Protocol (EGP)
            Border Gateway Protocol (BGP-4)
            Static routes

    * Do you want to configure dynamic ROUTED or GATED routing [NO]:[Return]

            A default route has not been configured.
    * Do you want to configure a default route [YES]: [Return]
    Enter your Default Gateway host name or address: GATE1.BUDGET.ACME.COM

          gate1.budget.acme.com is not in the local host database.

    Enter Internet address for gate1.budget.acme.com: 10.0.2.66

    BIND RESOLVER Configuration

     A BIND resolver has not been configured.

     Compaq TCP/IP Services for OpenVMS supports the Berkeley Internet Name
     Domain (BIND) resolver.  BIND is a network service that enables clients
     to name resources or objects and share information with other objects
     on the network.

     Before configuring your system as a BIND resolver, you should
     first be sure that there is at least one system on the network
     configured as either a BIND primary or secondary server for
     this domain.

     You can specify a BIND server by its address or name;
     however, if specified by name, an entry for it must
     exist in the TCPIP$HOST database.

     You will be asked one question for each server.
     Press Return at the prompt to terminate the list.

    Enter your BIND server name: NUMB9.BUDGET.ACME.COM [Return]

       numb9.budget.acme.com is not in the local host database.

    Enter Internet address for numb9.budget.acme.com: 10.0.2.11
    Enter your BIND server name: [Return]

     Creating file TCPIP$ETC:IPNODES.DAT
     Creating file TCPIP$ETC:SERVICES.DAT

       TCPIP uses timezone information provided by the OpenVMS Operating
       System. No additonal timezone configuration is needed for TCPIP
       when the operating system is configured correctly.

       This section verifies the current OpenVMS timezone configuration.
       A warning message (TCPIP-W-) indicates that corrective action should
       be taken. TCPIP will appear to operate but components may display
       either the wrong time or a time inconsistent with other applications.

    %TCPIP-I-INFO, Logical name SYS$TIMEZONE_RULE found.
    -TCPIP-I-INFO, Software for automatic Summer/Winter time (TDF) change
    -TCPIP-I-INFO, is present.
    -TCPIP-I-INFO, Further action to ensure TDF change is not necessary.

    %TCPIP-I-NORMAL, timezone information verified

    Press Return to continue ... [Return]

      Compaq TCP/IP Services for OpenVMS Core Environment Configuration Menu

      Configuration options:

           1  -  Domain
           2  -  Interfaces
           3  -  Routing
           4  -  BIND Resolver
           5  -  Time Zone

           A  -  Configure options 1 - 5
          [E] -  Exit menu

    Enter configuration option: [Return]

        Compaq TCP/IP Services for OpenVMS Configuration Menu

        Configuration options:

             1  -  Core environment
             2  -  Client components
             3  -  Server components
             4  -  Optional components

             5  -  Shutdown Compaq TCP/IP Services for OpenVMS
             6  -  Startup Compaq TCP/IP Services for OpenVMS
             7  -  Run tests

             A  -  Configure options 1 - 4
            [E] -  Exit configuration procedure

    Enter configuration option: 2 [Return]

        Compaq TCP/IP Services for OpenVMS Client Components Configuration Menu

        Configuration options:

             1  -  FTP              Disabled Stopped
             2  -  NFS Client       Disabled Stopped
             3  -  REXEC and RSH    Disabled Stopped
             4  -  RLOGIN           Disabled Stopped
             5  -  SMTP             Disabled Stopped
             6  -  TELNET           Disabled Stopped
             7  -  DHCP             Disabled Stopped
             8  -  Telnetsym        Disabled Stopped

             A  -  Configure options 1 - 8
            [E] -  Exit menu

    Enter configuration option: 6 [Return]

    TELNET Configuration

    Service is not defined in the TCPIP$SERVICE database.
    Service is not enabled.
    Service is stopped.

        TELNET configuration options:

             1 - Enable service on this node

            [E] - Exit TELNET configuration

    Enter configuration option: 1 [Return]
    Creating TELNET Service Entry

        Compaq TCP/IP Services for OpenVMS Client Components Configuration Menu

        Configuration options:

             1  -  FTP              Disabled Stopped
             2  -  NFS Client       Disabled Stopped
             3  -  REXEC and RSH    Disabled Stopped
             4  -  RLOGIN           Disabled Stopped
             5  -  SMTP             Disabled Stopped
             6  -  TELNET           Enabled  Stopped
             7  -  DHCP             Disabled Stopped
             8  -  Telnetsym        Disabled Stopped

             A  -  Configure options 1 - 8
            [E] -  Exit menu

    Enter configuration option: [Return]

        Compaq TCP/IP Services for OpenVMS Configuration Menu

        Configuration options:

             1  -  Core environment
             2  -  Client components
             3  -  Server components
             4  -  Optional components

             5  -  Shutdown Compaq TCP/IP Services for OpenVMS
             6  -  Startup Compaq TCP/IP Services for OpenVMS
             7  -  Run tests

             A  -  Configure options 1 - 4
            [E] -  Exit configuration procedure

    Enter configuration option: 3 [Return]

    Compaq TCP/IP Services for OpenVMS Server Components Configuration Menu

      1 - BIND         Enabled  Started    12 - NTP         Enabled  Started
      2 - BOOTP        Disabled Stopped    13 - PC-NFS      Enabled  Started
      3 - DHCP         Enabled  Started    14 - POP         Enabled  Started
      4 - FINGER       Enabled  Started    15 - PORTMAPPER  Enabled  Started
      5 - FTP          Enabled  Started    16 - RLOGIN      Enabled  Started
      6 - IMAP         Disabled Stopped    17 - RMT         Disabled Stopped
      7 - LBROKER      Disabled Stopped    18 - SNMP        Enabled  Stopped
      8 - LPR/LPD      Disabled Stopped    19 - TELNET      Enabled  Started
      9 - METRIC       Enabled  Started    20 - TFTP        Enabled  Started
     10 - NFS          Enabled  Started    21 - XDM         Enabled  Started
     11 - LOCKD/STATD  Disabled Stopped

      A  -  Configure options 1 - 21
     [E] -  Exit menu

    Enter configuration option: 5 [Return]

    FTP Configuration

    Service is defined in the SYSUAF.
    Service is not defined in the TCPIP$SERVICE database.
    Service is not enabled.
    Service is stopped.

        FTP configuration options:

             1 - Enable service on this node

            [E] - Exit FTP configuration

    Enter configuration option: 1 [Return]
    Creating FTP Service Entry

    The FTP CLIENT is enabled.

    * Do you want to configure FTP CLIENT [NO]: [Return]

    Compaq TCP/IP Services for OpenVMS Server Components Configuration Menu

      1 - BIND         Enabled  Started    12 - NTP         Enabled  Started
      2 - BOOTP        Disabled Stopped    13 - PC-NFS      Enabled  Started
      3 - DHCP         Enabled  Started    14 - POP         Enabled  Started
      4 - FINGER       Enabled  Started    15 - PORTMAPPER  Enabled  Started
      5 - FTP          Enabled  Started    16 - RLOGIN      Enabled  Started
      6 - IMAP         Disabled Stopped    17 - RMT         Disabled Stopped
      7 - LBROKER      Disabled Stopped    18 - SNMP        Enabled  Stopped
      8 - LPR/LPD      Disabled Stopped    19 - TELNET      Enabled  Started
      9 - METRIC       Enabled  Started    20 - TFTP        Enabled  Started
     10 - NFS          Enabled  Started    21 - XDM         Enabled  Started
     11 - LOCKD/STATD  Disabled Stopped

      A  -  Configure options 1 - 21
     [E] -  Exit menu

     Enter configuration option: [Return]

        Compaq TCP/IP Services for OpenVMS Configuration Menu

        Configuration options:

             1  -  Core environment
             2  -  Client components
             3  -  Server components
             4  -  Optional components

             5  -  Shutdown Compaq TCP/IP Services for OpenVMS
             6  -  Startup Compaq TCP/IP Services for OpenVMS
             7  -  Run tests

             A  -  Configure options 1 - 4
            [E] -  Exit configuration procedure

    Enter configuration option: 6 [Return]

    Begin Startup...

    %TCPIP-I-INFO, TCP/IP Services startup beginning at 5-MAR-2002 13:22:27
    .82
    %TCPIP-I-INFO, creating UCX compatibility file SYS$COMMON:[SYSEXE]UCX$S
    ERVICE.DAT
    %TCPIP-I-NORMAL, timezone information verified
    %RUN-S-PROC_ID, identification of created process is 00000058
    %TCPIP-I-SETLOCAL, setting domain and/or local host
    %TCPIP-I-STARTCOMM, starting communication
    %TCPIP-I-SETPROTP, setting protocol parameters
    %TCPIP-I-DEFINTE, defining interfaces
    %TCPIP-I-STARTNAME, starting name service
    %TCPIP-S-STARTDONE, TCP/IP Kernel startup completed
    %TCPIP-I-PROXYLOADED, loaded 0 NFS proxy records
    %TCPIP-I-LOADSERV, loading TCPIP server proxy information
    %TCPIP-I-SERVLOADED, auxiliary server loaded with 0 proxy records
    -TCPIP-I-SERVSKIP, skipped 0 communication proxy records
    -TCPIP-I-SERVTOTAL, total of 0 proxy records read
    %TCPIP-S-STARTDONE, TCPIP$PROXY startup completed
    %TCPIP-S-STARTDONE, TCPIP$FTP startup completed
    %TCPIP-S-STARTDONE, TCPIP$TELNET startup completed
    %TCPIP-S-STARTDONE, TCP/IP Services startup completed at 5-MAR-2002 13:
    23:00.49

    Startup request completed.
    Press Return to continue ...

前へ | 目次 | 索引