Document revision date: 30 March 2001

## OpenVMS System Management Utilities Reference Manual

Previous | Contents | Index

M
Magnetic tape devices
serving within a cluster
Management environment
defining
MAXBOB* system parameters
MAXBOBMEM system parameter
MAXBUF system parameter
MAXCLASSPRI system parameter
MAXPROCESSCNT system parameter
MAXQUEPRI system parameter
MAXSYSGROUP system parameter
MCR command
in SCACP
in SYSMAN #1
in SYSMAN #2
MC_SERVICES_P0 system parameter
MC_SERVICES_P1 system parameter
MC_SERVICES_P2 system parameter
MC_SERVICES_P3 system parameter
MC_SERVICES_P4 system parameter
MC_SERVICES_P5 system parameter
MC_SERVICES_P6 system parameter
MC_SERVICES_P7 system parameter
MC_SERVICES_P8 system parameter
MC_SERVICES_P9 system parameter
/MEDIA_FORMAT qualifier
in Backup utility
MEMBERS class
adding
fields belonging to
removing
Memory
multiport
MINCLASSPRI system parameter
MINPRPRI system parameter
MINWSCNT system parameter
MMG_CTLFLAGS system parameter
MODES class record
in Monitor utility
Modes of execution
for SYSMAN startup files
Modes of operation
image
physical
/MODIFIED qualifier
in Backup utility
MODIFY command
in Authorize utility
MODIFY/IDENTIFIER command
in Authorize utility
MODIFY/PROXY command
in Authorize utility
MODIFY/SYSTEM_PASSWORD command
in Authorize utility
Modifying page, swap, and dump file sizes
Modifying system parameters
recommended method
MONITOR ALL_CLASSES command
in Monitor utility
MONITOR CLUSTER command
in Monitor utility
MONITOR command
in Monitor utility
MONITOR DECNET command
in Monitor utility
MONITOR DISK command
in Monitor utility
MONITOR DLOCK command
in Monitor utility
MONITOR FCP command
in Monitor utility
MONITOR FILE_SYSTEM_CACHE command
in Monitor utility
MONITOR IO command
in Monitor utility
MONITOR LOCK command
in Monitor utility
MONITOR MODES command
in Monitor utility
MONITOR MSCP_SERVER command
in Monitor utility
MONITOR PAGE command
in Monitor utility
MONITOR PROCESSES command
in Monitor utility
MONITOR RLOCK command
in Monitor utility
MONITOR RMS command
in Monitor utility
MONITOR SCS command
in Monitor utility
MONITOR STATES command
in Monitor utility
MONITOR SYSTEM command
in Monitor utility
MONITOR TIMER command
in Monitor utility
MONITOR TRANSACTION command
in Monitor utility
Monitor utility (MONITOR)
classname qualifiers
/ALL
/CPU
/ITEM #1
/ITEM #2
/TOPBIO
/TOPCPU
/TOPDIO
/TOPFAULT
/TOPRBS
Cluster performance statistics
collection interval
command qualifiers
commands
CONVERT
EXECUTE
EXIT
HELP
INITIALIZE
MONITOR
MONITOR ALL_CLASSES
MONITOR CLUSTER
MONITOR DECNET
MONITOR DISK
MONITOR DLOCK
MONITOR FCP
MONITOR FILE_SYSTEM_CACHE
MONITOR IO
MONITOR LOCK
MONITOR MODES
MONITOR MSCP_SERVER
MONITOR PAGE
MONITOR PROCESSES
MONITOR RLOCK
MONITOR RMS
MONITOR SCS
MONITOR STATES
MONITOR SYSTEM
MONITOR TIMER
MONITOR TRANSACTION
MONITOR VBS
SET DEFAULT
SHOW DEFAULT
directing output
exiting
invoking
recording file record formats
relationship of qualifier and event
MONITOR VBS command
in Monitor utility
MONITOR VECTOR command
MONITOR_SERVER process
created on remote cluster node
log file
network startup
purpose
startup time
MOP downline load services
clearing counters
console carrier
displaying status and counters #1
displaying status and counters #2
trigger boot
MOUNT command
avoiding use of /CLUSTER with SYSMAN DO command
Mount error message
MOVE command
in Show Cluster utility
MOVE keypad function
MPDEV_D1 system parameter
MPDEV_ENABLE system parameter
MPDEV_LCRETRIES system parameter
MPDEV_POLLER system parameter
MPDEV_REMOTE system parameter
MPW_HILIMIT system parameter
MPW_IOLIMIT system parameter
MPW_LOLIMIT system parameter
MPW_LOWAITLIMIT system parameter
MPW_PRIO system parameter
MPW_THRESH system parameter
MPW_WAITLIMIT system parameter
MPW_WRTCLUSTER system parameter
MSCP_BUFFER system parameter
MSCP_CMD_TMO system parameter
MSCP_CREDITS system parameter
MSCP_LOAD system parameter
MSCP_SERVER class record
in Monitor utility
MSCP_SERVE_ALL system parameter
Multicast address
cluster
displaying
Multicast messages #1
Multicast messages #2
Multicast messages #3
timer for
Multiport memory
connecting
initializing
sharing
MULTIPROCESSING system parameter
MULTITHREAD system parameter
MVTIMEOUT system parameter

Previous | Next | Contents | Index

| privacy and legal statement |
6048PRO_INDEX_006.HTML