| #### Verifying the Ethernet Address During installation, you may receive the following prompt to verify the machine's 12-digit hexadecimal Ethernet address: The following IEEE 802 address has already been entered for this machine: 0000c0eac744 Is this correct? (y) You will receive this prompt under any of the following conditions: · If you are installing DCE for the first time · If you have used the dce_config REMOVE option to stop DCE daemons and remove any data files associated with those daemons. To answer the prompt, you have two choices: · If the displayed address is correct, press <Return>. · If the displayed address is incorrect, 1. Type n and press <Return>. The dce_config script prompts for the correct address. Enter your machine's IEEE 802 address as a 12 digit hex number (for example, 08002B0F59BB): 2. Type the correct address and press <Return>. The dce_config script continues the installation. Note: If dce_config cannot obtain the machine's Ethernet address, it prompts for the address without displaying an address to verify. ####