# BASEstartm Classic DAS
for OMNItm Software
Installation and User's Guide

Previous | Contents | Index

# 2.2 Installation Procedure

When your system meets all the hardware and software requirements, you can install the DAS for OMNI software. The installation takes from 5 to 10 minutes, depending on system load and configuration.

Install the DAS for OMNI software using the following steps:

1. Log in to a privileged system manager's account.
2. Set the default directory to SYS$UPDATE:

             $  SET DEFAULT SYS$UPDATE

3. Invoke VMSINSTAL:

       $ @SYS$UPDATE:VMSINSTAL DCM_OMNIVVA034 DDCU:

   where:
   - DCM_OMNIVVA034 argument is the kit name
   - 034 portion of the name is the version number
   - ddcu argument represents the name of the device on which the installation media is mounted, where:
     - dd is the device code
     - c is the controller designation
     - u is the unit number

VMSINSTAL prompts you for information during the installation. The following is an example of the output from the installation.

            OpenVMS VAX Software Product Installation Procedure V7.2

    It is 3-FEB-2000 at 08:20.

    Enter a question mark (?) at any time for help.

    * Are you satisfied with the backup of your system disk [YES]?

    The following products will be processed:

      DCM_OMNIVVA V3.4

            Beginning installation of DCM_OMNIVVA V3.4 at 08:21

    %VMSINSTAL-I-RESTORE, Restoring product save set A ...
    %VMSINSTAL-I-RELMOVED, Product's release notes have been moved to SYS$HELP.

       Copyright 1990 Compaq Computer Corporation

       Confidential computer software.  Valid license from Compaq or authorized
       sublicensor required for possession, use or copying.  Consistent with FAR
       12.211 and 12.212, Commercial Computer Software, Computer Software
       Documentation, and Technical Data for Commercial Items are licensed to the
       U.S. Government under vendor's standard commercial license.

       BASEstar Classic DAS for OMNI Software installation procedure.

       Checking for a valid license...

            Product:      DAS-OMNI-CL
            Producer:     DEC
            Version:      3.4
            Release Date: 13-DEC-1996

    * Does this product have an authorization key registered and loaded? y

       Now checking OpenVMS version...

       Now checking that BASEstar Classic is installed...

       Now checking that OMNI Software is installed...

       Now checking disk space...

    * Do you want to purge files replaced by this installation [YES]?
    * Do you want to run the IVP after the installation [YES]?

       The installation procedure has no further questions to ask and will
       complete in 2 to 10 minutes depending on the system and system load.

    ------------------------------------------------------------------------------
       The configuration template file for OMNI support, DCM_OMNI_CONFIG.TEMPLATE,
       is used to define the OMNI paths, types, and devices.  Edit this file, as
       necessary, to reflect your specific site configuration.

       During installation it will be placed in the directory BCC$SYSDATA.
    ------------------------------------------------------------------------------

    ------------------------------------------------------------------------------
       The startup file for ILAN$DEVSRV, ILAN$SYSTEM_STARTUP.COM must be modified
       in order to use the DAS for OMNI Software.  This installation provides a
       substitute template for this file called ILAN$SYSTEM_STARTUP.TEMPLATE with
       modified privileges and quotas.  After installation, edit this file as
       necessary to match your site requirements.  Be sure to restore this edited
       file when upgrading BASEstar Classic software to a new version.

       During installation it will be placed in the directory BCC$SYSDATA.
    ------------------------------------------------------------------------------

    ------------------------------------------------------------------------------
       A utility to show the configuration of all OMNI devices,
       DCM_OMNI$SHOW_DEVICE.COM is provided with this DAS.  This utility
       extracts definitions from the BASEstar Classic database as well as from
       ODS and allows you to see the configuration of all your OMNI devices.

       During installation it will be placed in the directory BCC$SYSTEM.
    ------------------------------------------------------------------------------

       Now linking ILAN_OMNI shared image...

       Now linking IVP test routines...

    %VMSINSTAL-I-SYSDIR, This product creates system directory [SYSTEST.DCM_OMNI].
    %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

       Copyright 1990 Compaq Computer Corporation

       Confidential commercial computer software.  Valid license required.

       Executing the Installation Verification Procedure.

       Now checking OSI version...

       DECnet Plus V7.2 is supported.

       Now checking process privileges...

       Now checking that files have reached target directories...

       In order to test DAS connections, BASEstar Classic needs to be started.
       BASEstar Classic will be automatically started if you continue this IVP.

    * OK to continue IVP? [YES]

       BASEstar Classic will be started, please wait.

       Starting BASEstar Classic, please wait...
       Starting BASEstar Classic, please wait...

       BASEstar Classic is now running.

       Creating objects for MMS runtime test...

       Creating MMS OSI transport template...

    Processing NSAP 49::00-22:AA-00-04-00-74-89:20 (LOCAL:.OHF.BASEX2)

       Creating MMS ODS definitions...

       Creating MMS BASEstar Classic objects...

    BASEstar V3.4 for VMS
    Copyright (c) 1994, Digital Equipment Corporation.  All Rights Reserved.

    %BCC-S-OBJCRE, DCM_OMNI$MMS_TYP created.
    %BCC-S-OBJCRE, DCM_OMNI$MMS_PTH created.
    %BCC-S-OBJCRE, DCM_OMNI$MMS_IVP created.

       Now running the MMS-IS receiver application...

    IVP_MMS_RCVR: Starting the IVP receiver.

    IVP_MMS_RCVR: listening...

       Now trying to access an MMS device.

       Now writing to the MMS device.

    Device      : DCM_OMNI$MMS_IVP
    Address     : var_1
    Format      : S_LONGWORD

    IVP_MMS_RCVR: Accepted the connect.

    IVP_MMS_RCVR: Received a write variable request...

       Now reading from the MMS device.

    IVP_MMS_RCVR: Received a read variable request...

    Device      : DCM_OMNI$MMS_IVP
    Address     : var_1
    Format      : S_LONGWORD

    Data:
        0       :            10

    IVP_MMS_RCVR: received an ABORT.

    IVP_MMS_RCVR: All done...

       Creating objects for SINEC-AP runtime test...

       Creating SINEC-AP OSI transport template...

    Routing inactive area defined = {49::FF-00}
    Local SINEC-AP/H1 address = AA0004007489

       Creating SINEC-AP ODS definitions...

       Creating SINEC-AP BASEstar Classic objects...

    BASEstar V3.4 for VMS
    Copyright (c) 1994, Digital Equipment Corporation.  All Rights Reserved.

    %BCC-S-OBJCRE, DCM_OMNI$AP_TYP created.
    %BCC-S-OBJCRE, DCM_OMNI$AP_PTH created.
    %BCC-S-OBJCRE, DCM_OMNI$AP_IVP created.

       Now running the SINEC-AP receiver application...

    IVP_AP_RCVR: Starting the IVP receiver.

    IVP_AP_RCVR: listening...

       Now trying to access a SINEC-AP device.
    IVP_AP_RCVR: Accepted the connect.

       Now writing to the SINEC-AP device.

    Device      : DCM_OMNI$AP_IVP
    Address     : var_1
    Format      : S_LONGWORD

    IVP_AP_RCVR: Received a write variable request...

       Now reading from the SINEC-AP device.

    IVP_AP_RCVR: Received a read variable request...

    Device      : DCM_OMNI$AP_IVP
    Address     : var_1
    Format      : S_LONGWORD

    Data:
        0       :            10

    IVP_AP_RCVR: received an ABORT.

    IVP_AP_RCVR: All done...

       Creating objects for SINEC-H1 runtime test...

       Creating SINEC-H1 OSI transport template...

    Routing inactive area defined = {49::FF-00}
    Local SINEC-AP/H1 address = AA0004007489

       Creating SINEC-H1 ODS definitions...

       Creating SINEC-H1 BASEstar Classic objects...

    BASEstar V3.4 for VMS
    Copyright (c) 1994, Digital Equipment Corporation.  All Rights Reserved.

    %BCC-S-OBJCRE, DCM_OMNI$H1_TYP created.
    %BCC-S-OBJCRE, DCM_OMNI$H1_PTH created.
    %BCC-S-OBJCRE, DCM_OMNI$H1_IVP created.

       Now running the SINEC-H1 receiver application...

    IVP_H1_RCVR: Starting the IVP receiver.

    IVP_H1_RCVR: listening...

       Now trying to access a SINEC-H1 device.
    IVP_H1_RCVR: Accepted the connect.

       Now writing to the SINEC-H1 device.

    Device      : DCM_OMNI$H1_IVP
    Address     : U\DB:190:7
    Format      : S_LONGWORD

    IVP_H1_RCVR: Received a write variable request...

       Now reading from the SINEC-H1 device.

    IVP_H1_RCVR: Received a read variable request...

    Device      : DCM_OMNI$H1_IVP
    Address     : U\DB:190:7
    Format      : S_LONGWORD

    Data:
        0       :            10

    IVP_H1_RCVR: received an ABORT.

    IVP_H1_RCVR: All done...

       Creating objects for Siemens-S7 runtime test...

       Creating Siemens-S7 OSI transport template...

    Routing inactive area defined = {49::FF-00}
    Local SINEC-AP/H1 address = AA0004007489

       Creating Siemens-S7 ODS definitions...

       Creating Siemens-S7 BASEstar Classic objects...

    BASEstar V3.4 for VMS
    Copyright (c) 1994, Digital Equipment Corporation.  All Rights Reserved.

    %BCC-S-OBJCRE, DCM_OMNI$S7_TYP created.
    %BCC-S-OBJCRE, DCM_OMNI$S7_PTH created.
    %BCC-S-OBJCRE, DCM_OMNI$S7_IVP created.

       Now running the SINEC-S7 receiver application...

    IVP_S7_RCVR: Starting the IVP receiver.

    IVP_S7_RCVR: listening...

       Now trying to access a SINEC-S7 device.
    IVP_S7_RCVR: Accepted the connect.

       Now writing to the SINEC-S7 device.

    Device      : DCM_OMNI$S7_IVP
    Address     : U\DB:190:7
    Format      : S_LONGWORD

    IVP_S7_RCVR: Received a write variable request...

       Now reading from the SINEC-S7 device.

    IVP_S7_RCVR: Received a read variable request...

    Device      : DCM_OMNI$S7_IVP
    Address     : U\DB:190:7
    Format      : S_LONGWORD

    Data:
        0       :            10

    IVP_S7_RCVR: received an ABORT.

    IVP_S7_RCVR: All done...

       The BASEstar Classic DAS for OMNI Software IVP has successfully completed.

            Installation of DCM_OMNIVVA V3.4 completed at 08:25

            VMSINSTAL procedure done at 08:25

Previous | Next | Contents | Index