Document revision date: 30 March 2001

## OpenVMS Alpha System Analysis Tools Manual

Previous | Contents | Index

## CLUE CLEANUP

> Performs housekeeping operations to conserve disk space.

### Format

> CLUE CLEANUP

### Parameters

> None.

### Qualifiers

> None.

### Description

> CLUE CLEANUP performs housekeeping operations to conserve disk space. To avoid filling up the system disk with listing files generated by CLUE, CLUE CLEANUP is run during system startup to check the overall disk space used by all CLUE$*.LIS files.

> If the CLUE$COLLECT:CLUE$*.LIS files occupy more space than the logical CLUE$MAX_BLOCKS allows, then the oldest files are deleted until the threshold is reached. If this logical name is not defined, a default value of 5,000 disk blocks is assumed. A value of zero disables housekeeping and no check on the disk space is performed.

### Example

    SDA>  CLUE CLEANUP
    %CLUE-I-CLEANUP, housekeeping started...
    %CLUE-I-MAXBLOCK, maximum blocks allowed 5000 blocks
    %CLUE-I-STAT, total of 4 CLUE files, 192 blocks.

> In this example, the CLUE CLEANUP command displays that the total number of blocks of disk space used by CLUE files does not exceed the maximum number of blocks allowed. No files are deleted.

## CLUE CONFIG

> Displays the system, memory, and device configurations.

### Format

> CLUE CONFIG

### Parameters

> None.

### Qualifiers

> None.

### Description

> CLUE CONFIG displays the system, memory, and device configurations.

Example

## CLUE CRASH

> Displays a crash dump summary.

### Format

> CLUE CRASH

### Parameters

> None.

### Qualifiers

> None.

### Description

> CLUE CRASH displays a crash dump summary, which includes the following items:
> - Bugcheck type
> - Current process and image
> - Failing PC and PS
> - Executive image section name and offset
> - General registers
> - Failing instructions
> - Exception frame, signal and mechanism arrays (if available)
> - CPU state information (spinlock related bugchecks only)

### Example

    SDA>  CLUE CRASH
    Crash Time:        30-AUG-1996 13:13:46.83
    Bugcheck Type:     SSRVEXCEPT, Unexpected system service exception
    Node:              SWPCTX  (Standalone)
    CPU Type:          DEC 3000 Model 400
    VMS Version:       X6AF-FT2
    Current Process:   SYSTEM
    Current Image:     $31$DKB0:[SYS0.][SYSMGR]X.EXE;1
    Failing PC:        00000000.00030078    SYS$K_VERSION_01+00078
    Failing PS:        00000000.00000003
    Module:            X
    Offset:            00030078

    Boot Time:         30-AUG-1996 09:06:22.00
    System Uptime:               0 04:07:24.83
    Crash/Primary CPU: 00/00
    System/CPU Type:   0402
    Saved Processes:   18
    Pagesize:          8 KByte (8192 bytes)
    Physical Memory:   64 MByte (8192 PFNs, contiguous memory)
    Dumpfile Pagelets: 98861 blocks
    Dump Flags:        olddump,writecomp,errlogcomp,dump_style
    Dump Type:         raw,selective
    EXE$GL_FLAGS:      poolpging,init,bugdump
    Paging Files:      1 Pagefile and 1 Swapfile installed

    Stack Pointers:
    KSP = 00000000.7FFA1C98   ESP = 00000000.7FFA6000   SSP = 00000000.7FFAC100
    USP = 00000000.7AFFBAD0

    General Registers:
    R0  = 00000000.00000000   R1  = 00000000.7FFA1EB8   R2  = FFFFFFFF.80D0E6C0
    R3  = FFFFFFFF.80C63460   R4  = FFFFFFFF.80D12740   R5  = 00000000.000000C8
    R6  = 00000000.00030038   R7  = 00000000.7FFA1FC0   R8  = 00000000.7FFAC208
    R9  = 00000000.7FFAC410   R10 = 00000000.7FFAD238   R11 = 00000000.7FFCE3E0
    R12 = 00000000.00000000   R13 = FFFFFFFF.80C6EB60   R14 = 00000000.00000000
    R15 = 00000000.009A79FD   R16 = 00000000.000003C4   R17 = 00000000.7FFA1D40
    R18 = FFFFFFFF.80C05C38   R19 = 00000000.00000000   R20 = 00000000.7FFA1F50
    R21 = 00000000.00000000   R22 = 00000000.00000001   R23 = 00000000.7FFF03C8
    R24 = 00000000.7FFF0040   AI  = 00000000.00000003   RA  = FFFFFFFF.82A21080
    PV  = FFFFFFFF.829CF010   R28 = FFFFFFFF.8004B6DC   FP  = 00000000.7FFA1CA0
    PC  = FFFFFFFF.82A210B4   PS  = 18000000.00000000

    Exception Frame:
    R2  = 00000000.00000003   R3  = FFFFFFFF.80C63460   R4  = FFFFFFFF.80D12740
    R5  = 00000000.000000C8   R6  = 00000000.00030038   R7  = 00000000.7FFA1FC0
    PC  = 00000000.00030078   PS  = 00000000.00000003

    Signal Array:                            64-bit Signal Array:
    Arg Count    = 00000005                  Arg Count      =          00000005
    Condition    = 0000000C                  Condition      = 00000000.0000000C
    Argument #2  = 00010000                  Argument #2    = 00000000.00010000
    Argument #3  = 00000000                  Argument #3    = 00000000.00000000
    Argument #4  = 00030078                  Argument #4    = 00000000.00030078
    Argument #5  = 00000003                  Argument #5    = 00000000.00000003

    Mechanism Array:
    Arguments    = 0000002C                  Establisher FP = 00000000.7AFFBAD0
    Flags        = 00000000                  Exception FP   = 00000000.7FFA1F00
    Depth        = FFFFFFFD                  Signal Array   = 00000000.7FFA1EB8
    Handler Data = 00000000.00000000         Signal64 Array = 00000000.7FFA1ED0
    R0  = 00000000.00020000   R1  = 00000000.00000000   R16 = 00000000.00020004
    R17 = 00000000.00010050   R18 = FFFFFFFF.FFFFFFFF   R19 = 00000000.00000000
    R20 = 00000000.7FFA1F50   R21 = 00000000.00000000   R22 = 00000000.00010050
    R23 = 00000000.00000000   R24 = 00000000.00010051   R25 = 00000000.00000000
    R26 = FFFFFFFF.8010ACA4   R27 = 00000000.00010050   R28 = 00000000.00000000

    System Registers:
    Page Table Base Register (PTBR)                           00000000.00001136
    Processor Base Register (PRBR)                            FFFFFFFF.80D0E000
    Privileged Context Block Base (PCBB)                      00000000.003FE080
    System Control Block Base (SCBB)                          00000000.000001DC
    Software Interrupt Summary Register (SISR)                00000000.00000000
    Address Space Number (ASN)                                00000000.0000002F
    AST Summary / AST Enable (ASTSR_ASTEN)                    00000000.0000000F
    Floating-Point Enable (FEN)                               00000000.00000000
    Interrupt Priority Level (IPL)                            00000000.00000000
    Machine Check Error Summary (MCES)                        00000000.00000000
    Virtual Page Table Base Register (VPTB)                   FFFFFFFC.00000000

    Failing Instruction:
    SYS$K_VERSION_01+00078:         LDL             R28,(R28)

    Instruction Stream (last 20 instructions):
    SYS$K_VERSION_01+00028:         LDQ             R16,#X0030(R13)
    SYS$K_VERSION_01+0002C:         LDQ             R27,#X0048(R13)
    SYS$K_VERSION_01+00030:         LDA             R17,(R28)
    SYS$K_VERSION_01+00034:         JSR             R26,(R26)
    SYS$K_VERSION_01+00038:         LDQ             R26,#X0038(R13)
    SYS$K_VERSION_01+0003C:         BIS             R31,SP,SP
    SYS$K_VERSION_01+00040:         BIS             R31,R26,R0
    SYS$K_VERSION_01+00044:         BIS             R31,FP,SP
    SYS$K_VERSION_01+00048:         LDQ             R28,#X0008(SP)
    SYS$K_VERSION_01+0004C:         LDQ             R13,#X0010(SP)
    SYS$K_VERSION_01+00050:         LDQ             FP,#X0018(SP)
    SYS$K_VERSION_01+00054:         LDA             SP,#X0020(SP)
    SYS$K_VERSION_01+00058:         RET             R31,(R28)
    SYS$K_VERSION_01+0005C:         BIS             R31,R31,R31
    SYS$K_VERSION_01+00060:         LDA             SP,#XFFE0(SP)
    SYS$K_VERSION_01+00064:         STQ             FP,#X0018(SP)
    SYS$K_VERSION_01+00068:         STQ             R27,(SP)
    SYS$K_VERSION_01+0006C:         BIS             R31,SP,FP
    SYS$K_VERSION_01+00070:         STQ             R26,#X0010(SP)
    SYS$K_VERSION_01+00074:         LDA             R28,(R31)
    SYS$K_VERSION_01+00078:         LDL             R28,(R28)
    SYS$K_VERSION_01+0007C:         BEQ             R28,#X000007
    SYS$K_VERSION_01+00080:         LDQ             R26,#XFFE8(R27)
    SYS$K_VERSION_01+00084:         BIS             R31,R26,R0
    SYS$K_VERSION_01+00088:         BIS             R31,FP,SP

## CLUE ERRLOG

> Extracts the error log buffers from the dump file and places them into the binary file called CLUE$ERRLOG.SYS.

### Format

> CLUE ERRLOG [/OLD]

### Parameters

> None.

### Qualifier

> #### /OLD

> Dumps the errorlog buffers into a file using the old errorlog format. The default action, if /OLD is not specified, is to dump the errorlog buffers in the common event header format.

### Description

> CLUE ERRLOG extracts the error log buffers from the dump file and places them into the binary file called CLUE$ERRLOG.SYS.

> These buffers contain messages not yet written to the error log file at the time of the failure. When you analyze a failure on the same system on which it occurred, you can run the Error Log utility on the actual error log file to see these error log messages. When analyzing a failure from another system, use the CLUE ERRLOG command to create a file containing the failing system's error log messages just prior to the failure. System failures are often triggered by hardware problems, so determining what, if any, hardware errors occurred prior to the failure can help you troubleshoot a failure.

> You can define the logical CLUE$ERRLOG to any file specification if you want error log information written to a file other than CLUE$ERRLOG.SYS.

> Note You need at least DECevent V2.9 to analyze the new common event header (CEH) format file. The old format file can be analyzed by ANALYZE/ERROR or any version of DECevent.

### Example

    SDA>  CLUE ERRLOG

    Sequence  Date        Time
    --------  ----------- -----------
         128  11-MAY-1994 00:39:31.30
         129  11-MAY-1994 00:39:32.12
         130  11-MAY-1994 00:39:44.83
         131  11-MAY-1994 00:44:38.97 * Crash Entry

> In addition to writing the error log buffers into CLUE$ERRLOG.SYS, the CLUE ERRLOG command displays the sequence, date, and time of each error log buffer extracted from the dump file.

## CLUE FRU

> Outputs the Field Replacement Unit (FRU) table to a file for display by DECevent.

### Format

> CLUE FRU

### Parameters

> None.

### Qualifiers

> None.

### Description

> The FRU command extracts the FRU table into an output file (CLUE$FRU.SYS), which can then be displayed by DECevent. This command works on the running system, as well as on dump files.

## CLUE HISTORY

> Updates history file and generates crash dump summary output.

### Format

> CLUE HISTORY [/qualifier]

### Parameters

> None.

### Qualifier

> #### /OVERRIDE

> Allows execution of this command even if the dump file has already been analyzed (DMP$V_OLDDUMP bit set).

### Description

> This command updates the history file pointed to by the logical name CLUE$HISTORY with a one-line entry and the major crash dump summary information. If CLUE$HISTORY is not defined, a file CLUE$HISTORY.DAT in your default directory will be created.

> In addition, a listing file with summary information about the system failure is created in the directory pointed to by CLUE$COLLECT. The file name is of the form CLUE$node_ddmmyy_hhmm.LIS where the timestamp (hhmm) corresponds to the system failure time and not the time when the file was created.

> The listing file contains summary information collected from the following SDA commands:

> - CLUE CRASH
> - CLUE CONFIG
> - CLUE MEMORY/FILES
> - CLUE MEMORY/STATISTIC
> - CLUE PROCESS/RECALL
> - CLUE XQP/ACTIVE

> Refer to the reference section for each of these commands to see examples of the displayed information.

> The logical name CLUE$FLAG controls how much information is written to the listing file.

> - Bit 0---Include crash dump summary
> - Bit 1---Include system configuration
> - Bit 2---Include stack decoding information
> - Bit 3---Include page and swap file usage
> - Bit 4---Include memory management statistics
> - Bit 5---Include process DCL recall buffer
> - Bit 6---Include active XQP process information
> - Bit 7---Include XQP cache header

> If this logical name is undefined, all bits are set by default internally and all information is written to the listing file. If the value is zero, no listing file is generated. The value has to be supplied in hexadecimal form (for example, DEFINE CLUE$FLAG 81 will include the crash dump summary and the XQP cache header information).

> If the logical name CLUE$SITE_PROC points to a valid and existing file, it will be executed as the final step of the CLUE HISTORY command (for example, automatic saving of the dump file during system startup). If used, this file should contain only valid SDA commands.

> Refer to Chapter 2, Section 2.2.3 for more information on site-specific command files.

## CLUE MCHK

> This command is obsolete.

### Format

> CLUE MCHK

### Parameters

> None.

### Qualifiers

> None.

### Description

> The CLUE MCMK command has been withdrawn. Issuing the command produces the following output, explaining the correct way to obtain MACHINECHECK information from a crash dump.

>     Please use the following commands in order to extract the errorlog buffers
>     from the dumpfile header and analyze the machine check entry:

>     $ analyze/crash sys$system:sysdump.dmp
>     SDA> clue errlog
>     SDA> exit
>     $ diagnose clue$errlog

## CLUE MEMORY

> Displays memory- and pool-related information.

### Format

> CLUE MEMORY [/qualifier[,...]]

### Parameters

> None.

### Qualifiers

> #### /FILES

> Displays information about page and swap file usage.

> #### /FREE [/FULL]

> Validates and displays dynamic nonpaged free packet list queue.

> #### /GH [/FULL]

> Displays information about the granularity hint regions.

> #### /LAYOUT

> Decodes and displays much of the system virtual address space layout.

> #### /LOOKASIDE

> Validates the lookaside list queue heads and counts the elements for each list.

> #### /STATISTIC

> Displays systemwide performance data such as page fault, I/O, pool, lock manager, MSCP, and file system cache.

### Description

> The CLUE MEMORY command displays memory- and pool-related information.

### Examples

#1
    SDA> CLUE MEMORY/FILES
    Paging File Usage (blocks):
    ---------------------------

    Swapfile (Index   1)                     Device                    DKA0:
       PFL Address      FFFFFFFF.81531340    UCB Address      FFFFFFFF.814AAF00
       Free Blocks                  44288    Bitmap           FFFFFFFF.815313E0
       Total Size (blocks)          44288    Flags             inited,swap_file
       Total Write Count                0    Total Read Count                 0
       Smallest Chunk (pages)        2768    Largest Chunk (pages)         2768
       Chunks GEQ 64 Pages              1    Chunks LT 64 Pages               0

    Pagefile (Index 254)                     Device                    DKA0:
       PFL Address      FFFFFFFF.8152E440    UCB Address      FFFFFFFF.814AAF00
       Free Blocks                1056768    Bitmap           FFFFFFFF.6FB16008
       Total Size (blocks)        1056768    Flags                       inited
       Total Write Count                0    Total Read Count                 0
       Smallest Chunk (pages)       66048    Largest Chunk (pages)        66048
       Chunks GEQ 64 Pages              1    Chunks LT 64 Pages               0

       Summary:  1 Pagefile and 1 Swapfile installed

       Total Size of all Swap Files:            44288 blocks
       Total Size of all Paging Files:        1056768 blocks
       Total Committed Paging File Usage:      344576 blocks

> This example shows the display produced by the CLUE MEMORY/FILES command.

#2
    SDA>  CLUE MEMORY/FREE/FULL
    Non-Paged Dynamic Storage Pool - Variable Free Packet Queue:
    ------------------------------------------------------------
    CLASSDR  FFFFFFFF.80D157C0 :    64646464 64646464 00000040 80D164C0  ÀdÑ.@...dddddddd
    CLASSDR  FFFFFFFF.80D164C0 :    64646464 64646464 00000080 80D17200  .rÑ.....dddddddd
    CLASSDR  FFFFFFFF.80D17200 :    64646464 64646464 00000080 80D21AC0  À.Ò.....dddddddd
    CLASSDR  FFFFFFFF.80D21AC0 :    64646464 64646464 00000080 80D228C0  À(Ò.....dddddddd
    VCC      FFFFFFFF.80D228C0 :    801CA5E8 026F0040 00000040 80D23E40  @>Ò.@...@.o.è¥..
    CLASSDR  FFFFFFFF.80D23E40 :    64646464 64646464 00000040 80D24040  @@Ò.@...dddddddd
    CLASSDR  FFFFFFFF.80D24040 :    64646464 64646464 00000040 80D26FC0  ÀoÒ.@...dddddddd
    CLASSDR  FFFFFFFF.80D26FC0 :    64646464 64646464 00000080 80D274C0  ÀtÒ.....dddddddd
    CLASSDR  FFFFFFFF.80D274C0 :    64646464 64646464 00000040 80D2E200  .âÒ.@...dddddddd
    CLASSDR  FFFFFFFF.80D2E200 :    64646464 64646464 00000080 80D2E440  @äÒ.....dddddddd
    CLASSDR  FFFFFFFF.80D2E440 :    64646464 64646464 00000040 80D2F000  .Ò.@...dddddddd
    CLASSDR  FFFFFFFF.80D2F000 :    64646464 64646464 00000080 80D2F400  .ôÒ.....dddddddd
       .
       .
       .
    CLASSDR  FFFFFFFF.80E91D40 :    64646464 64646464 00000500 80E983C0  À.é.....dddddddd
    CLASSDR  FFFFFFFF.80E983C0 :    64646464 64646464 00031C40 00000000  ....@...dddddddd
    Free Packet Queue, Status: Valid, 174 elements
       Largest free chunk:        00031C40 (hex)    203840 (dec)  bytes
       Total free dynamic space:  0003D740 (hex)    251712 (dec)  bytes

> The CLUE MEMORY/FREE/FULL command validates and displays dynamic nonpaged free packet list queue.

#3
    SDA>  CLUE MEMORY/GH/FULL
    Granularity Hint Regions - Huge Pages:
    --------------------------------------

    Execlet Code Region                                                 Pages/Slices
       Base/End VA     FFFFFFFF.80000000 FFFFFFFF.80356000  Current Size  427/   427
       Base/End PA     00000000.00400000 00000000.00756000  Free             /     0
       Total Size      00000000.00356000            3.3 MB  In Use           /   427
       Bitmap VA/Size  FFFFFFFF.80D17CC0 00000000.00000040  Initial Size  512/   512
       Slice Size      00000000.00002000                    Released       85/    85
       Next free Slice 00000000.000001AB

       Image                                 Base               End          Length
       SYS$PUBLIC_VECTORS             FFFFFFFF.80000000  FFFFFFFF.80001A00  00001A00
       SYS$BASE_IMAGE                 FFFFFFFF.80002000  FFFFFFFF.8000D400  0000B400
       SYS$CNBTDRIVER                 FFFFFFFF.8000E000  FFFFFFFF.8000F000  00001000
       SYS$NISCA_BTDRIVER             FFFFFFFF.80010000  FFFFFFFF.8001FA00  0000FA00
       SYS$ESBTDRIVER                 FFFFFFFF.80020000  FFFFFFFF.80022400  00002400
       SYS$OPDRIVER                   FFFFFFFF.80024000  FFFFFFFF.80027C00  00003C00
       SYSTEM_DEBUG                   FFFFFFFF.80028000  FFFFFFFF.80050200  00028200
       SYSTEM_PRIMITIVES              FFFFFFFF.80052000  FFFFFFFF.80089000  00037000
       SYSTEM_SYNCHRONIZATION         FFFFFFFF.8008A000  FFFFFFFF.80095400  0000B400
       ERRORLOG                       FFFFFFFF.80096000  FFFFFFFF.80099200  00003200
       SYS$CPU_ROUTINES_0402          FFFFFFFF.8009A000  FFFFFFFF.800A3A00  00009A00
       EXCEPTION_MON                  FFFFFFFF.800A4000  FFFFFFFF.800BC800  00018800
       IO_ROUTINES_MON                FFFFFFFF.800BE000  FFFFFFFF.800E2000  00024000
       SYSDEVICE                      FFFFFFFF.800E2000  FFFFFFFF.800E5C00  00003C00
       PROCESS_MANAGEMENT_MON         FFFFFFFF.800E6000  FFFFFFFF.8010B000  00025000
       SYS$VM                         FFFFFFFF.8010C000  FFFFFFFF.80167200  0005B200
       SHELL8K                        FFFFFFFF.80168000  FFFFFFFF.80169200  00001200
       LOCKING                        FFFFFFFF.8016A000  FFFFFFFF.8017BE00  00011E00
       MESSAGE_ROUTINES               FFFFFFFF.8017C000  FFFFFFFF.80182A00  00006A00
       LOGICAL_NAMES                  FFFFFFFF.80184000  FFFFFFFF.80186C00  00002C00
       F11BXQP                        FFFFFFFF.80188000  FFFFFFFF.80190400  00008400
       SYSLICENSE                     FFFFFFFF.80192000  FFFFFFFF.80192400  00000400
       IMAGE_MANAGEMENT               FFFFFFFF.80194000  FFFFFFFF.80197A00  00003A00
       SECURITY                       FFFFFFFF.80198000  FFFFFFFF.801A0E00  00008E00
       SYSGETSYI                      FFFFFFFF.801A2000  FFFFFFFF.801A3A00  00001A00
       SYS$TRANSACTION_SERVICES       FFFFFFFF.801A4000  FFFFFFFF.801C5000  00021000
       SYS$UTC_SERVICES               FFFFFFFF.801C6000  FFFFFFFF.801C7000  00001000
       SYS$VCC_MON                    FFFFFFFF.801C8000  FFFFFFFF.801D4E00  0000CE00
       SYS$IPC_SERVICES               FFFFFFFF.801D6000  FFFFFFFF.80214A00  0003EA00
       SYSLDR_DYN                     FFFFFFFF.80216000  FFFFFFFF.80219200  00003200
       SYS$MME_SERVICES               FFFFFFFF.8021A000  FFFFFFFF.8021B000  00001000
       SYS$TTDRIVER                   FFFFFFFF.8021C000  FFFFFFFF.8022FE00  00013E00
       SYS$PKCDRIVER                  FFFFFFFF.80230000  FFFFFFFF.80240400  00010400
       SYS$DKDRIVER                   FFFFFFFF.80242000  FFFFFFFF.80251600  0000F600
       RMS                            FFFFFFFF.80252000  FFFFFFFF.802C5E00  00073E00
       SYS$GXADRIVER                  FFFFFFFF.802C6000  FFFFFFFF.802CE000  00008000
       SYS$ECDRIVER                   FFFFFFFF.802CE000  FFFFFFFF.802D1000  00003000
       SYS$LAN                        FFFFFFFF.802D2000  FFFFFFFF.802D8E00  00006E00
       SYS$LAN_CSMACD                 FFFFFFFF.802DA000  FFFFFFFF.802E6600  0000C600
       SYS$MKDRIVER                   FFFFFFFF.802E8000  FFFFFFFF.802F1C00  00009C00
       SYS$YRDRIVER                   FFFFFFFF.802F2000  FFFFFFFF.802F9600  00007600
       SYS$SODRIVER                   FFFFFFFF.802FA000  FFFFFFFF.802FF000  00005000
       SYS$INDRIVER                   FFFFFFFF.80300000  FFFFFFFF.8030EA00  0000EA00
       NETDRIVER                      FFFFFFFF.80310000  FFFFFFFF.80310200  00000200
       NETDRIVER                      FFFFFFFF.80312000  FFFFFFFF.80329E00  00017E00
       SYS$IMDRIVER                   FFFFFFFF.8032A000  FFFFFFFF.8032EA00  00004A00
       SYS$IKDRIVER                   FFFFFFFF.80330000  FFFFFFFF.8033AC00  0000AC00
       NDDRIVER                       FFFFFFFF.8033C000  FFFFFFFF.8033F800  00003800
       SYS$WSDRIVER                   FFFFFFFF.80340000  FFFFFFFF.80341600  00001600
       SYS$CTDRIVER                   FFFFFFFF.80342000  FFFFFFFF.8034D200  0000B200
       SYS$RTTDRIVER                  FFFFFFFF.8034E000  FFFFFFFF.80351800  00003800
       SYS$FTDRIVER                   FFFFFFFF.80352000  FFFFFFFF.80354200  00002200

    Execlet Data Region                                                 Pages/Slices
       Base/End VA     FFFFFFFF.80C00000 FFFFFFFF.80CC0000  Current Size   96/  1536
       Base/End PA     00000000.00800000 00000000.008C0000  Free             /    11
       Total Size      00000000.000C0000            0.7 MB  In Use           /  1525
       Bitmap VA/Size  FFFFFFFF.80D17D00 00000000.00000100  Initial Size  128/  2048
       Slice Size      00000000.00000200                    Released       32/   512
       Next free Slice 00000000.000005F5

       Image                                 Base               End          Length
       SYS$PUBLIC_VECTORS             FFFFFFFF.80C00000  FFFFFFFF.80C05000  00005000
       SYS$BASE_IMAGE                 FFFFFFFF.80C05000  FFFFFFFF.80C25E00  00020E00
       SYS$CNBTDRIVER                 FFFFFFFF.80C25E00  FFFFFFFF.80C26200  00000400
       SYS$NISCA_BTDRIVER             FFFFFFFF.80C26200  FFFFFFFF.80C29400  00003200
       SYS$ESBTDRIVER                 FFFFFFFF.80C29400  FFFFFFFF.80C29800  00000400
       SYS$OPDRIVER                   FFFFFFFF.80C29800  FFFFFFFF.80C2A200  00000A00
       SYSTEM_DEBUG                   FFFFFFFF.80C2A200  FFFFFFFF.80C4E400  00024200
       SYSTEM_PRIMITIVES              FFFFFFFF.80C4E400  FFFFFFFF.80C58200  00009E00
       SYSTEM_SYNCHRONIZATION         FFFFFFFF.80C58200  FFFFFFFF.80C5A000  00001E00
       ERRORLOG                       FFFFFFFF.80C5A000  FFFFFFFF.80C5A600  00000600
       SYS$CPU_ROUTINES_0402          FFFFFFFF.80C5A600  FFFFFFFF.80C5CA00  00002400
       EXCEPTION_MON                  FFFFFFFF.80C5CA00  FFFFFFFF.80C64C00  00008200
       IO_ROUTINES_MON                FFFFFFFF.80C64C00  FFFFFFFF.80C6AA00  00005E00
       SYSDEVICE                      FFFFFFFF.80C6AA00  FFFFFFFF.80C6B600  00000C00
       PROCESS_MANAGEMENT_MON         FFFFFFFF.80C6B600  FFFFFFFF.80C72600  00007000
       SYS$VM                         FFFFFFFF.80C72600  FFFFFFFF.80C79000  00006A00
       SHELL8K                        FFFFFFFF.80C79000  FFFFFFFF.80C7A000  00001000
       LOCKING                        FFFFFFFF.80C7A000  FFFFFFFF.80C7BA00  00001A00
       MESSAGE_ROUTINES               FFFFFFFF.80C7BA00  FFFFFFFF.80C7D000  00001600
       LOGICAL_NAMES                  FFFFFFFF.80C7D000  FFFFFFFF.80C7E200  00001200
       F11BXQP                        FFFFFFFF.80C7E200  FFFFFFFF.80C7FA00  00001800
       SYSLICENSE                     FFFFFFFF.80C7FA00  FFFFFFFF.80C7FE00  00000400
       IMAGE_MANAGEMENT               FFFFFFFF.80C7FE00  FFFFFFFF.80C80600  00000800
       SECURITY                       FFFFFFFF.80C80600  FFFFFFFF.80C83000  00002A00
       SYSGETSYI                      FFFFFFFF.80C83000  FFFFFFFF.80C83200  00000200
       SYS$TRANSACTION_SERVICES       FFFFFFFF.80C83200  FFFFFFFF.80C89E00  00006C00
       SYS$UTC_SERVICES               FFFFFFFF.80C89E00  FFFFFFFF.80C8A200  00000400
       SYS$VCC_MON                    FFFFFFFF.80C8A200  FFFFFFFF.80C8BC00  00001A00
       SYS$IPC_SERVICES               FFFFFFFF.80C8BC00  FFFFFFFF.80C91000  00005400
       SYSLDR_DYN                     FFFFFFFF.80C91000  FFFFFFFF.80C92200  00001200
       SYS$MME_SERVICES               FFFFFFFF.80C92200  FFFFFFFF.80C92600  00000400
       SYS$TTDRIVER                   FFFFFFFF.80C92600  FFFFFFFF.80C94C00  00002600
       SYS$PKCDRIVER                  FFFFFFFF.80C94C00  FFFFFFFF.80C96A00  00001E00
       SYS$DKDRIVER                   FFFFFFFF.80C96A00  FFFFFFFF.80C99800  00002E00
       RMS                            FFFFFFFF.80C99800  FFFFFFFF.80CAAC00  00011400
       RECOVERY_UNIT_SERVICES         FFFFFFFF.80CAAC00  FFFFFFFF.80CAB000  00000400
       SYS$GXADRIVER                  FFFFFFFF.80CAB000  FFFFFFFF.80CAF000  00004000
       SYS$ECDRIVER                   FFFFFFFF.80CAF000  FFFFFFFF.80CAFC00  00000C00
       SYS$LAN                        FFFFFFFF.80CAFC00  FFFFFFFF.80CB0800  00000C00
       SYS$LAN_CSMACD                 FFFFFFFF.80CB0800  FFFFFFFF.80CB1800  00001000
       SYS$MKDRIVER                   FFFFFFFF.80CB1800  FFFFFFFF.80CB3000  00001800
       SYS$YRDRIVER                   FFFFFFFF.80CB3000  FFFFFFFF.80CB3C00  00000C00
       SYS$SODRIVER                   FFFFFFFF.80CB3C00  FFFFFFFF.80CB4E00  00001200
       SYS$INDRIVER                   FFFFFFFF.80CB4E00  FFFFFFFF.80CB5E00  00001000
       NETDRIVER                      FFFFFFFF.80CB5E00  FFFFFFFF.80CB8800  00002A00
       SYS$IMDRIVER                   FFFFFFFF.80CB8800  FFFFFFFF.80CB9400  00000C00
       SYS$IKDRIVER                   FFFFFFFF.80CB9400  FFFFFFFF.80CBAA00  00001600
       NDDRIVER                       FFFFFFFF.80CBAA00  FFFFFFFF.80CBB400  00000A00
       SYS$WSDRIVER                   FFFFFFFF.80CBB400  FFFFFFFF.80CBBC00  00000800
       SYS$CTDRIVER                   FFFFFFFF.80CBBC00  FFFFFFFF.80CBD800  00001C00
       SYS$RTTDRIVER                  FFFFFFFF.80CBD800  FFFFFFFF.80CBE200  00000A00
       SYS$FTDRIVER                   FFFFFFFF.80CBE200  FFFFFFFF.80CBEA00  00000800
       11 free Slices                 FFFFFFFF.80CBEA00  FFFFFFFF.80CC0000  00001600

    S0/S1 Executive Data Region                                         Pages/Slices
       Base/End VA     FFFFFFFF.80D00000 FFFFFFFF.80ECA000  Current Size  229/   229
       Base/End PA     00000000.00900000 00000000.00ACA000  Free             /     0
       Total Size      00000000.001CA000            1.7 MB  In Use           /   229
       Bitmap VA/Size  FFFFFFFF.80D17E00 00000000.00000020  Initial Size  229/   229
       Slice Size      00000000.00002000                    Released        0/     0
       Next free Slice 00000000.00000007

       Item                                  Base               End          Length
       System Header                  FFFFFFFF.80D00000  FFFFFFFF.80D0A000  0000A000
       Error Log Allocation Buffers   FFFFFFFF.80D0A000  FFFFFFFF.80D0C000  00002000
       Nonpaged Pool (initial size)   FFFFFFFF.80D0E000  FFFFFFFF.80ECA000  001BC000

    Resident Image Code Region                                          Pages/Slices
       Base/End VA     FFFFFFFF.80400000 FFFFFFFF.80C00000  Current Size 1024/  1024
       Base/End PA     00000000.00C00000 00000000.01400000  Free             /   223
       Total Size      00000000.00800000            8.0 MB  In Use           /   801
       Bitmap VA/Size  FFFFFFFF.80D17E20 00000000.00000080  Initial Size 1024/  1024
       Slice Size      00000000.00002000                    Released        0/     0
       Next free Slice 00000000.00000321

       Image                                 Base               End          Length
       LIBRTL                         FFFFFFFF.80400000  FFFFFFFF.8049EA00  0009EA00
       LIBOTS                         FFFFFFFF.804A0000  FFFFFFFF.804AEC00  0000EC00
       CMA$TIS_SHR                    FFFFFFFF.804B0000  FFFFFFFF.804B2600  00002600
       DPML$SHR                       FFFFFFFF.804B4000  FFFFFFFF.8050B600  00057600
       DECC$SHR                       FFFFFFFF.8050C000  FFFFFFFF.80657000  0014B000
       SECURESHRP                     FFFFFFFF.80658000  FFFFFFFF.80676000  0001E000
       SECURESHR                      FFFFFFFF.80676000  FFFFFFFF.8068C000  00016000
       SECURESHR                      FFFFFFFF.8068C000  FFFFFFFF.8068C200  00000200
       LBRSHR                         FFFFFFFF.8068E000  FFFFFFFF.806A3E00  00015E00
       DECW$TRANSPORT_COMMON          FFFFFFFF.806A4000  FFFFFFFF.806B0C00  0000CC00
       CDE$UNIX_ROUTINES              FFFFFFFF.806B2000  FFFFFFFF.806C1E00  0000FE00
       DECW$XLIBSHR                   FFFFFFFF.806C2000  FFFFFFFF.80781C00  000BFC00
       DECW$XTLIBSHRR5                FFFFFFFF.80782000  FFFFFFFF.807C7600  00045600
       DECW$XMLIBSHR12                FFFFFFFF.807C8000  FFFFFFFF.8096AE00  001A2E00
       DECW$MRMLIBSHR12               FFFFFFFF.8096C000  FFFFFFFF.80994200  00028200
       DECW$DXMLIBSHR12               FFFFFFFF.80996000  FFFFFFFF.80A40400  000AA400
       223 free Slices                FFFFFFFF.80A42000  FFFFFFFF.80C00000  001BE000

    S2 Executive Data Region                                            Pages/Slices
       Base/End VA     FFFFFFFE.00000000 FFFFFFFE.00050000  Current Size   40/     8
       Base/End PA     00000000.00350000 00000000.003A0000  Free             /     0
       Total Size      00000000.00050000            0.3 MB  In Use           /     8
       Bitmap VA/Size  FFFFFFFF.80D17EA0 00000000.00000008  Initial Size   40/     8
       Slice Size      00000000.0000A000                    Released        0/     0
       Next free Slice 00000000.00000008

       Item                                  Base               End          Length
       PFN Database                   FFFFFFFE.00000000  FFFFFFFE.00050000  00050000

> Previous | Next | Contents | Index

> | privacy and legal statement |
> 6549PRO_022.HTML