# Compaq ACMS for OpenVMS
Remote Systems Management Guide

Previous | Contents | Index

## 9.4.1 Field Descriptions

Following are descriptions of the fields in Table 9-3.

- record_state
  The current state of this table entry. Valid states are VALID (the process is currently running and maintaining this table entry) or INACTIVE (the process is no longer running). Inactive rows are subject to reuse.
- id_coll_state
  The current collection state for this class and this process. Collection states can be modified by modifying entries in the Collection table. See Section 5.1 and Section 9.3 for discussions of data collection.
- process_name
  The OpenVMS process name for the process.
- pid
  The OpenVMS process identifier for the process.
- start_time
  Date and time the process was started.
- end_time
  Date and time the process ended. If the process has not yet ended, this field is null.
- user_name
  The OpenVMS account under which the process is running.
- astlm_active, biolm_active, bytlm_active, diolm_active, enqlm_active, fillm_active, pgflquota_active, tqelm_active, wsdefault_active, wsextent_active, wsquota_active
  The default value of the related OpenVMS process quota. This is the value of the quota when the CP process was started.
- astlm_stored, biolm_stored, bytlm_stored, diolm_stored, enqlm_stored, fillm_stored, pgflquota_stored, tqelm_stored, wsdefault_stored, wsextent_stored, wsquota_stored
  The value of the related process quota currently stored in the OpenVMS system user authorization file (SYSUAF.DAT).
- runtime_coll_state
  The current collection state for this class and this process. Collection states can be modified by modifying entries in the Collection table. See Section 5.1 and Section 9.3 for discussions of data collection.
  If this field is set to DISABLED, the process is not currently collecting data for the fields in this class. Any field values reflect activity during a prior period when collection was enabled.
- acms_state
  The ACMS state of the process.
- decnet_object
  If the process has a current DECnet object, the value of this field is STARTED. Otherwise, the value is STOPPED. If the DECnet object is stopped (and the runtime_coll_state is enabled for this process), either distributed processing has not been enabled (that is, the node_name parameter in the ACMSGEN file is NULL) or there is currently a problem with DECnet. Also, check the ACC CONFIG parameters node_name_active and node_name_stored to determine the current status of the ACMSGEN node_name field.
- current_attached_terms
  The number of terminals currently attached to the CP.
- active_task_calls
  The number of task calls currently being executed by all users of the CP.
- active_tdms_menu_reqs
  The number of TDMS menu requests currently being executed by all users of the CP.
- total_tdms_menu_reqs
  The total number of TDMS menu requests executed by all users of the CP since the CP was started.
- active_tdms_reqs
  The number of TDMS requests of all types currently being executed by all users of the CP.
- active_tdms_read_msgs
  The number of TDMS read messages currently being executed by all users of the CP.
- active_tdms_write_msgs
  The number of TDMS write messages currently being executed by all users of the CP.
- active_tdms_cancels
  The number of TDMS cancels currently being executed by all users of the CP.
- total_tdms_reqs
  The total number of TDMS requests (menu and exchange) executed by all users of the CP since the CP was started.

- total_tdms_read_msgs
  The total number of TDMS read messages executed by all users of the CP since the CP was started.
- total_tdms_write_msgs
  The total number of TDMS write messages executed by all users of the CP since the CP was started.
- total_tdms_cancels
  The total number of TDMS cancels executed by all users of the CP since the CP was started.
- active_df_menu_reqs
  The number of DECforms menu requests currently being executed by all users of the CP.
- total_df_menu_reqs
  The total number of DECforms menu requests executed by all users of the CP since the CP was started.
- active_df_reqs
  The number of DECforms requests of all types currently being executed by all users of the CP.
- active_df_enables
  The number of DECforms enable requests currently being executed by all users of the CP.
- active_df_disables
  The number of DECforms disable requests currently being executed by all users of the CP.
- active_df_cancels
  The number of DECforms cancel requests currently being executed by all users of the CP.
- active_df_sends
  The number of DECforms requests currently being executed by all users of the CP.
- active_df_receives
  The number of DECforms receive requests currently being executed by all users of the CP.
- active_df_transceives
  The number of DECforms enable transceives currently being executed by all users of the CP.
- total_df_reqs
  The total number of DECforms requests of all types executed by all users of the CP since the CP was started.
- total_df_enables
  The total number of DECforms enable requests executed by all users of the CP since the CP was started.

- total_df_disables
  The total number of DECforms disable requests executed by all users of the CP since the CP was started.
- total_df_cancels
  The total number of DECforms cancel requests executed by all users of the CP since the CP was started.
- total_df_sends
  The total number of DECforms send requests executed by all users of the CP since the CP was started.
- total_df_receives
  The total number of DECforms receive requests executed by all users of the CP since the CP was started.
- total_df_transceives
  The total number of DECforms transceive requests executed by all users of the CP since the CP was started.
- data_set_hangups
  The total number of data set hangups detected by the CP since the CP was started.
- astlm_current, biolm_current, bytlm_current, diolm_current, enqlm_current, fillm_current, pgflquota_current, tqelm_current, wssize_current, channelcnt_current
  The actual amount of the related OpenVMS process or system resource that is being consumed by the CP process. The frequency with which these fields are updated is based on the value of the vms_coll_interval field in the Parameter table (see Table 9-8).
- pool_coll_state
  The current collection state for this class and this process. Collection states can be modified by modifying entries in the Collection table. See Section 9.3 and Section 5.1 for discussions of data collection.
  If this field is set to DISABLED, the process is not currently collecting data for the fields in this class. Any field values reflect activity during a prior period when collection was enabled.
- mss_process_total
  The total size of the MSS process pool allocated for this process. The frequency with which this field is updated is based on the value of the Parameter table field mss_coll_interval (see Table 9-8).
- mss_process_free
  The amount of unused MSS process pool for this process. The frequency with which this field is updated is based on the value of the Parameter table field mss_coll_interval (see Table 9-8).
- mss_process_largest
  The largest unused block available in the MSS process pool for this process. The frequency with which this field is updated is based on the value of the Parameter table field mss_coll_interval (see Table 9-8).

- mss_process_failures
  The number of failed attempts to allocate space in the MSS process pool for this process. The frequency with which this field is updated is based on the value of the Parameter table field mss_coll_interval (see Table 9-8).
- mss_process_garbage
  The number of garbage collections that have been run to reclaim space in this processes MSS process pool. The frequency with which this field is updated is based on the value of the Parameter table field mss_coll_interval (see Table 9-8).
- err_coll_state
  The current collection state for this class and this process. Collection states can be modified by modifying entries in the Collection table. See Section 5.1 and Section 9.3 for discussions of data collection.
  Errors for this process are only sent to the Remote Manager if this field is set to ENABLED. If this field is set to DISABLED, the process will not collect data for the fields in this class; existing field values reflect activity during a prior period when collection was enabled.
- err_count
  The total number of errors related to this process that were sent to the Remote Manager.
- last_err_msg
  The text of the most recent error message related to this process that was sent to the Remote Manager.
- time_of_last_error
  Date and time of the most recent error message related to this process that was sent to the Remote Manager.

# 9.5 Error Filter Table

The Error Filter table enables users to increase the usefulness and manage the size of the Remote Manager error log by preventing an ACMS process from relaying repetitive or non-critical system messages. Each error filter record specifies a particular system message to suppress. These messages continue to be displayed on ACMS systems, but they are not sent to or recorded by the Remote Manager.

The following table shows the fields in an ACMS error filter record. Note that the data in this table is persistent and durable. However, table entries can removed manually using the ACMSMGR DELETE FILTER command.

Table 9-4 Error Filter Table
Field Name | Data Type | SNMP Access | RPC Access | Dynamic
--- | --- | --- | --- | ---
node_name++ | string | RW | RW |
message_code++ | integer | RW | RW |
message_name++ | string | RW | RW |

++Only valid for use with systems running ACMS Version 4.4 or higher.

Key to Access Modes

- R---Read Access
- RW---Read/Write Access
- Blank---Not available to the interface
- D---Field is dynamic

## 9.5.1 Field Descriptions

Following are descriptions of the fields in Table 9-4.

- node_name
  Name of the OpenVMS node on which to filter error messages.
- message_code
  The hexadecimal value or symbolic error name associated with the message being filtered.

# 9.6 EXC Table

The EXC table is sized according to the MAX_APPLS ACMSGEN parameter.

Table 9-5 EXC Table
Collection Class | Field | Data Type | SNMP Access | RPC Access | Dynamic
--- | --- | --- | --- | --- | ---
ID | record_state | integer | R | R |
ID | id_coll_state | integer | R | R |
ID | process_name | string | R | R |
ID | user_name | string | R | R |
ID | pid | integer | R | R |
ID | start_time | time | R | R |
ID | end_time | time | R | R |
ID | appl_name | string | R | R |
ID | build_time | time | R | R |
ID | exc_appl_tbl_state | integer | R |  |
ID | exc_server_types | integer | R |  |
ID | exc_task_groups | integer | R |  |
CONFIG | config_coll_state | integer | R | R |
CONFIG | acms_state | integer | RW | R | D
CONFIG | audit_state_active | integer | RW | RW | D
CONFIG | audit_state_stored | state1 | R | R |
CONFIG | max_tasks_active | integer | RW | RW | D
CONFIG | max_tasks_stored | integer | R | R |
CONFIG | sp_monitoring_interval_active | integer | RW | RW | D
CONFIG | sp_monitoring_interval_stored | state1 | R | R |
CONFIG | max_servers_active | integer | RW | RW | D
CONFIG | max_servers_stored | integer | R | R |
CONFIG | transaction_timeout_active | integer | RW | RW | D
CONFIG | transaction_timeout_stored | integer | R | R |
CONFIG | astlm_active++ | integer | R | R |
CONFIG | astlm_stored++ | integer | RW | RW |
CONFIG | biolm_active++ | integer | R | R |
CONFIG | biolm_stored++ | integer | RW | RW |
CONFIG | bytlm_active++ | integer | R | R |
CONFIG | bytlm_stored++ | integer | RW | RW |
CONFIG | diolm_active++ | integer | R | R |
CONFIG | diolm_stored++ | integer | RW | RW |
CONFIG | enqlm_active++ | integer | R | R |
CONFIG | enqlm_stored++ | integer | RW | RW |
CONFIG | fillm_active++ | integer | R | R |
CONFIG | fillm_stored++ | integer | RW | RW |
CONFIG | pgflquota_active++ | integer | R | R |
CONFIG | pgflquota_stored++ | integer | RW | RW |
CONFIG | tqelm_active++ | integer | R | R |
CONFIG | tqelm_stored++ | integer | RW | RW |
CONFIG | wsdefault_active++ | integer | R | R |
CONFIG | wsdefault_stored++ | integer | RW | RW |
CONFIG | wsextent_active++ | integer | R | R |
CONFIG | wsextent_stored++ | integer | RW | RW |
CONFIG | wsquota_active++ | integer | R | R |
CONFIG | wsquota_stored++ | integer | RW | RW |
CONFIG | ws_poolsize++ | integer | R | R |
CONFIG | wsc_poolsize++ | integer | R | R |
CONFIG | tws_poolsize++ | integer | R | R |
CONFIG | twsc_poolsize++ | integer | R | R |
RUNTIME | runtime_coll_state | integer | R | R |
RUNTIME | decnet_object | integer | R | R |
RUNTIME | current_servers | gauge | R | R |
RUNTIME | current_submitters | gauge | R | R |
RUNTIME | current_tasks | gauge | R | R |
RUNTIME | total_tasks_executed | integer | R | R |
RUNTIME | total_submitters | integer | R | R |
RUNTIME | current active_servers | gauge | R | R |
RUNTIME | current_free_servers | gauge | R | R |
RUNTIME | current_waiting_tasks | gauge | R | R |
RUNTIME | server_start_count | integer | R | R |
RUNTIME | server_failure_count | integer | R | R |
RUNTIME | server_process_total++ | gauge | R | R |
RUNTIME | task_failures | integer | R | R |
RUNTIME | task_start_failures | integer | R | R |
RUNTIME | task_security_failures | integer | R | R |
RUNTIME | task_cancels | integer | R | R |
RUNTIME | active_tdms_requests | gauge | R | R |
RUNTIME | active_tdms_read_messages | gauge | R | R |
RUNTIME | active_tdms_write_messages | gauge | R | R |
RUNTIME | active_tdms_cancels | gauge | R | R |
RUNTIME | total_tdms_requests | integer | R | R |
RUNTIME | total_tdms_read_messages | integer | R | R |
RUNTIME | total_tdms_write_messages | integer | R | R |
RUNTIME | total_tdms_cancels | integer | R | R |
RUNTIME | total_dataset_hangups | integer | R | R |
RUNTIME | astlm_current++ | gauge | R | R |
RUNTIME | biolm_current++ | gauge | R | R |
RUNTIME | bytlm_current++ | gauge | R | R |
RUNTIME | diolm_current++ | gauge | R | R |
RUNTIME | enqlm_current++ | gauge | R | R |
RUNTIME | fillm_current++ | gauge | R | R |
RUNTIME | pgflquota_current++ | gauge | R | R |
RUNTIME | tqelm_current++ | gauge | R | R |
RUNTIME | wssize_current++ | gauge | R | R |
RUNTIME | channelcnt_current++ | gauge | R | R |
POOL | pool_coll_state | integer | R | R |
POOL | mss_process_total | integer | R | R |
POOL | mss_process_free | min gauge | R | R |
POOL | mss_process_largest | min gauge | R | R |
POOL | mss_process_failures | integer | R | R |
POOL | mss_process_garbage | integer | R | R |
POOL | ws_pool_total | integer | R | R |
POOL | ws_pool_used++ | gauge | R | R |
POOL | ws_pool_free | min gauge | R | R |
POOL | ws_pool_largest | min gauge | R | R |
POOL | ws_pool_failures | integer | R | R |
POOL | ws_pool_garbage | integer | R | R |
POOL | wsc_pool_total | integer | R | R |
POOL | wsc_pool_used++ | gauge | R | R |
POOL | wsc_pool_free | min gauge | R | R |
POOL | wsc_pool_largest | min gauge | R | R |
POOL | wsc_pool_failures | integer | R | R |
POOL | wsc_pool_garbage | integer | R | R |
POOL | tws_pool_total++ | integer | R | R |
POOL | tws_poolsize_total++ | integer | R | R |
POOL | tws_pool_large_used++ | gauge | R | R |
POOL | twsc_pool_total++ | integer | R | R |
POOL | twsc_poolsize_total++ | integer | R | R |
POOL | twsc_pool_large_used++ | gauge | R | R |
ERROR | err_coll_state++ | integer | R | R |
ERROR | err_count++ | integer | R | R |
ERROR | last_err_msg++ | string | R | R |
ERROR | time_of_last_error++ | time | R | R |

++Only valid for use with systems running ACMS Version 4.4 or higher.

Key to Access Modes

- R---Read Access
- RW---Read/Write Access
- Blank---Not available to the interface
- D---Field is dynamic

Previous | Next | Contents | Index