# BASEstartm Open DAS
for Modicon®
on Tru64tm UNIX®
Installation and User's Guide

Previous | Contents | Index

# Appendix B
DAS Error Messages

This appendix contains returned values and associated error messages specific to the DAS for Modicon programmable controllers.

> aborting, The connection to the device is being aborted,

Explanation: Error. The connection to the device is being aborted by an error or by user request. No more requests will be processed by the DAS until the connection is restored.
User Action: If the abort was caused by a device error, take action based on the error that occurred. If the abort was a result of a user request. Reconnect to the device before attempting further operations.

> addresstoolong, Variable address string too long,

Explanation: Error. A variable address that is being defined is too long. An address must be 30 characters of less in length.
User Action: Redefine the variable using a shorter address.

> apptypeunsupp, The given application type is not supported for this DAS,

Explanation: Error. The application type that was specified in the variable definition is not supported by this DAS.
User Action: Change the application type to a valid type for this DAS.

> devfailed, Failure in associated device,

Explanation: Error. The slave's programmable controller has failed to respond to a message or an abortive error occurred.
User Action: An irrecoverable error in the programmable controller occurred. Replace or repair the defective programmable controller.

> devilladdress, Illegal data address,

Explanation: Error. The address referenced in the data field is not an allowable address for the addressed slave location.
User Action: Check the model of the programmable controller and the documentation to determine a valid address for the programmable controller. Then modify the address to a valid address for this programmable controller.

> devillegalfnc, Illegal function,

Explanation: Error. The message function received is not an allowable action for the addressed slave. This error is most likely caused by setting an incorrect application profile, so a command is being sent to a wrong model programmable controller.
User Action: Check that the corrrect application profile is being used for this model of programmable controller.

> devillvalue, Illegal data value,

Explanation: Error. The value referenced in the data field is not an allowable value for this addressed slave location.
User Action: Check the model of the programmable controller and the documentation to determine a valid value for the programmable controller. Then modify the value to a valid value for this programmable controller.

> internalerror, Internal error,

Explanation: Error. An internal error occurred in the DAS.
User Action: Submit an SPR describing the circumstances that caused the error.

> invaddresstype, Invalid address type,

Explanation: Error. A variable that is being defined is defined as an illegal address type. The unconstrained address type is used for Modicon 584 and 984 extended files. The numeric address type is used for all other registers/coils.
User Action: Redefine the variable using the proper unconstrained or numeric address type.

> invalidaddress, The specified programmable controller address is not supported by this DAS,

Explanation: Error. An address was sent by a programmable controller but the address is not supported by this DAS.
User Action: Reprogram the programmable controller and specify a valid address for this DAS. Consult the DAS documentation to determine a valid address.

> invaliddrop, Invalid drop time specified in MODBUS_TELNET ODS entry,

Explanation: Error. The drop time specified is not a valid number. The drop time must be a number greater than 0.
User Action: Use ODS to enter a valid drop time attribute.

> invalidgroup, Variables in a group must all belong to the same address type,

Explanation: Error. A group read was attempted without all the variables in the group belonging to the same address reference type (coil, holding register, input, etc.).
User Action: Examine the members of the group to determine which variable does not belong, remove that variable from the list and retry the group read.

> invalidgroupmem, Variable XX in a group read for device XX does not belong,

Explanation: Error. A group read was attempted without all the variables in the group belonging to the same address reference type (coil, holding register, input, etc.).
User Action: Remove the incorrect variable from the list and retry the group read.

> invalidipaddress, Invalid IP_ADDRESS ODS attribute for the given line,

Explanation: Error. The IP_ADDRESS must be less than 50 characters in length.
User Action: Enter an IP address that is 50 characters or less in length.

> invalidmodem, Invalid modem attribute specified in the MODBUS_LINE ODS entry,

Explanation: Error. The modem attribute must be one of TRUE, ON, YES, 1 or FALSE, OFF, NO, 0.
User Action: Use ODS to enter a valid modem attribute.

> invalidparity, Invalid parity specified in the MODBUS_LINE ODS entry,

Explanation: Error. The parity defined must be either EVEN, ODD or NONE.
User Action: Use ODS to enter a valid parity (EVEN, ODD, NONE).

> invalidport, Invalid port name specified in the ODS entry,

Explanation: Error. Port names must be 10 characters or less.
User Action: Use ODS to enter a port name that is less than 10 characters.

> invalidportnum, Invalid PORT_NUMBER ODS attribute for the given line,

Explanation: Error. The PORT_NUMBER must be less than 10 characters in length.
User Action: Enter a PORT_NUMBER address that is 10 characters or less in length.

> invalidprobe, Invalid probe time specified in MODBUS_TELNET ODS entry,

Explanation: Error. The probe time specified is not a valid number. The probe time must be a number greater than 0.
User Action: Use ODS to enter a valid probe time attribute.

> invalidretries, Invalid retries number in the ODS entry,

Explanation: Error. The retries attribute must be between 0-20.
User Action: Use ODS to enter a retries number between 0-20.

> invalidslaveaddress, Invalid slave address number in the MODBUS_PATH ODS entry,

Explanation: Error. Modbus slave address numbers must be a number between 1-247.
User Action: Use ODS to enter a slave address number between 1-247.

> invalidspeed, Invalid speed (baud rate) specified in the MODBUS_LINE ODS entry,

Explanation: Error. Baud rates from 110 to 19200 are supported for the Modicon DAS.
User Action: Use ODS to enter a speed from 110 to 19200.

> invalidtimeout, Invalid timeout value in the ODS entry,

Explanation: Error. An invalid timeout value was entered for the timeout value in ODS. Timeouts must be between 2 and 10 seconds.
User Action: Use ODS to enter a timeout value between 2-10.

> invalidtrace, Invalid trace attribute specified in the MODBUS_LINE or MODBUS_PATH ODS entry,

Explanation: Error. The trace attribute must be one of TRUE, ON, YES, 1 or FALSE, OFF, NO, 0.
User Action: Use ODS to enter a valid trace attribute.

> invidnotfound, Matching invocation ID not found for VMD = XX, ID = !UW,

Explanation: Error. A response was received from the device, but no matching request was found either because the request timed out or because this is a duplicate response. A request and response have a unique invocation ID (transaction number) that allows the request and response to be matched up.
User Action: Increase the device timeout or analyze the network to determine where network delays could be ocurring and then take action to decrease network delays.

> ltnthreadexcep, Listen thread exception, Status = X,

Explanation: Error. The listen thread (listening for connection requests from TCP/IP clients) has received an unexpected exception (error).
User Action: Examine the Status for the thread and take based on the error found.

> mmsaddrtypeunsupp, The given MMS type is unsupported for the given address,

Explanation: Error. The MMS type is not supported for the variable address given.
User Action: Modify the MMS type to one supported for the given address or modify the address to one supported for the MMS type.

> mmstypeunsupp, The given MMS type is not supported for this DAS,

Explanation: Error. The MMS type that was specified in the variable definition is not supported by by this DAS.
User Action: Change the MMS type to a valid type for this DAS.

> modbuserror, A modbus error occurred,

Explanation: Error. A Modbus error occurred when reading or writing to the programmable controller.
User Action: Retry issuing the command.

> neterr, Modbus network error occurred,

Explanation: Error. A network error on the Modicon Modbus occurred.
User Action: Examine the network status in the returned IOSB to determine the specific network error that occurred and take action based on that error.

> noipaddress, No "IP_ADDRESS" ODS entry for the given line,

Explanation: Error. The DAS requires an IP_ADDRESS attribute defined in ODS. The IP_ADDRESS attribute is defined for the MODBUS_TELNET class within ODS.
User Action: Use the MODBUS_TELNET object class within ODS to define the IP_ADDRESS attribute for this line. Use a valid IP address for this attribute.

> nolicense, No software license.,

Explanation: Error. The Modicon DAS requires a software license.
User Action: Install the license PAK for the Modicon DAS.

> noline, No "/LINE=" ODS entry for the given application simple name,

Explanation: Error. The Modicon DAS requires a /LINE= attribute defined for the ODS entry corresponding to the application simple name entry for the remote VMD. The /LINE= attribute is defined for MODBUS_PATH and MODPLUS_SLAVE_PATH object classes within ODS.
User Action: Use the MODBUS_PATH object class (for Modbus) or MODPLUS_SLAVE_PATH object class (for Modbus Plus) within ODS to define the application simple name for this VMD. Use a valid line name when defining the /LINE= attribute.

> nomodem, No "MODEM" ODS entry for the given line,

Explanation: Error. The Modicon DAS requires a MODEM attribute defined in ODS. The MODEM attribute is defined for the MODBUS_LINE object class within ODS.
User Action: Use the MODBUS_LINE object class within ODS to define the MODEM attribute for this line. Modem control is either enabled (TRUE, ON, YES, 1) or disabled (FALSE, OFF, NO, 0).

> noparity, No "PARITY" ODS entry for the given line,

Explanation: Error. The Modicon DAS requires a PARITY attribute defined in ODS. The PARITY attribute is defined for the MODBUS_LINE object class within ODS.
User Action: Use the MODBUS_LINE object class within ODS to define the PARITY attribute for this line. Use a valid parity (EVEN, NONE) when defining the PARITY attribute.

> noport, No "PORT" ODS entry for the given line,

Explanation: Error. The Modicon DAS requires a PORT attribute defined in ODS. The PORT attribute is defined for the MODBUS_LINE object class within ODS.
User Action: Use the MODBUS_LINE object class within ODS to define the PORT attribute for this line. Use a valid port name when defining the PORT attribute.

> noportnumber, No "PORT_NUMBER" ODS entry for the given line,

Explanation: Error. The DAS requires a PORT_NUMBER attribute defined in ODS. The PORT_NUMBER attribute is defined for the MODBUS_TELNET class within ODS.
User Action: Use the MODBUS_TELNET object class within ODS to define the PORT_NUMBER attribute for this line. Use a valid IP port number for this attribute.

> noretries, No "RETRIES" ODS entry for the given line,

Explanation: Error. The Modicon DAS requires a RETRIES attribute defined in ODS. The RETRIES attribute is defined for the MODBUS_LINE object class within ODS.
User Action: Use the MODBUS_LINE object class within ODS to define the RETRIES attribute for this line. Use a valid number when defining the RETRIES attribute.

> noslaveaddress, No "SLAVE_ADDRESS" ODS entry for the given application simple name,

Explanation: Error. The Modicon DAS requires a SLAVE_ADDRESS attribute defined for the ODS entry corresponding to the application simple name entry for the remote VMD. The SLAVE_ADDRESS attribute is defined for MODBUS_PATH object class within ODS.
User Action: Use the MODBUS_PATH object class within ODS to define the application simple name for this VMD. Use a valid Modbus slave address number when defining the SLAVE_ADDRESS attribute.

> nospeed, No "SPEED" ODS entry for the given line,

Explanation: Error. The Modicon DAS requires a SPEED attribute defined in ODS. The SPEED attribute is defined for the MODBUS_LINE object class within ODS.
User Action: Use the DH_LINE object class within ODS to define the SPEED attribute for this line. Use a valid baud rate when defining the SPEED attribute.

> notimeout, No "TIMEOUT" ODS entry for the given line,

Explanation: Error. The Modicon DAS requires a TIMEOUT attribute defined in ODS. The TIMEOUT attribute is defined for the MODBUS_LINE object class within ODS.
User Action: Use the MODBUS_LINE object class within ODS to define the TIMEOUT attribute for this line. Use a valid number when defining the TIMEOUT attribute.

> notrace, No "TRACE" ODS entry,

Explanation: Error. The Modicon DAS requires a TRACE attribute defined in ODS. The TRACE attribute is defined for the MODBUS_PATH, MODBUS_LINE, MODPLUS_LINE, MODPLUS_SLAVE_PATH and MODPLUS_NODE_PATH object classes within ODS.
User Action: Use the appropriate object class within ODS to define the TRACE attribute for this line. Trace is either enabled (TRUE, ON, YES, 1) or disabled (FALSE, OFF, NO, 0).

> parsefailed, The parsing of a variable address failed,

Explanation: Error. When defining a variable, the parsing of the address failed. Either the syntax or the value of the address is incorrect.
User Action: Consult the user documentation to determine a valid address for the variable being defined and redefine the variable using the correct syntax.

> rcvthreadexcep, Receive thread exception for device XX, Status = X,

Explanation: Error. The receiver thread (waiting for input in response to a request for data) has received an unexpected exception (error).
User Action: Examine the Status for the thread and take based on the error found.

> reqpending, Conclude rejected because of a pending read/write request,

Explanation: Error. The conclude request was rejected because either a read or a write request was currently pending.
User Action: Either abort the connection or wait for the current request(s) to complete before retrying the conclude.

> retriesexceeded, The retry count was exceeded,

Explanation: Error. When trying to communicate to the device, the retry count was exceeded. The retry being exceeded means that the message being sent to the device was garbled during transmission and did not match the checksum.
User Action: Check cabling to ensure there are no shorts or breaks and is properly grounded. Make sure the cable is routed such that it does not pass close to electrical interference such as transformers and high power cables.

> timeout, Modbus timeout when reading from the programmable controller,

Explanation: Error. The programmable controller did not respond when attempting to read a response from the programmable controller. The response could be part of a read or a write operation.
User Action: Check all cabling to make sure that it is properly shielded, grounded and seated. Verify that the communication parameters are set up properly on both programmable controller and the host. Verify that the correct slave address has been selected on the programmable controller and on the host.

> tmrthreadexcep, Timer thread exception for device XX, Status = X,

Explanation: Error. The timer thread (timing out responses to requests for data) has received an unexpected exception (error).
User Action: Examine the Status for the thread and take based on the error found.

> unsupported, The requested function is not supported by the DAS,

Explanation: Error. An attempt was made to execute a OMNI function that is not supported by this DAS.
User Action: Consult the user documentation to determine which functions are supported by the DAS and limit the OMNI functions used to those supported by the DAS.

> writenotsupport, Writes are not supported for the specified address,

Explanation: Error. An attempt was made to write to an address that the Modbus protocol does not allow write access to.
User Action: Consult the documentation to determine addresses that can be written to and change the address of the variable or only perform reads when using this variable.

Index | Contents