Document revision date: 30 March 2001

## OpenVMS System Management Utilities Reference Manual

Previous | Contents | Index

    **************************** ENTRY       6. ****************************
    ERROR SEQUENCE 3.                                 LOGGED ON SID 03003700

    MACHINE CHECK,  6-MAR-2000 10:11:34.70
                    KA730 REV# 0. MIC# 55.

          EXCEPTION PC    80038DC0

          ERROR PSL       01C00000
                                          INTERRUPT PRIORITY LEVEL = 00.
                                          PREVIOUS MODE = USER
                                          CURRENT MODE  = EXECUTIVE

          SUMMARY CODE    00000007
                                          UNCORRECTABLE ECC ERROR
          1ST PARAMETER   00166200
                                          PAGE #2865. IN ERROR
    **************************** ENTRY      60. ****************************
    ERROR SEQUENCE 4872.                              LOGGED ON SID 02006148

    MACHINE CHECK, 6-MAR-2000 03:50:08.28
                   KA750 REV# 72. MIC# 97.

          EXCEPTION PC    80006173

          ERROR PSL       00C80009
                                          C-BIT
                                          N-BIT
                                          INTERRUPT PRIORITY LEVEL = 08.
                                          PREVIOUS MODE = USER
                                          CURRENT MODE  = KERNEL
          SUMMARY CODE    00000002
                                          TRANSLATION BUFFER OR BUS ERROR
          VA LAST REF     800A079E
          PC AT ERROR     80006178
          MDR             8009F38C
          SMR             00000008
                                          CPU MODE = KERNEL
                                          VIRTUAL
                                          READ
          RLTO            00000000
          TBER            00000007
                                          TB G0 DATA ERROR
                                          TB G1 DATA ERROR
                                          TB G0 TAG ERROR
          CAER            00000000
          BER             00000000
          MCESR           00000004
                                          OPERAND REFERENCE
                                          TB PARITY ERROR
    **************************** ENTRY      84. ****************************
    ERROR SEQUENCE 4949.                              LOGGED ON SID 01388525

    MACHINE CHECK,  6-MAR-2000 15:09:11.31
                    KA780 REV# 7. SERIAL# 1317.

          EXCEPTION PC    00004890

          ERROR PSL       03C00000
                                          INTERRUPT PRIORITY LEVEL = 00.
                                          PREVIOUS MODE = USER
                                          CURRENT MODE  = USER

          SUMMARY CODE    00000000
                                          CP READ TIMEOUT
                                          - OR ERROR CONFIRMATION FAULT
          CES             00010084
                                          SUPERVISOR AST PENDING
                                          ALU C31
                                          NESTED ERROR
          MICRO PC        00000200
          VA/VIBA         7FF735D4
          D REGISTER      FFFFC284
          TBER0           0000DC81
                                          ENABLE MEMORY MANAGEMENT
                                          TB HIT GROUP 1
                                          MICRO CODE "MCT" FIELD = 07
                                          MICRO CODE "ADS"
                                          MICRO CODE "FS"
          TBER1           00000040
                                          LAST TB WRITE PULSE TO GROUP 1
          SBITA           E00B83F5
                                          TIMEOUT CONSOLE ADDR = 002E0FD4
                                          PROTECTION CHECKED REFERENCE
                                          TIMEOUT REFERENCE IN USER MODE
          CACHE PE REG    00004000
                                          CP ERROR
          SBIER           00001802
                                          SBI NOT BUSY
                                          WAITING FOR READ DATA TIMEOUT
                                          CPU TIMEOUT

     **************************** ENTRY      82. ****************************
     ERROR SEQUENCE 1077.                              LOGGED ON SID 04FFFFFF
     MACHINE CHECK  30-MAR-2000 20:55:17.41
                    KA86  REV# 255.  SERIAL# 4095.  MFG PLANT 7.
           EHMSTS          40000802
                                           VMS ERROR CODE = EBOX
                                           MICRO TRAP VECTOR = 08 (X)
                                           EHM ENTERED
           EVMQSAV         00000004
                                           VIRTUAL ADDRESS FOR EBOX PORT
                                           _ REQUESTS
           EBCS            00000800
                                           ECS PARITY ERROR
           EDPSR           00000000
           CSLINT          04183D1F
                                           C BUS ADDRESS = 1F (X)
                                           C BUS DATA = 3D (X)
                                           INTERRUPT PRIORITY REQUEST = 8.
                                           INTERNAL SOURCE
                                           I/O ADAPTER = 0.
                                           INTERVAL TIMER
           IBESR           00004000
                                           UOP SEL = IBOX REGISTER SELECT
                                           UTPR <2:0> = EBOX PORT
                                           ENABLE ETRAP
           EBXWD1          00000004
                                           TOP OF "SP STACK"
                                           _ CONTENT IS ONE OF THE LAST
                                           _ LONGWORDS WRITTEN TO MBOX
           EBXWD2          7FF593D0
                                           TOP OF "SP STACK" MINUS ONE
                                           _ CONTENT IS ONE OF THE LAST
                                           _ LONGWORDS WRITTEN TO MBOX
           VASAV           7FF593F8
                                           VIRTUAL ADDRESS FOR OP FETCH
                                           _ PORT REQUEST ADDRESS
                                           _ CALCULATION FOR OPERAND
                                           _ PRE-FETCH AND RESULT DELIVERY
           VIBASAV         0000E7FF
                                           VIRTUAL ADDRESS OF NEXT IBUF
                                           _ PORT REQUEST TO FILL IBUFFER
           ESASAV          0000E7F2
                                           PC OF INSTRUCTION DURING EBOX
                                           _ EXECUTION AND RESULT STORAGE
           ISASAV          0000E7F2
                                           PC OF INSTRUCTION WHICH VA
                                           _ CALCULATION UNIT IS DOING ADDRESS
                                           _ CALCULATION OR OPERAND PRE-FETCH
                                           _ OR IS PASSING OPERAND DATA
           CPC             0000E7F4
                                           PC OF INSTRUCTION IN
                                           _ DECODE UNIT
           MSTAT1          84006004
                                           C0 TAG MISS
                                           BLOCK HIT
                                           ABUS ADAPTER = 0.
                                           WORD COUNT = 0.
                                           CYCLE TYPE = READ REGISTER
                                           DEST CP = EBOX
           MSTAT2          00004F00
                                           DIAGNOSTIC STATUS FROM SBIA
                                           _    RD COM/MSK <3:0> = F (X)
                                           _    RD DAT L/S <1:0> = 0 (X)
                                           _    ABUS BAD DATA CODE
                                           PAMM DATA = ARRAY #0.,SLOT #1.
           MDECC           00066200
                                           (* DATA NOT VALID *)
           MERG            04000100
                                           MEMORY MANAGEMENT ENABLE
           CSHCTL          00000003
                                           CACHE 0 ENABLE
                                           CACHE 1 ENABLE
           MEAR            0000007C
                                           PHYSICAL ADDRESS IN PA LATCH
                                           AT TIME OF ERROR = 0000007C
           MEDR            0000001F
                                           DATA WORD USED DURING ERROR
           FBXERR          FFFFFFFF
                                           (* DATA NOT VALID *)
           CSES            1BD73E01
                                           CS CODE = EBOX CONTROL STORE PARITY ERROR
                                           CS SYNDROME = 3E (X)
                                           CS ADDRESS = 1BD7 (X)
           ERROR PC        0000E7F2

           ERROR PSL       03C00004
                                           Z-BIT
                                           INTERRUPT PRIORITY LEVEL = 00.
                                           PREVIOUS MODE = USER
                                           CURRENT MODE  = USER
           IOA ES          00000000
                                           (* DATA NOT VALID *)

    AN/ER/INC=MACH ERR:ERRLOG.SYS_31MAR2000/ENT=S=82/OUT=DP.

Memory Error Entries Example

Memory error log entries consist of two types: fatal and nonfatal. A nonfatal memory error indicates that a single bit has failed within a memory location, and that the ECC (error code correctable) was able to compensate for the error and correct the data. A fatal error indicates that multiple bits were erroneous, and that the ECC could not correct the data.

Both the fatal and nonfatal memory entries are similar in their format. The memory error log reports can be divided into two logical areas of information. The first section of a memory error log report is the identification area. The second section contains memory controller-specific information. This data represents the information contained within the memory controller registers at the time of the memory error. Bit-to-text translation of the registers is performed and then listed on the right side of the report.

    **************************** ENTRY       7. ****************************
    ERROR SEQUENCE 4.                                 LOGGED ON SID 03003700

    MEMORY ERROR,  6-MAR-2000 10:11:34.70
                   KA730 REV# 0. MIC# 55.

          CSR0            00166200
                                          ERROR SYNDROME = 7F
                                          CORRECTED ERROR, BIT #31.
                                          ARRAY #1. IN ERROR
          CSR1            18000000
                                          MEMORY MAPPING ENABLE
                                          ENABLE "CRD" REPORTING
          CSR2            8100000F
                                          MEMORY SIZE = 2048.K
                                          64K RAMS PRESENT

    **************************** ENTRY      91. ****************************
    ERROR SEQUENCE 342.                               LOGGED ON SID 0138207A

    FATAL MEMORY ERROR, 4-MAR-00 08:16:45.20
                        KA780 REV# 7. SERIAL# 122.

    CONTROLLER AT TR #5.

          PRTCFNG         00000040
                                          ADAPTER IS MULTI-PORT MEMORY
                                          PORT NUMBER = 0.
          PRTCR           00000003
                                          MASTER INTERRUPT ENABLE
                                          PORT INTERFACE INTERRUPT ENABLE
                                          RAM COUNT 0.
          PCSR            07870003
                                          ERROR INTERRUPT ENABLE
          IVDTCR          01870001
                                          INVALIDATE CACHE DEVICE ID = 0.
                                          8. ARRAY BOARD(S) PRESENT
                                          MEMORY BASE ADDRESS = 6144.K
          AER             16A70005
                                          ERROR SYNDROME = 05
                                          RDS ERROR
                                          ARRAY #6. IN ERROR
                                          ARRAY BANK #1. IN ERROR
                                          ERROR LOG REQUEST
          CSR0            0000C2C8
                                          MEMORY CONTAINS VALID DATA
                                          PORT #2. POWERED DOWN
                                          PORT #3. POWERED DOWN
                                          ERROR INTERRUPT FROM PORT #1.
                                          PORT #2. OFFLINE
                                          PORT #3. OFFLINE
          CSR1            0000380A
                                          PORT #0. CONNECTED TO AN SBI
                                          PORT #1. CONNECTED TO AN SBI
                                          PORT #2. NOT PRESENT
                                          PORT #3. NOT PRESENT
                                          INVALIDATION MAP PRESENT
                                          PORT #0. INVALIDATION ACK RECEIVED
                                          PORT #1. INVALIDATION ACK RECEIVED
          MAT             0000C000

Nonfatal and User Bugchecks Entry Example

The following example shows a fatal bugcheck. Nonfatal and user bugcheck reports have the same format. These reports consist of three sections: identification, bugcheck reason and process information, and system register information.

     Error Log Report Generator                                         Version 7.3

     ******************************* ENTRY      25. *******************************
     ERROR SEQUENCE 15.                              LOGGED ON:  CPU_TYPE 00000002
     DATE/TIME 22-JUL-2000 13:43:48.96                           SYS_TYPE 00000003
     SYSTEM UPTIME: 90 DAYS 00:07:26
     SCS NODE: LSR3                                                OpenVMS V7.3

     FATAL BUGCHECK SYS_TYPE = 03

     OPERATOR, Operator requested system shutdown

           PROCESS NAME    Aut
           PROCESS ID      00010004

           ERROR PC        00000000 000304A0

        Process Status = 08000000 00001F03, SW = 03, Previous Mode = USER
        System State = 00, Current Mode = KERNEL
        VMM = 00 IPL = 31, SP Alignment = 8
     STACK POINTERS

     KSP 00000000 7FF95F08  ESP 00000000 7FF9A000  SSP 00000000 7FFA04C0
     USP 00000000 7FE63B80

     GENERAL REGISTERS

     R0  00000000 00000001  R1  00000000 00000000  R2  FFFFFFFF 805ED100
     R3  00000000 00000001  R4  00000000 00000001  R5  00000000 00000001
     R6  00000000 00000000  R7  00000000 00000000  R8  00000000 7FFA05F8
     R9  00000000 7FFA0800  R10 00000000 00000000  R11 00000000 7FFBE3E0
     R12 00000000 00000004  R13 00000000 00010100  R14 00000000 02080061
     R15 FFFFFFFF 80403C30  R16 00000000 00000474  R17 00000000 00004000
     R18 00000000 00000000  R19 00000000 00000000  R20 FFFFFFFF 805C04B6
     R21 00000000 00800000  R22 FFFFFFFF 804308E8  R23 88000000 E4000003
     R24 00000000 00000000  R25 00000000 00000001  R26 00000000 00000002
     R27 00000000 00000002  R28 00000000 00030440  FP  00000000 7FF95F10
     SP  00000000 7FF95F08  PC  00000000 000304A0  PS  08000000 00001F03
     SYSTEM REGISTERS

           PTBR            00000000 000005D3
                                           Page Table Base Register
           PCBB            00000000 00B98080
                                           Privileged Context Block Base
           PRBR            FFFFFFFF 805C0000
                                           Processor Base Register
           SCBB            00000002 00000000
                                           System Control Block Base
           SISR            00000000 0000017B
                                           Software Interrupt Summary Register
           ASN             00000000 00000000
                                           Address Space Number
           ASTSR_ASTEN     00000000 0000003F
                                           AST Summary/AST Enable
           AT              00000000 0000000F
                                           Absolute Time

Unknown Entries Examples

The following examples are sample reports for error log entries of unknown type. Each report has an identification section and an error log record section. The error log record section contains two types of records: interpretable and noninterpretable. If ERROR LOG can interpret the fields of the record, the utility gives the name of the field, its contents, and interprets what the field is. If the utility cannot interpret the fields of a record, it gives the longword value of the field and its contents in hexadecimal format.

    **************************** ENTRY      95. ****************************
    ERROR SEQUENCE 2.                                 LOGGED ON SID 03003600

    "UNKNOWN DEVICE" ENTRY,  4-MAR-00 10:12:12.44
                             KA730 REV# 0. MIC# 54.

    ERROR LOG RECORD

          ERF$L_SID       03003600
                                          SYSTEM ID REGISTER
          ERL$W_ENTRY         0062
                                          ERROR ENTRY TYPE
          EXE$GQ_SYSTIME  C9764980
                          008C2F30        64 BIT TIME WHEN ERROR LOGGED
          ERL$GL_SEQUENCE     0002
                                          UNIQUE ERROR SEQUENCE = 2.
          UCB$W_STS           0110
                                          DEVICE STATUS
          UCB$B_DEVCLASS        42
                                          DEVICE CLASS = 66.
          UCB$B_DEVTYPE         42
                                          DEVICE TYPE = 66.
          UCB$W_UNIT          0000
                                          PHYSICAL UNIT NUMBER = 0.
          UCB$W_ERRCNT        0001
                                          UNIT ERROR COUNT = 1.
          UCB$L_OPCNT     00000001
                                          UNIT OPERATION COUNT = 1.
          ORB$L_OWNER     00010004
                                          OWNER UIC = [001,004]
          UCB$L_DEVCHAR   0C440007
                                          DEVICE CHARACTERISTICS
          UCB$B_SLAVE           00
                                          DEVICE SLAVE CONTROLLER = 0.
          DDB$T_NAME      41515403
                          00000000
                          00000000
                          00000000
                                          /.TQA............/
          LONGWORD 1.     00000008

          LONGWORD 2.     00000007

          LONGWORD 3.     00000502

          LONGWORD 4.     04000000

          LONGWORD 5.     00010000

          LONGWORD 6.     00000000

          LONGWORD 7.     00000080

          LONGWORD 8.     00000000

          LONGWORD 9.     00000000

    **************************** ENTRY     161. ****************************
    ERROR SEQUENCE 213.                               LOGGED ON SID 070001FF

    "UNKNOWN ENTRY", 4-MAR-00 11:35:15.73
                     UVAX1 REV# 255. MIC# 1.

    ERROR LOG RECORD

          ERF$L_SID       070001FF
                                          SYSTEM ID REGISTER
          ERL$W_ENTRY         0008
                                          ERROR ENTRY TYPE
          EXE$GQ_SYSTIME  89953F20
                          008C3E2A        64 BIT TIME WHEN ERROR LOGGED

          ERL$GL_SEQUENCE     00D5
                                          UNIQUE ERROR SEQUENCE = 213.
          LONGWORD 1.     00000001
                                          /..../
          LONGWORD 2.     00410001
                                          /..A./

Example of a Brief Report

The following example shows a report generated with the /BRIEF qualifier.

     Error Log Report Generator                                   Version 7.3

     **************************** ENTRY       1. ****************************
     ERROR SEQUENCE 11.                          LOGGED ON:      SID 08000000
     DATA/TIME 18-JUL-2000 22:53:41.57                      SYS_TYPE 00000000

     DEVICE ERROR  KA630

     RD32 SUB-SYSTEM, UNIT _RICHIE$DUA0:

           DMA ADDRESS       000000

           DSECT      CHEAD      DHEAD      CCYL       DCYL       SCNT
           06         14         14         9C         9C         01

           RTCNT      CSTAT      MODE       DSTAT      TERM       ISTAT
           F0         08         C0         B2         BD         28

           CMD
           56

Previous | Next | Contents | Index

| privacy and legal statement |
6048PRO_027.HTML