# Compaq TCP/IP Services for OpenVMS
Management Command Reference

## Index

Previous | Contents

Master Alphabetic Index
A | B | C | D | E | F | G | H | I | L | M | N | O | P | Q | R | S | T | U | V | Y | Z

A
Account
OpenVMS user
creating #1
creating #2
deleting
displaying
ADD EXPORT command
ADD PROXY command
Address
0.0.0.0
displaying device sockets
host-name-to-address lookups
See Lookups
IP
defining #1
defining #2
displaying
mapping IP to Ethernet/FDDI #1
mapping IP to Ethernet/FDDI #2
Address Resolution Protocol
See ARP
Alias
for defining a cluster #1
for defining a cluster #2
ANALYZE CONTAINER command
ANALYZE MAIL command
ANALYZE SERVICE command
Anonymous FTP
See FTP
"ANY host"
displaying device sockets
Applications
customer-developed
ADD PROXY command
registering clients
ARP
SET ARP command
SHOW ARP command
Authentication
ADD PROXY command #1
ADD PROXY command #2
CREATE PROXY command
REMOVE PROXY command
AUTHORIZE command (DCL)
Auxiliary server
messages from
multithreading
restarting the NFS server
uses the BIND Resolver
uses the BIND resolver
B
Berkeley Internet Name Domain
See BIND
BG device driver
See Internet interface
BIND command
See MAP command
BIND database
SHOW HOST command
BIND resolver
configuration
displaying
configuring #1
configuring #2
defining the domain #1
defining the domain #2
deleting the domain #1
deleting the domain #2
disabling
displaying the configuration
enabling
SHOW HOST command
BIND server
configuration
displaying
configuring
CONVERT/CONFIGURATION BIND command
CONVERT/UNIX BIND command
disabling
monitoring
reloading
SET CONFIGURATION BIND command
Binding
See MAP command
Booting, remote
See BOOTP
BOOTP
Database
CONVERT/VMS BOOTP command
creating
displaying
disabling
enabling at system startup
monitoring
SET BOOTP command
SHOW BOOTP command
BOOTP database
adding entries to
Bootstrap Protocol
See BOOTP
Buffers
displaying
SHOW COMMUNICATION command
setting
C
Clients
adding, to BOOTP database
Cluster load balancing
See BIND Server
Commands
DCL
AUTHORIZE
SHOW DEVICE
displaying information
guidelines for entering
program design
configuration commands
CONVERT commands
creating database files
managing NFS
starting software
stopping software
validating databases
See individual commands
UNIX
`/etc/mount`
using
how to enter
Communication proxies
Communication proxy
APPLICATION_PROXY flag
Configuration
BIND Server
creating
creating
Database
BIND Server entries
creating
creating
displaying
lower-layer software entries
creating
lower-level protocol entries
creating
Name Server entries
creating
SMTP entries
creating
SNMP entries
creating
displaying
Name Server
creating
permanent
See also individual SET CONFIGURATION commands
SMTP
creating
SNMP
creating
Configuration protocol
displaying
Configuring protocols
Controller
Ethernet
identifying
identifying with SET INTERFACE command
FDDI
identifying
identifying with SET INTERFACE command
SLIP
identifying
identifying with SET INTERFACE command
CONVERT/CONFIGURATION BIND command
CONVERT/UNIX BIND command
CONVERT/UNIX HOST command
CONVERT/UNIX NETWORK command
CONVERT/VMS BOOTP command
CONVERT/VMS HOST command
CONVERT/VMS NETWORK command
CONVERT/VMS PROXY command
Converting
BIND 4 configuration to BIND 8
CREATE BOOTP command
CREATE CONFIGURATION command
CREATE CONTAINER command
CREATE DIRECTORY command
CREATE EXPORT command
CREATE HOST
CREATE NETWORK
CREATE PROXY command
CREATE ROUTE command
Customer-developed applications
ADD PROXY command
registering clients
D
Data link
See Internet interface
Data link interface
See Internet interface
Database
BIND
SHOW HOST command
BIND Server
CONVERT/UNIX BIND command
BOOTP
adding entries to
CONVERT/VMS BOOTP command
creating
displaying
Configuration
BIND Server entries
creating
creating
displaying
lower-layer software entries
creating
lower-level protocol entries
creating
Name Server entries
creating
SMTP entries
creating
SNMP entries
creating
Export
adding directory names in the Export Database
CREATE EXPORT command
deleting directory names from the Export Database
SHOW EXPORT command
Hosts
cluster alias
specifying #1
specifying #2
CONVERT/UNIX HOST command
CONVERT/VMS HOST command
SHOW HOST command
MX
SET MX_RECORD command
SHOW MX_RECORDS command
network
CONVERT/UNIX NETWORK
CONVERT/VMS NETWORK
networks
adding entries
displaying entries
Proxy
adding entries to #1
adding entries to #2
creating
deleting entries from
SHOW PROXY command
Routes
CREATE ROUTE command
SET MX_RECORD command
SHOW MX_RECORDS command
Services
ANALYZE SERVICE command
SET SERVICE command
SHOW SERVICE command
SHOW MX_RECORDS command
DCL
AUTHORIZE command
SHOW DEVICE command
Defense Data Network
See DDN
DEFINE COMMUNICATION_CONTROLLER command
Defining
cluster alias #1
cluster alias #2
interface identifier #1
interface identifier #2
DELETE COMMUNICATION_CONTROLLER command
DELETE CONTAINER command
Device driver
internet #1
internet #2
internet #3
Device socket
SHOW DEVICE_SOCKET command
DIRECTORY command
DISABLE SERVICE command
DISCONNECT DEVICE_SOCKET command
DISMOUNT command
DNFSn:
See NFS
DNS
See also BIND
Domain
SET CONFIGURATION BIND command
Domain Name Service
See BIND
See DNS
Downline loading
See Downloading
Dynamic routing
See Routing

Previous | Next | Contents | Index