Document revision date: 30 March 2001

## OpenVMS System Services Reference Manual

Previous | Contents | Index

Appendix A
Appendix A | Obsolete Services
Index
| Index
Tables
SYS-1 | Abort Reason Codes
SYS-2 | Description of$AUDIT_EVENT Types and Subtypes
SYS-3 | Services That Do Not Accept Shared Page Table Regions
SYS-4 | Sample Returned Values from$CREATE_REGION_64
SYS-5 | User Privileges
SYS-6 | Required and Optional Arguments for the$CRMPSC Service
SYS-7 | Shared Page Tables
SYS-8 | $DNS Item Codes and Their Data Types
SYS-9 | Compatibility of Lock Modes
SYS-10 | Legal QUECVT Conversions
SYS-11 | $FAO Directives
SYS-12 | $FAO Output Field Lengths and Fill Characters
SYS-13 | Attributes of an Identifier
SYS-14 | Region Summary Buffer Format
SYS-15 | Format of the IEEE Floating-Point Control Register (Alpha Only)
SYS-16 | Flags Used with$PROCESS_SCAN
SYS-17 | Valid Function Codes
SYS-18 | Item Code Summary
SYS-19 | CPU Time Limit Decision Table
SYS-20 | Working Set Decision Table

Previous | Next | Contents | Index

| privacy and legal statement |
4527PRO_CONTENTS_001.HTML