# BASEstartm Classic DAS
for OMNItm Software
Installation and User's Guide

## Index

Previous | Contents

Master Alphabetic Index
A | C | D | E | F | G | H | I | L | M | N | O | P | R | S | T | U | W

A
Accessing DAS functions
Additional software
required
Application Simple Name
Automatic data collection
pollsets
unsolicited data
C
Configuration
NCL
ODS
Configuration file
device records
Configuration File
editing
Configuration file
path records
type records
Configuring parameters
ILAN$MAX_SPT_REQUESTS
D
DAS
See Device Access Software
Data types
Defining DAS Constants
Device Access Software
accessing functions
defining constants
description of
functions #1
functions #2
functions #3
installation of
installation requirements
MMS functions
overview
SINEC-AP functions
SINEC-H1 functions
SINEC-S7 functions
supported devices
supported functions #1
supported functions #2
using
Device records
Devices
communications
Directory function
Disk space required
Download function
E
Exchange message function #1
Exchange message function #2
Exchange message indication
automatic reply
F
Files
created during installation
Functions
device specific #1
device specific #2
directory
download
exchange message #1
exchange message #2
read data
read message #1
read message #2
read status
start
stop
upload
write data
write message #1
write message #2
G
Group reads
H
Hardware
required
I
Information report
Installation
files created
messages
post installation tasks
procedure
requirements
L
Local VMD
M
Message exchange indication
manual reply
Messages
error and return values
installation
logged
N
NCL
configuration
null internet
RFC-1006
transport templates
O
ODS
attributes
configuration
OSI Tracing
P
Path records
Pollsets
scattered reads
Post installation tasks
Problem reporting
Product failure
Protocol Profile
R
Read data function
Read indication
automatic reply
manual reply
Read message function #1
Read message function #2
Read status function
Remote VMD
S
Scattered read
pollsets
Shop floor equipment
setting up
Sinec-AP
message support
Sinec-AP and SINEC-H1
specific functions
Software
required
Specific functions
device
SPT block usage
Start function
Stop function
SYSGEN parameters
T
Tracing
OSI messages
Tuning ILAN$DEVSRV
Type records
U
Unsolicited data
information report
message exchange indication
read indication
write indication
Upload function
W
Write data function
Write indication
Write message function #1
Write message function #2