Document revision date: 30 March 2001

## OpenVMS Alpha System Analysis Tools Manual

Previous | Contents | Index

## SHOW LAN

> Displays information contained in various local area network (LAN) data structures.

### Format

> SHOW LAN [/qualifier[,...]]

### Parameters

> None.

### Qualifiers

> #### /CLIENT=name

> Specifies that information be displayed for the specified client. Valid client designators are SCA, DECNET, LAT, MOPRC, TCPIP, DIAG, ELN, BIOS, LAST, USER, ARP, MOPDL, LOOP, BRIDGE, DNAME, ENCRY, DTIME, and LTM. The /CLIENT, /DEVICE, and /UNIT qualifiers are synonymous and mutually exclusive.

> #### /CLUEXIT

> Specifies that cluster protocol information be displayed.

> #### /COUNTERS

> Specifies that the LAN station block (LSB) and unit control block (UCB) counters be displayed.

> #### /CSMACD

> Specifies that Carrier Sense Multiple Access with Collision Detect (CSMA/CD) information for the LAN be displayed. By default, both CSMA/CD and Fiber Distributed Data Interface (FDDI) information is displayed.

> #### /DEVICE=name

> Specifies that information be displayed for the specified device, unit, or client. For each LAN adapter on the system there is one device and multiple users of that device called units or clients. Device designators are specified in the format XXdn, where XX is the type of device, d is the device letter, and n is the unit number. The device letter and unit number are optional. The first unit, which is always present, is the template unit. These are specified as indicated in this example, for a DEMNA which is called EX:

> > /DEVICE=EX---display all EX devices on the system
> > /DEVICE=EXA---display the first EX device only
> > /DEVICE=EXA0---display the first EXA unit
> > /DEVICE=SCA---display SCA unit
> > /DEVICE=LAT---display LAT units

> Valid client names are listed in the /CLIENT=name qualifier. The /CLIENT, /DEVICE, and /UNIT qualifiers are synonymous and mutually exclusive.

> #### /ELAN

> Specifies information from an Emulated LAN (ELAN) that runs over an asynchronous transfer mode (ATM) network. The /ELAN qualifier displays the LAN Station Block (LSB) address, device state, and the LSB fields pertinent to an ELAN for both the parent ATM device and the ELAN pseudo-device drivers. It also specifies the name, description, parent device, state, and LAN emulation client (LEC) attributes of the ELAN.

> The qualifier /ELAN used with the device qualifier (/LAN/device=ELA) will only display information for the specified device or pseudo-device.

> #### /ERRORS

> Specifies that the LSB and UCB error counters be displayed.

> #### /FDDI

> Specifies that Fiber Distributed Data Interface (FDDI) information for the LAN be displayed. By default, both CSMA/CD and FDDI information is displayed.

> #### /FULL

> Specifies that all information from the LAN, LSB, and UCB data structures be displayed.

> #### /ICOUNTERS

> Specifies internal counters of the drivers by displaying the internal counters. If the /ICOUNTERS qualifier is used with the /DEVICE qualifier, the /ICOUNTERS specifies the internal counters of a specific driver.

> #### /QUEUE

> Specifies a listing of all queues, whether their status is valid or invalid, and all elements of the queues. If the /QUEUE qualifier is used with the /DEVICE qualifier, the /QUEUE specifies a specific queue.

> #### /SUMMARY

> Specifies that only a summary of LAN information (a list of flags, LSBs, UCBs, and base addresses) be printed. This is the default.

> #### /TIMESTAMPS

> Specifies that time information (such as start and stop times and error times) from the device and unit data structures be printed. SDA displays the data in chronological order.

> #### /UNIT=name

> Specifies that information be displayed for the specified unit. See the descriptions for /CLIENT=name and /DEVICE=name qualifiers.

> #### /VCI

> Specifies that information be displayed for the VMS Communication Interface Block (VCIB) for each LAN device with an active VCI user. If you use the /VCI qualifier with the /DEVICE qualifier, the VCIB is only displayed for the specified device.

### Description

> The SHOW LAN command displays information contained in various local area network (LAN) data structures. By default, or when the /SUMMARY qualifier is specified, SHOW LAN displays a list of flags, LSBs, UCBs, and base addresses. When the /FULL qualifier is specified, SHOW LAN displays all information found in the LAN, LSB, and UCB data structures.

### Examples

#1

    SDA>  SHOW LAN/FULL
    LAN Data Structures
    -------------------
                   -- LAN Information Summary 23-MAY-1996 13:07:52 --
    LAN flags:  00000004 LAN_INIT
    LAN block address           80DB7140    Timer DELTA time            10000000
    Number of stations                 2    DAT sequence number                1
    LAN module version                 1    First SVAPTE                FFDF60F0
    LANIDEF version                   51    Number of PTEs                     3
    LANUDEF version                   26    SVA of first page           8183C000
    First LSB address           80DCA980

                -- LAN CSMACD Network Management 23-MAY-1996 13:07:52 --
    Creation time                   None    Times created                      0
    Deletion time                   None    Times deleted                      0
    Module EAB                  00000000    Latest EIB                  00000000
    Port EAB                    00000000
    Station EAB                 00000000
    NM flags:   00000000
                 -- LAN FDDI Network Management 23-MAY-1996 13:07:52 --
    Creation time                   None    Times created                      0
    Deletion time                   None    Times deleted                      0
    Module EAB                  00000000    Link EAB                    00000000
    Port EAB                    00000000    PHY port EAB                00000000
    Station EAB                 00000000    Module EIB                  00000000
    NM flags:   00000000
    LAN Data Structures
    -------------------
                   -- ESA Device Information 23-MAY-1996 13:07:52 --
    LSB address                 80DCA980    Driver code address         80CAE838
    Driver version     00000001.07010037    Device1 code address        00000000
    Device1 version    00000000.00000000    Device2 code address        00000000
    Device2 version    00000000.00000000    LAN code address            80CAFA00
    LAN version        00000001.07010112    DLL type                      CSMACD
    Device name                 EY_NITC2    MOP name                         MXE
    MOP ID                            94    HW serial               Not supplied
    HW version                  00000000    Promiscuous mode                 OFF
    Controller mode               NORMAL    Promiscuous UCB             00000000
    Internal loopback                OFF    All multicast state              OFF
    Hardware address   08-00-03-DE-00-12    CRC generation mode               ON
    Physical address   AA-00-04-00-88-FE    Full Duplex Enable               OFF
    Active unit count                  1    Full Duplex State                OFF
    Line speed                        10
    Flags:  00000000
    Char:   00000000
    Status: 00000003 RUN,INITED

    LAN Data Structures
    -------------------
                -- ESA Device Information (cont) 23-MAY-1996 13:07:52 --
    Put rcv ptr/index           00000000    Get rcv ptr/index           00000015
    Put xmt ptr/index           80DCB620    Get xmt ptr/index           80DCB620
    Put cmd ptr/index           00000000    Get cmd ptr/index           00000000
    Put uns ptr/index           00000000    Get uns ptr/index           00000000
    Put smt ptr/index           00000000    Get smt ptr/index           00000000
    RBufs owned by dev                 0    Rcv packet limit                  32
    XEnts owned by dev                 0    XEnts owned by host                4
    CEnts owned by dev                 0    Transmit timer                     0
    UEnts owned by dev                 0    Control timer                      0
    SEnts owned by dev                 0    Periodic SYSID timer             599
    Current rcv buffers               17    Ring unavail timer                 0
    Rqst MAX rcv buffers              32    USB timer                         26
    Rqst MIN rcv buffers              16    Receive alignment                  0
    Curr MAX rcv buffers              32    Receive buffer size             1518
    Curr MIN rcv buffers              16    Min 1st chain segment              0
    FILL rcv buffers                  16    Min transmit length                0
    ADD  rcv buffers                  32    Dev xmt header size                0
    LAN Data Structures
    -------------------
                -- ESA Device Information (cont) 23-MAY-1996 13:07:52 --
    Last receive         23-MAY 13:07:51    Last transmit        23-MAY 13:07:50
    ADP address                 80D4B280    IDB address                 80DCA880
    DAT stage                   00000000    DAT xmt status     0000003C.003C0001
    DAT number started                 1    DAT xmt complete     23-MAY 13:07:19
    DAT number failed                  0    DAT rcv found                   None
    DAT VCRP                    80DCBB80    DAT UCB                     00000000
    Mailbox enable flag                0    CRAM read comman            00000000
    CSR base phys addr 00000000.00000000    CRAM write comma            00000000
    Mailboxes in use                   0    Media                           UNDF
    2nd LW status flags         00000000
    LAN Data Structures
    -------------------
             -- ESA Network Management Information 23-MAY-1996 13:07:52 --
    Creation time                   None    Create count                       0
    Deletion time                   None    Enable count                       0
    Enabled time                    None    Number of ports                    0
    Disabled time                   None    Events logged                      0
    EIB address                 00000000    NMgmt assigned addr             None
    LLB address                 00000000    Station name itmlst         00000000
    LHB address                 00000000    Station itmlst len                 0
    First LPB address           00000000
    LAN Data Structures
    -------------------
                    -- ESA Fork Information 23-MAY-1996 13:07:52 --
    ISR   FKB sched      23-MAY 13:07:51    ISR   FKB in use flag           FREE
    ISR   FKB time       23-MAY 13:07:51    ISR   FKB count                  200
    IPL8  FKB sched      23-MAY 13:07:20    IPL8  FKB in use flag           FREE
    IPL8  FKB time       23-MAY 13:07:20    IPL8  FKB count                    1
    RESET FKB sched                 None    RESET FKB in use flag           FREE
    RESET FKB time                  None    RESET FKB count                    0
    NM    FKB sched                 None    NM    FKB in use flag           FREE
    NM    FKB time                  None    NM    FKB count                    0
    Fork status code                   0

    LAN Data Structures
    -------------------
                    -- ESA Queue Information 23-MAY-1996 13:07:52 --
    Control hold queue      80DCACF0  Status:  Valid, empty
    Control request queue   80DCACF8  Status:  Valid, empty
    Control pending queue   80DCAD00  Status:  Valid, empty
    Transmit request queue  80DCACE8  Status:  Valid, empty
    Transmit pending queue  80DCAD18  Status:  Valid, empty
    Receive buffer list     80DCAD38  Status:  Valid, 17 elements
    Receive pending queue   80DCAD20  Status:  Valid, empty
    Post process queue      80DCAD08  Status:  Valid, empty
    Delay queue             80DCAD10  Status:  Valid, empty
    Auto restart queue      80DCAD28  Status:  Valid, empty
    Netwrk mgmt hold queue  80DCAD30  Status:  Valid, empty
              -- ESA Multicast Address Information 23-MAY-1996 13:07:52 --
    AB-00-00-04-00-00
                      -- ESA Unit Summary 23-MAY-1996 13:07:52 --
    UCB      UCB Addr  Fmt   Value           Client     State
    ---      --------  ---   -----           ------  -----------
    ESA0     80D4F6C0
    ESA1     80E35400  Eth   60-03           DECNET  0017 STRTN,LEN,UNIQ,STRTD
    LAN Data Structures
    -------------------
                  -- ESA Counters Information 23-MAY-1996 13:07:52 --
    Octets received                  596    Octets sent                      230
    PDUs received                      8    PDUs sent                          5
    Mcast octets received            596    Mcast octets sent                138
    Mcast PDUs received                8    Mcast PDUs sent                    3
    Unrec indiv dest PDUs              0    PDUs sent, deferred                0
    Unrec mcast dest PDUs              1    PDUs sent, one coll                0
    Data overruns                      0    PDUs sent, mul coll                0
    Unavail station buffs              0    Excessive collisions               0
    Unavail user buffers               0    Late collisions                    0
    CRC errors                         0    Carrier check failure              0
    Alignment errors                   0    Last carrier failure            None
    Rcv data length err                0    Coll detect chk fail               5
    Frame size errors                  0    Short circuit failure              0
    Frames too long                    0    Open circuit failure               0
    Seconds since zeroed              34    Transmits too long                 0
    Station failures                   0    Send data length err               0

    LAN Data Structures
    -------------------
               -- ESA Counters Information (cont) 23-MAY-1996 13:07:52 --
    No work transmits                  0    Ring avail transitions             0
    Buffer_Addr transmits              0    Ring unavail transitions           0
    SVAPTE/BOFF transmits              0    Loopback sent                      0
    Global page transmits              0    System ID sent                     0
    Bad PTE transmits                  0    ReqCounters sent                   0
    Restart pending counter            0    Internal counters size            40
    +00 MCA not enabled              187    +2C Generic (or unused)     00000000
    +04 Xmt underflows                 0    +30 Generic (or unused)     00000000
    +08 Rcv overflows                  0    +34 Generic (or unused)     00000000
    +0C Memory errors                  0    +38 Generic (or unused)     80DCAD18
    +10 Babbling errors                0    +3C Generic (or unused)     80DCAD18
    +14 Local buffer errors            0    +40 Generic (or unused)     004E0840
    +18 LANCE interrupts             202    +44 Generic (or unused)     61616161
    +1C Xmt ring <31:0>         00000000    +48 Generic (or unused)     61616161
    +20 Xmt ring <63:32>        00000000    +4C Generic (or unused)     61616161
    +24 Soft errors handled            0    +50 Generic (or unused)     61616161
    +28 Generic (or unused)     00000000    +54 Generic (or unused)     61616161
    LAN Data Structures
    -------------------
                    -- ESA Error Information 23-MAY-1996 13:07:52 --
    Fatal error count                  0    Last error CSR              00000000
    Fatal error code                None    Last fatal error                None
    Prev  error code                None    Prev fatal error                None
    Transmit timeouts                  0    Last USB time                   None
    Control timeouts                   0    Last UUB time                   None
    Restart failures                   0    Last CRC time                   None
    Power failures                     0    Last CRC srcadr                 None
    Bad PTE transmits                  0    Last length erro                None
    Loopback failures                  0    Last exc collisi                None
    System ID failures                 0    Last carrier fai                None
    ReqCounters failures               0    Last late collis                None
    LAN Data Structures
    -------------------
                 -- ESA0 Template Unit Information 23-MAY-1996 13:07:52 --
    LSB address                 80DCA980    Error count                        0
    VCIB address                00000000    Parameter mask              00000000
    Stop IRP address            00000000    Promiscuous mode                 OFF
    Restart IRP address         00000000    All multicast mode               OFF
    LAN medium                    CSMACD    Source Routing mode      TRANSPARENT
    Packet format               Ethernet    Access mode                EXCLUSIVE
    Eth protocol type              00-00    Shared user DES                 None
    802E protocol ID      00-00-00-00-00    Padding mode                      ON
    802.2 SAP                         00    Automatic restart           DISABLED
    802.2 Group SAPs         00,00,00,00    Allow prom client                 ON
    Controller mode               NORMAL    Can change address               OFF
    Internal loopback                OFF    802.2 service                   User
    CRC generation mode               ON    Rcv buffers to save                1
    Functional Addr mod               ON    Minimum rcv buffers                4
    Hardware address   08-00-03-DE-00-12    User transmit FC/AC               ON
    Physical address   FF-FF-FF-FF-FF-FF    User receive FC/AC               OFF

    LAN Data Structures
    -------------------
              -- ESA1 60-03 (DECNET) Unit Information 23-MAY-1996 13:07:52 --
    LSB address                 80DCA980    Error count                        0
    VCIB address                00000000    Parameter mask              00DA8695
    Stop IRP address            80E047C0    Promiscuous mode                 OFF
    Restart IRP address         00000000    All multicast mode               OFF
    LAN medium                    CSMACD    Source Routing mode      TRANSPARENT
    Packet format               Ethernet    Access mode                EXCLUSIVE
    Eth protocol type              60-03    Shared user DES                 None
    802E protocol ID      00-00-00-00-00    Padding mode                      ON
    802.2 SAP                         00    Automatic restart           DISABLED
    802.2 Group SAPs         00,00,00,00    Allow prom client                 ON
    Controller mode               NORMAL    Can change address               OFF
    Internal loopback                OFF    802.2 service                   User
    CRC generation mode               ON    Rcv buffers to save               10
    Functional Addr mod               ON    Minimum rcv buffers                4
    Hardware address   08-00-03-DE-00-12    User transmit FC/AC               ON
    Physical address   AA-00-04-00-88-FE    User receive FC/AC               OFF
    LAN Data Structures
    -------------------
          -- ESA1 60-03 (DECNET) Unit Information (cont) 23-MAY-1996 13:07:52 --
    Last receive         23-MAY 13:07:47    Starter's PID               0001000F
    Last transmit        23-MAY 13:07:50    Maximum header size               16
    Last start attempt   23-MAY 13:07:20    Maximum buffer size             1498
    Last start done      23-MAY 13:07:20    Rcv quota charged              15040
    Last start failed               None    Default FC value                  00
    MCA match enabled                 01    Default AC value                  00
    Last MCA filtered  AB-00-00-04-00-00    Maintenance state                 ON
    UCB status:  00000017 STRTN,LEN,UNIQ,STRTD
    Receive IRP queue       80E356E8  Status:  Valid, 1 element
    Receive pending queue   80E356E0  Status:  Valid, empty
    Multicast address table, embedded:
      AB-00-00-04-00-00
    LAN Data Structures
    -------------------
            -- ESA1 60-03 (DECNET) Counters Information 23-MAY-1996 13:07:52 --
    Octets received                  483    Octets sent                      180
    PDUs received                      7    PDUs sent                          3
    Mcast octets received            483    Mcast octets sent                180
    Mcast PDUs received                7    Mcast PDUs sent                    3
    Unavail user buffer                0    Multicast not enabled              0
    Last UUB time                   None    User buffer too small              0

> The SHOW LAN/FULL command displays information for all LAN, LSB, and UCB data structures.

#2
    SDA>  SHOW LAN/TIME
                   -- LAN History Information 12-FEB-1995 11:08:48 --
    12-FEB 11:08:47.92  ESA               Last receive
    12-FEB 11:08:47.92  ESA               Last fork scheduled
    12-FEB 11:08:47.92  ESA               Last fork time
    12-FEB 11:08:47.77  ESA5     LAST     Last receive
    12-FEB 11:08:47.72  ESA3     LAT      Last receive
    12-FEB 11:08:41.25  ESA               Last transmit
    12-FEB 11:08:41.25  ESA5     LAST     Last transmit
    12-FEB 11:08:40.02  ESA2     DECnet   Last receive
    12-FEB 11:08:39.14  ESA2     DECnet   Last transmit
    12-FEB 11:08:37.39  ESA3     LAT      Last transmit
    12-FEB 10:19:25.31  ESA               Last unavail user buffer
    12-FEB 10:19:25.31  ESA2     DECnet   Last unavail user buffer
    11-FEB 14:10:20.09  ESA5     LAST     Last start completed
    11-FEB 14:10:02.16  ESA3     LAT      Last start completed
    11-FEB 14:09:58.44  ESA2     DECnet   Last start completed
    11-FEB 14:09:57.44  ESA               Last DAT transmit

> The SHOW LAN/TIME command displays print time information from device and unit data structures.

#3
    SDA> SHOW LAN/VCI/DEVICE=ICB
                   -- ICB VCI Information 17-APR-1996 14:22:07 --
    LSB address  = 80A1D580
    Device state = 00000003 RUN,INITED
             -- ICB2 80-41 (LAST) VCI Information 17-APR-1996 14:22:07 --
    VCIB address =    8096F238
    CLIENT flags:     00000001 RCV_DCB
    LAN flags:        00000004 LAN_INIT
    DLL flags:        00000005 XMT_CHAIN,PORT_STATUS
    UCB status:       00000015 STRTN,UNIQ,STRTD
    VCI ID                         LAST    VCI version               00010001
    UCB address                80A4C5C0    DP VCRP address           00000000
    Hardware address  00-00-93-08-52-CF    LDC address               80A1D720
    Physical address  00-00-93-08-52-CF    LAN medium                      TR
    Transmit available         80A1D670    Outstanding operations           0
    Maximum receives                  0    Outstanding receives             0
    Max xmt size                   4444    Header size                     52
    Build header rtn           808BF230    Report event rtn          86327130
    XMT initiate rtn           808BF200    Transmit complete rtn     86326D80
    XMT frame rtn              808BF210    Receive complete rtn      86326A80
          -- ICB2 80-41 (LAST) VCI Information (cont) 17-APR-1996 14:22:07 --
    Portmgmt initiate rtn      808BF0C0    Portmgmt complete rtn     86327100
    Monitor request rtn        00000000    Monitor transmit rtn      00000000
    Monitor flags              00000000    Monitor receive rtn       00000000
    Port usable                00000000    Port unusable             00000000

> The SHOW LAN/VCI/DEVICE=ICB command displays the VCIB for a Token Ring device (ICB) which has an active VCI user (LAST).

#4
    SDA> SHOW LAN/ELAN
            -- HCA Emulated LAN LSB Information 17-APR-1996 14:08:02 --
    LSB address = 8098D200
    Device state = 00000101 RUN,RING_AVAIL
    Driver CM VC setup adr   808986A0    Driver CM VC teardown adr    80898668
    NIPG CM handle adr       8096C30C    NIPG CM SVC handle           00000000
    NIPG CM agent handle adr 809B364C    NIPG CM mgr lineup handle    809B394C
    NIPG CM ILMI IO handle   809B378C    MIB II handle adr            809B94CC
    MIB handle adr           809B3ACC    Queue header for EL LSBs     00000000
    DEC MIB handle adr       809BBD8C    NIPG current TQEs used       00000000
    Count of allocated TQEs  0000000D    NIPG current pool used       0000D2C0
    NIPG pool allocations    00075730
            -- ELA Emulated LAN LSB Information 17-APR-1996 14:08:02 --
    LSB address = 80AB08C0
    Device state = 00000001 RUN
    ELAN name = ELAN 1
    ELAN description = ATM ELAN
    ELAN parent = HCA0
    ELAN state = 00000001 ACTIVE
    MAX transmit size     MTU_1516          ELAN media type      LAN_802_3
    LEC attr buff adr     80AB1FC0          LEC attr buff size    00000328
    Event mask            00000000          PVC identifer         00000000
    Extended sense        00000000
             -- ELA Emulated LAN LEC Attributes 17-APR-1996 14:08:02 --
    LAN type          00000000          LAN MTU              00000001
    Proxy flag        00000000          Control timeout      0000000A
    Max UF count      00000001          Max UF time          00000001
    VCC timeout       000004B0          Max retry count      00000002
    LEC id            00000002          Forw delay time      0000000F
    Flush timeout     00000004          Path switch delay    00000006
    SM state          00000070          Illegal CTRL frames  00000000
    CTRL xmt failures 00000000          CTRL frames sent     0000000C
    CTRL frames_rcvd  00000012          LEARPs sent          00000000
    LEARPS rcvd       00000000          UCASTs sent direct   00000000
    UCASTs flooded    00000006          UCASTs discarded     00000001
    NUCASTs sent      00000000
    Local ESI         00000000.00000000
    BUS ATM addr      3999990000000008002BA57E80.AA000302FF12.00
    LES ATM addr      3999990000000008002BA57E80.AA000302FF14.00
    My ATM addr       3999990000000008002BA57E80.08002B2240A0.00

> The SHOW LAN/ELAN command displays information for the parent ATM device (HCA) driver and the ELAN pseudo-device (ELA) driver.

#5
    SDA> SHOW LAN/ELAN/DEV=ELA
            -- ELA Emulated LAN LSB Information 17-APR-1996 14:08:22 --
    LSB address = 80AB08C0
    Device state = 00000001 RUN
    ELAN name = ELAN 1
    ELAN description = ATM ELAN
    ELAN parent = HCA0
    ELAN state = 00000001 ACTIVE
    MAX transmit size     MTU_1516          ELAN media type      LAN_802_3
    LEC attr buff adr     80AB1FC0          LEC attr buff size    00000328
    Event mask            00000000          PVC identifer         00000000
    Extended sense        00000000
             -- ELA Emulated LAN LEC Attributes 17-APR-1996 14:08:22 --
    LAN type             00000000          LAN MTU              00000001
    Proxy flag           00000000          Control timeout      0000000A
    Max UF count         00000001          Max UF time          00000001
    VCC timeout          000004B0          Max retry count      00000002
    LEC id               00000002          Forw delay time      0000000F
    Flush timeout        00000004          Path switch delay    00000006
    SM state             00000070          Illegal CTRL frames  00000000
    CTRL xmt failures    00000000          CTRL frames sent     0000000C
    CTRL frames_rcvd     00000012          LEARPs sent          00000000
    LEARPS rcvd          00000000          UCASTs sent direct   00000000
    UCASTs flooded       00000006          UCASTs discarded     00000001
    NUCASTs sent         00000000
    Local ESI            00000000.00000000
    BUS ATM addr         3999990000000008002BA57E80.AA000302FF12.00
    LES ATM addr         3999990000000008002BA57E80.AA000302FF14.00
    My ATM addr          3999990000000008002BA57E80.08002B2240A0.00

> The SHOW LAN/ELAN/DEVICE=ELA command displays information for the ELAN pseudo-device (ELA) driver only.

#6
    SDA>  SHOW LAN/ELAN/DEVICE=HCA
           -- HCA Emulated LAN LSB Information 17-APR-1996 14:08:25 --
    LSB address = 8098D200
    Device state = 00000101 RUN,RING_AVAIL
    Driver CM VC setup adr   808986A0    Driver CM VC teardown adr    80898668
    NIPG CM handle adr       8096C30C    NIPG CM SVC handle           00000000
    NIPG CM agent handle adr 809B364C    NIPG CM mgr lineup handle    809B394C
    NIPG CM ILMI IO handle   809B378C    MIB II handle adr            809B94CC
    MIB handle adr           809B3ACC    Queue header for EL LSBs     00000000
    DEC MIB handle adr       809BBD8C    NIPG current TQEs used       00000000
    Count of allocated TQEs  0000000D    NIPG current pool used       0000D2C0
    NIPG pool allocations    000757B2

> The SHOW LAN/ELAN/DEVICE=HCA command displays information for the ATM device (HCA) driver only.

Previous | Next | Contents | Index

| privacy and legal statement |
6549PRO_013.HTML