| ## dce_server_inq_attr(3dce) Obtains from dced the value of an attribute known to the server Synopsis #include <dce/dced.h> void dce_server_inq_attr( uuid_t *attribute_uuid, sec_attr_t *value, error_status_t *status); Parameters Input attribute_uuid The UUID dced uses to identify an attribute. Output value Returns the attribute. status Returns the status code from this routine. This status code indicates whether the routine completed successfully or, if not, why not. Description The dce_server_inq_attr( ) routine obtains an attribute from the environment created by dced when it started the server. Each server maintains among other things, a list of attributes that are used to describe application-specific behavior. Errors The following describes a partial list of errors that might be returned. Refer to the OSF DCE Problem Determination Guide for complete descriptions of all error messages. error_status_ok dced_s_server_attr_not_found dced_s_not_started_by_dced Related Information Routines: sec_intro(3sec) dced_intro(3dce) dce_server_inq_uuids(3dce) dce_server_inq_server(3dce) Book: OSF DCE Application Development Guide - Core Components ##