| ### Matching Server Epochs At startup, a server's epoch number must match those of the other servers with which it synchronizes. When synchronizing, a server disregards clock values that are from servers whose epoch numbers do not match its own. When DTS servers are initially enabled, the epoch number for each server is 0, so you need not change the epoch numbers at initial installation. Later, if you add a server to an existing network, or change a clerk to a server, ensure that the new server and the preexisting servers have matching epoch numbers. Enter the DCE control program's dts show command to find out the epoch number of the server. For example: dcecp> dts show /.:/hosts/orion/dts-server Examine the attributes list that the command returns for the server's epoch attribute value. If the epoch of the server that you just created matches those of the other servers, the new server can synchronize immediately. If the epochs do not match, however, and you do not change the epoch of the new server, the new server ignores the preexisting servers. The following example shows how to change a server's epoch number after you enable the server: dcecp> clock set -abruptly -epoch 0 dcecp> Once you know that a server is starting up with the proper epoch number, do not change the epoch unless serious system or network problems corrupt all of the server clock values. In the unlikely event that the majority of the server clocks become faulty, use the dts show and clock set command to isolate problem servers so that you can perform troubleshooting and maintenance without affecting the rest of the DTS application. ###