| ## dce_aud_free_ev_info(3sec) Frees the memory allocated for an event information structure returned from calling dce_aud_get_ev_info( ). Used by the audit trail analysis and examination tools. Synopsis #include <dce/audit.h> void dce_aud_free_ev_info( dce_aud_ev_info_t *event_info, unsigned32 *status); Parameters Input event_info Designates an event-specific information item returned from a previous successful call to the dce_aud_get_ev_info( ) function. Output status The status code returned by this routine. Description The dce_aud_free_ev_info( ) function frees the memory allocated for an event information structure returned by a previous successful call to the dce_aud_get_ev_info( ) function. Return Values No value is returned. Errors The following describes a partial list of errors that might be returned. Refer to the OSF DCE Problem Determination Guide for complete descriptions of all error messages. aud_s_ok The call was successful. Related Information Functions: dce_aud_next(3sec) dce_aud_get_ev_info(3sec) ##