# Compaq DECwindows Motif
for OpenVMS
Installation Guide

Previous | Contents | Index

# Appendix B
VMSINSTAL Sample Installation

This appendix contains a sample VMSINSTAL product installation.

# B.1 Sample Installation Using VMSINSTAL on a VMS Version 5.5--2 System

Example B-1 contains a sample installation of the Compaq DECwindows Motif for OpenVMS software on a VMS Version 5.5-2 operating system using the VMSINSTAL procedure. The sample installation assumes that no users are logged in to the system and that you specified OPTIONS N to display the release notes.

Example B-1 Sample Installation Using VMSINSTAL

    $ @SYS$UPDATE:VMSINSTAL DWMOTIFVAXU6012

            VAX/VMS Software Product Installation Procedure V5.5-2

    It is 26-MAR-2000 at 10:36.

    Enter a question mark (?) at any time for help.

    * Are you satisfied with the backup of your system disk [YES]? [Return]
    * Where will the distribution volumes be mounted: DAD2:[000000][Return]
    Enter the products to be processed from the first distribution volume set.
    * Products: dwmotifvaxu6012 [Return]
    * Enter installation options you wish to use (none): [Return]
    The following products will be processed:

      DWMOTIFVAXU6 V1.2

            Beginning installation of DWMOTIFVAXU6 V1.2 at 10:36

    %VMSINSTAL-I-RESTORE, Restoring product save set A ...
    %VMSINSTAL-I-RELMOVED, Product's release notes have been moved to SYS$HELP.

            *** Installing DECwindows Motif for OpenVMS VAX software ***

      Copyright 2000 Compaq Computer Corporation

      COMPAQ Registered in U.S. Patent and Trademark Office.

      Confidential computer software. Valid license from Compaq or authorized
      sublicensor required for possession, use , or copying. Consistent with
      FAR 12.211 and 12.212, Commercial Computer Software, Computer Software
      Documentation, and Technical Data for Commercial Items are licensed
      to the U.S. Government under vendor's standard commercial license.

      You can install the DECwindows Motif kit completely or in selected
      portions.  A complete installation requires as many as 68,400 blocks.
      If you choose to perform a partial installation, you can select
      (tailor) the programming support files that support your DECwindows
      Motif application development.  Whether you perform a complete or partial
      installation, this kit provides support for running DECwindows Motif
      applications on OpenVMS compute servers.

    * Do you want to install the entire kit [Y]? No [Return]
      This installation procedure provides support files for developing
      DECwindows Motif applications in several programming languages.  These
      files are needed only to develop applications and are not required to run
      DECwindows Motif applications.  The free disk space requirement for each
      programming support file ranges from 3000 to 8000 blocks.

    * Do you want to install DECwindows Motif programming support [Y]? [Return]
      Support files are supplied for the following OpenVMS programming languages:

      FORTRAN, Pascal

      In addition, support files are supplied for programming in the C language
      using conventions and standards developed at the Massachusetts Institute
      of Technology.

    * Do you want to install all programming language support files [Y]? [Return]
    * Do you want to install DECwindows Motif programming examples [Y]? [Return]
      You have selected the following portions of the kit:

            o  DECwindows Motif Applications and Run-time Libraries

            o  DECwindows Motif programming examples

            o  DECwindows Motif programming support
                    FORTRAN, Pascal
                    MIT C language programming conventions

    * Are these selections correct [Y]? [Return]
      A registered and loaded product authorization key for DW-MOTIF is
      required to run any DECwindows Motif for OpenVMS application. If you
      answer NO to the next question, the installation of DECwindows Motif for
      OpenVMS will be terminated.

            Product:      DW-MOTIF
            Producer:     DEC
            Version:
            Release Date:

    * Does this product have an authorization key registered and loaded? Yes [Return]
      DECwindows Motif will not start if your system parameters are not
      correct.

      o If you allow a system shutdown, the installation procedure will
        reboot the system at the end of the installation.  If your system
        parameters are incorrect, the installation will run AUTOGEN prior
        to the system reboot.

      o If you do not allow a system shutdown, the installation procedure
        will continue, and you will be informed at the end of the
        installation whether you need to modify your system parameters in
        order to start DECwindows Motif.

        To complete the installation of this product, you should reboot
        the system.  If it is not convenient to reboot at this time, then
        enter NO to the following question.

        If you enter NO, the installation procedure will continue.

    * Will you allow a system shutdown after this product is installed [YES]? No [Return]
      No further questions will be asked.

    %VMSINSTAL-I-RESTORE, Restoring product save set B ...
    %VMSINSTAL-I-RESTORE, Restoring product save set C ...
    %VMSINSTAL-I-RESTORE, Restoring product save set D ...
    %VMSINSTAL-I-RESTORE, Restoring product save set E ...
    %VMSINSTAL-I-RESTORE, Restoring product save set F ...
    %VMSINSTAL-I-RESTORE, Restoring product save set G ...
    %VMSINSTAL-I-RESTORE, Restoring product save set H ...
    %VMSINSTAL-I-RESTORE, Restoring product save set I ...
    %VMSINSTAL-I-RESTORE, Restoring product save set J ...
    %VMSINSTAL-I-RESTORE, Restoring product save set L ...
    %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

      You may safely ignore the following NCP error message(s):

    %NCP-I-SUCCESS,  Success
    Object = X$X0
    %NML-I-RECDELET, Database entry deleted

      The Installation Verification Procedure (IVP) should be run after the
      installation has been completed and DECwindows Motif has been restarted.
      The IVP can be found in SYS$TEST:DECW$IVP.COM.

      The installation procedure has determined that your system parameters are
      set correctly and that it will not be necessary to run AUTOGEN or reboot
      the system.

      If your system is already running DECwindows Motif, restart DECwindows
      Motif with the following DCL command:

           $ @SYS$MANAGER:DECW$STARTUP RESTART

      If your system is NOT already running DECwindows Motif, start DECwindows
      Motif with the following DCL command:

           $ @SYS$MANAGER:DECW$STARTUP

                                * * * N O T E * * *

      If you are installing DECwindows Motif from your workstation console, log
      off after you enter the command to start DECwindows Motif.

      The installation procedure has determined that your system parameter values
      are acceptable.  A reboot of the system is not required.

            Installation of DWMOTIFVAXU6 V1.2 completed at 10:57

    Enter the products to be processed from the next distribution volume set.
    * Products: [Return]
        VMSINSTAL procedure done at 12:45

# Appendix C
Software Components

If you installed Compaq DECwindows Motif for OpenVMS using the POLYCENTER Software Installation utility, you can obtain a list of all installed files and the directories and subdirectories into which the files were installed.

To obtain this list, enter the following POLYCENTER Software Installation utility command:

    $ PRODUCT SHOW OBJECT/product=dwmotif

Following is a sample output from this command.

    OBJECT                                   OBJECT TYPE
    ------                                   -----------
    [000000]                                 directory
    [000000]DEC-AXPVMS-DWMOTIF-V0102-6-1.PCSI$DESCRIPTION file
    [000000]DEC-AXPVMS-DWMOTIF-V0102-6-1.PCSI$TLB file
    [CDA$LIBRARY]                            directory
    [CDA$LIBRARY]CL_DAY.DOC_STYLE            file
    [CDA$LIBRARY]DEFSTYLE.DDIF               file
    [CDE$DEFAULTS]                           directory
    [CDE$DEFAULTS]                           directory
    [CDE$DEFAULTS.SYSTEM]                    directory
    [CDE$DEFAULTS.SYSTEM]                    directory
    [CDE$DEFAULTS.SYSTEM.APP-DEFAULTS]       directory
    [CDE$DEFAULTS.SYSTEM.APP-DEFAULTS.C]     directory
    [CDE$DEFAULTS.SYSTEM.APP-DEFAULTS.C]DT.DAT file
    [CDE$DEFAULTS.SYSTEM.APP-DEFAULTS.C]DTCALC.DAT file
    [CDE$DEFAULTS.SYSTEM.APP-DEFAULTS.C]DTCREATE.DAT file
    [CDE$DEFAULTS.SYSTEM.APP-DEFAULTS.C]DTFILE.DAT file
    [CDE$DEFAULTS.SYSTEM.APP-DEFAULTS.C]DTHELLO.DAT file
    .
    .
    .

Index | Contents