| ### dcecp Operations for DTS The following table summarizes the operations performed by dcecp commands on DTS objects. dcecp Operations for DTS
Operations | Description
activate | Changes the state of the clerk or server process from inactive to active and causes the object to synchronize its time.
catalog | Returns a list of DTS servers in the specified cell.
compare | Compares the time reported by the local clerk with that of a specified server.
configure | Configures a server as a global or local server.
deactivate | Changes the state of a clerk or server process from active to inactive and causes the object to stop synchronizing its time.
help | Displays a list of operations that can be performed on the clerk, server, or clock, or a verbose description of the specified object.
modify | Modifies the attribute information for a clerk or server.
operations | Displays a short list of the operations that can be performed on the clerk, server, or clock.
set | Sets the clock gradually or immediately to the time specified by the argument (in DTS-style timestamp format).
show | For a clerk or server, displays information about attributes or counters. For a clock, displays the clock's time in the DTS-style timestamp format.
stop | Stops the clerk or server process.
synchronize | Tells the dtsd to gradually or immediately synchronize (the -abruptly option) with the DTS servers.
###